## Reconyx Tags

The following tags are extracted from the maker notes of Reconyx Hyperfire cameras such as the HC500, HC600 and PC900.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MakerNoteVersion | N |
> 1 | FirmwareVersion | N |
> 4 | FirmwareDate | int16u[2] |
> 6 | TriggerMode | string[2] | 'C' = CodeLoc Not Entered 'E' = External Sensor 'M' = Motion Detection 'T' = Time Lapse
> 7 | Sequence | int16u[2] |
> 9 | EventNumber | int16u[2] |
> 11 | DateTimeOriginal | int16u[6] |

> 18

> MoonPhase

> int16u

> 0 = New 1 = New Crescent 2 = First Quarter 3 = Waxing Gibbous |  | 4 = Full 5 = Waning Gibbous 6 = Last Quarter 7 = Old Crescent |

> 19 | AmbientTemperatureFahrenheit | int16s |
> 20 | AmbientTemperature | int16s |
> 21 | SerialNumber | undef[30] |
> 36 | Contrast | int16u |
> 37 | Brightness | int16u |
> 38 | Sharpness | int16u |
> 39 | Saturation | int16u |
> 40 | InfraredIlluminator | int16u | 0 = Off 1 = On
> 41 | MotionSensitivity | int16u |
> 42 | BatteryVoltage | int16u |
> 43 | UserLabel | string[22] |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Oct 21, 2011

<-- ExifTool Tag Names