## Olympus Tags

Tags 0x0000 through 0x0103 are used by some older Olympus cameras, and are the same as Konica/Minolta tags. These tags are also used for some models from other brands such as Acer, BenQ, Epson, Hitachi, HP, Maginon, Minolta, Pentax, Ricoh, Samsung, Sanyo, SeaLife, Sony, Supra and Vivitar.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | MakerNoteVersion | undef |
> 0x0001 | MinoltaCameraSettingsOld | - | --> Minolta CameraSettings Tags
> 0x0003 | MinoltaCameraSettings | - | --> Minolta CameraSettings Tags
> 0x0040 | CompressedImageSize | int32u |
> 0x0081 | PreviewImageData | N |
> 0x0088 | PreviewImageStart | N |
> 0x0089 | PreviewImageLength | N |
> 0x0100 | ThumbnailImage | undef |
> 0x0104 | BodyFirmwareVersion | string |
> 0x0200 | SpecialMode | int32u[3]~ | (3 numbers: 1. Shooting mode: 0=Normal, 2=Fast, 3=Panorama; 2. Sequence Number; 3. Panorama Direction: 1=Left-Right, 2=Right-Left, 3=Bottom-Top, 4=Top-Bottom)
> 0x0201 | Quality | int16u~ | (Quality values are decoded based on the CameraType tag. All types represent SQ, HQ and SHQ as sequential integers, but in general SX-type cameras start with a value of 0 for SQ while others start with 1)
> 0x0202 | Macro | int16u | 0 = Off 1 = On 2 = Super Macro
> 0x0203 | BWMode | int16u | 0 = Off 1 = On
> 0x0204 | DigitalZoom | rational64u |
> 0x0205 | FocalPlaneDiagonal | rational64u |
> 0x0206 | LensDistortionParams | int16s[6] |
> 0x0207 | CameraType | string | --> Olympus CameraType Values
> 0x0208 | TextInfo | - | --> Olympus TextInfo Tags
> 0x0209 | CameraID | string |
> 0x020b | EpsonImageWidth | int16u |
> 0x020c | EpsonImageHeight | int16u |
> 0x020d | EpsonSoftware | string |
> 0x0280 | PreviewImage | int8u | (found in ERF and JPG images from some Epson models)
> 0x0300 | PreCaptureFrames | int16u |
> 0x0301 | WhiteBoard | int16u |
> 0x0302 | OneTouchWB | int16u | 0 = Off 1 = On 2 = On (Preset)
> 0x0303 | WhiteBalanceBracket | int16u |
> 0x0304 | WhiteBalanceBias | int16u |

> 0x0403

> SceneMode

> int16u

> 0 = Normal
> 1 = Standard
> 2 = Auto
> 3 = Intelligent Auto
> 4 = Portrait
> 5 = Landscape+Portrait
> 6 = Landscape
> 7 = Night Scene
> 8 = Night+Portrait
> 9 = Sport
> 10 = Self Portrait
> 11 = Indoor
> 12 = Beach & Snow
> 13 = Beach
> 14 = Snow
> 15 = Self Portrait+Self Timer
> 16 = Sunset
> 17 = Cuisine
> 18 = Documents
> 19 = Candle

> 20 = Fireworks
> 21 = Available Light
> 22 = Vivid
> 23 = Underwater Wide1
> 24 = Underwater Macro
> 25 = Museum
> 26 = Behind Glass
> 27 = Auction
> 28 = Shoot & Select1
> 29 = Shoot & Select2
> 30 = Underwater Wide2
> 31 = Digital Image Stabilization
> 32 = Face Portrait
> 33 = Pet
> 34 = Smile Shot
> 35 = Quick Shutter
> 43 = Hand-held Starlight
> 100 = Panorama
> 101 = Magic Filter
> 103 = HDR

> 0x0404 | SerialNumber | string |
> 0x0405 | Firmware | string |
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x0f00 | DataDump | N |
> 0x0f01 | DataDump2 | N |
> 0x0f04 | ZoomedPreviewStart | int32u* |
> 0x0f05 | ZoomedPreviewLength | int32u* |
> 0x0f06 | ZoomedPreviewSize | int16u[2] |
> 0x1000 | ShutterSpeedValue | rational64s |
> 0x1001 | ISOValue | rational64s |
> 0x1002 | ApertureValue | rational64s |
> 0x1003 | BrightnessValue | rational64s |
> 0x1004 | FlashMode | int16u | 2 = On 3 = Off
> 0x1005 | FlashDevice | int16u | 0 = None 1 = Internal 4 = External 5 = Internal + External
> 0x1006 | ExposureCompensation | rational64s |
> 0x1007 | SensorTemperature | int16s |
> 0x1008 | LensTemperature | int16s |
> 0x1009 | LightCondition | int16u |
> 0x100a | FocusRange | int16u | 0 = Normal 1 = Macro
> 0x100b | FocusMode | int16u | 0 = Auto 1 = Manual
> 0x100c | ManualFocusDistance | rational64u |
> 0x100d | ZoomStepCount | int16u |
> 0x100e | FocusStepCount | int16u |
> 0x100f | Sharpness | int16u | 0 = Normal 1 = Hard 2 = Soft
> 0x1010 | FlashChargeLevel | int16u |
> 0x1011 | ColorMatrix | int16u[9] |
> 0x1012 | BlackLevel | int16u[4] |
> 0x1013 | ColorTemperatureBG? | int16u |
> 0x1014 | ColorTemperatureRG? | int16u |

> 0x1015

> WBMode

> int16u[2]

> 1 = Auto
> '1 0' = Auto
> '1 2' = Auto (2)
> '1 4' = Auto (4)
> '2 2' = 3000 Kelvin
> '2 3' = 3700 Kelvin

> '2 4' = 4000 Kelvin
> '2 5' = 4500 Kelvin
> '2 6' = 5500 Kelvin
> '2 7' = 6500 Kelvin
> '2 8' = 7500 Kelvin
> '3 0' = One-touch

> 0x1017 | RedBalance | int16u[2] |
> 0x1018 | BlueBalance | int16u[2] |
> 0x1019 | ColorMatrixNumber | int16u |
> 0x101a | SerialNumber | string |
> 0x101b | ExternalFlashAE1_0? | int32u |
> 0x101c | ExternalFlashAE2_0? | int32u |
> 0x101d | InternalFlashAE1_0? | int32u |
> 0x101e | InternalFlashAE2_0? | int32u |
> 0x101f | ExternalFlashAE1? | int32u |
> 0x1020 | ExternalFlashAE2? | int32u |
> 0x1021 | InternalFlashAE1? | int32u |
> 0x1022 | InternalFlashAE2? | int32u |
> 0x1023 | FlashExposureComp | rational64s |
> 0x1024 | InternalFlashTable | int16u |
> 0x1025 | ExternalFlashGValue | rational64s |
> 0x1026 | ExternalFlashBounce | int16u | 0 = No 1 = Yes
> 0x1027 | ExternalFlashZoom | int16u |
> 0x1028 | ExternalFlashMode | int16u |
> 0x1029 | Contrast | int16u | 0 = High 1 = Normal 2 = Low
> 0x102a | SharpnessFactor | int16u |
> 0x102b | ColorControl | int16u[6] |
> 0x102c | ValidBits | int16u[2] |
> 0x102d | CoringFilter | int16u |
> 0x102e | OlympusImageWidth | int32u |
> 0x102f | OlympusImageHeight | int32u |
> 0x1030 | SceneDetect | int16u |
> 0x1031 | SceneArea? | int32u[8] |
> 0x1033 | SceneDetectData? | int32u[720] |
> 0x1034 | CompressionRatio | rational64u |
> 0x1035 | PreviewImageValid | int32u | 0 = No 1 = Yes
> 0x1036 | PreviewImageStart | int32u* |
> 0x1037 | PreviewImageLength | int32u* |
> 0x1038 | AFResult | int16u |
> 0x1039 | CCDScanMode | int16u | 0 = Interlaced 1 = Progressive
> 0x103a | NoiseReduction | int16u | 0 = Off 1 = On
> 0x103b | FocusStepInfinity | int16u |
> 0x103c | FocusStepNear | int16u |
> 0x103d | LightValueCenter | rational64s |
> 0x103e | LightValuePeriphery | rational64s |
> 0x103f | FieldCount? | int16u |
> 0x2010 | Equipment EquipmentIFD | - - | --> Olympus Equipment Tags --> Olympus Equipment Tags
> 0x2020 | CameraSettings CameraSettingsIFD | - - | --> Olympus CameraSettings Tags --> Olympus CameraSettings Tags
> 0x2030 | RawDevelopment RawDevelopmentIFD | - - | --> Olympus RawDevelopment Tags --> Olympus RawDevelopment Tags
> 0x2031 | RawDev2 RawDev2IFD | - - | --> Olympus RawDevelopment2 Tags --> Olympus RawDevelopment2 Tags
> 0x2040 | ImageProcessing ImageProcessingIFD | - - | --> Olympus ImageProcessing Tags --> Olympus ImageProcessing Tags
> 0x2050 | FocusInfo FocusInfoIFD CameraParameters | - - undef | --> Olympus FocusInfo Tags --> Olympus FocusInfo Tags
> 0x2100 | Olympus2100 Olympus2100IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2200 | Olympus2200 Olympus2200IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2300 | Olympus2300 Olympus2300IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2400 | Olympus2400 Olympus2400IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2500 | Olympus2500 Olympus2500IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2600 | Olympus2600 Olympus2600IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2700 | Olympus2700 Olympus2700IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2800 | Olympus2800 Olympus2800IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x2900 | Olympus2900 Olympus2900IFD | - - | --> Olympus FE Tags --> Olympus FE Tags
> 0x3000 | RawInfo RawInfoIFD | - - | --> Olympus RawInfo Tags --> Olympus RawInfo Tags
> 0x4000 | MainInfo MainInfoIFD | - - | --> Olympus Tags --> Olympus Tags
> 0x5000 | UnknownInfo UnknownInfoIFD | - - | --> Olympus UnknownInfo Tags --> Olympus UnknownInfo Tags

## Olympus CameraType Values

These values are currently decoded only for Olympus models. Models with Olympus-style maker notes from other brands such as Acer, BenQ, Hitachi, HP, Premier, Konica-Minolta, Maginon, Ricoh, Rollei, SeaLife, Sony, Supra, Vivitar are not listed.

> Value | CameraType | Value | CameraType | Value | CameraType
> --- | --- | --- | --- | --- | ---
> 'D4028' | = X-2,C-50Z | 'D4381' | = uT8000,ST8000 | 'S0010' | = E-510
> 'D4029' | = E-20,E-20N,E-20P | 'D4382' | = u9000,S9000 | 'S0011' | = E-3
> 'D4034' | = C720UZ | 'D4384' | = SP590UZ | 'S0013' | = E-410
> 'D4040' | = E-1 | 'D4385' | = FE3010,X895 | 'S0016' | = E-420
> 'D4041' | = E-300 | 'D4386' | = FE3000,X890 | 'S0017' | = E-30
> 'D4083' | = C2Z,D520Z,C220Z | 'D4387' | = FE35,X30 | 'S0018' | = E-520
> 'D4106' | = u20D,S400D,u400D | 'D4388' | = u550WP,S550WP | 'S0019' | = E-P1
> 'D4120' | = X-1 | 'D4390' | = FE5000,X905 | 'S0023' | = E-620
> 'D4122' | = u10D,S300D,u300D | 'D4391' | = u5000 | 'S0026' | = E-P2
> 'D4125' | = AZ-1 | 'D4392' | = u7000,S7000 | 'S0027' | = E-PL1
> 'D4141' | = C150,D390 | 'D4396' | = FE5010,X915 | 'S0029' | = E-450
> 'D4193' | = C-5000Z | 'D4397' | = FE25,X20 | 'S0030' | = E-600
> 'D4194' | = X-3,C-60Z | 'D4398' | = FE45,X40 | 'S0032' | = E-P3
> 'D4199' | = u30D,S410D,u410D | 'D4401' | = XZ-1 | 'S0033' | = E-5
> 'D4205' | = X450,D535Z,C370Z | 'D4402' | = uT6010,ST6010 | 'S0034' | = E-PL2
> 'D4210' | = C160,D395 | 'D4406' | = u7010,S7010 / u7020,S7020 | 'S0036' | = E-M5
> 'D4211' | = C725UZ | 'D4407' | = FE4010,X930 | 'S0038' | = E-PL3
> 'D4213' | = FerrariMODEL2003 | 'D4408' | = X560WP | 'S0039' | = E-PM1
> 'D4216' | = u15D | 'D4409' | = FE26,X21 | 'S0040' | = E-PL1s
> 'D4217' | = u25D | 'D4410' | = FE4000,X920,X925 | 'S0042' | = E-PL5
> 'D4220' | = u-miniD,Stylus V | 'D4411' | = FE46,X41,X42 | 'S0043' | = E-PM2
> 'D4221' | = u40D,S500,uD500 | 'D4412' | = FE5020,X935 | 'SR45' | = D220
> 'D4231' | = FerrariMODEL2004 | 'D4413' | = uTough-3000 | 'SR55' | = D320L
> 'D4240' | = X500,D590Z,C470Z | 'D4414' | = StylusTough-6020 | 'SR83' | = D340L
> 'D4244' | = uD800,S800 | 'D4415' | = StylusTough-8010 | 'SR85' | = C830L,D340R
> 'D4256' | = u720SW,S720SW | 'D4417' | = u5010,S5010 | 'SR852' | = C860L,D360L
> 'D4261' | = X600,D630,FE5500 | 'D4418' | = u7040,S7040 | 'SR872' | = C900Z,D400Z
> 'D4262' | = uD600,S600 | 'D4419' | = u9010,S9010 | 'SR874' | = C960Z,D460Z
> 'D4301' | = u810/S810 | 'D4423' | = FE4040 | 'SR951' | = C2000Z
> 'D4302' | = u710,S710 | 'D4424' | = FE47,X43 | 'SR952' | = C21
> 'D4303' | = u700,S700 | 'D4426' | = FE4030,X950 | 'SR953' | = C21T.commu
> 'D4304' | = FE100,X710 | 'D4428' | = FE5030,X965,X960 | 'SR954' | = C2020Z
> 'D4305' | = FE110,X705 | 'D4430' | = u7030,S7030 | 'SR955' | = C990Z,D490Z
> 'D4310' | = FE-130,X-720 | 'D4432' | = SP600UZ | 'SR956' | = C211Z
> 'D4311' | = FE-140,X-725 | 'D4434' | = SP800UZ | 'SR959' | = C990ZS,D490Z
> 'D4312' | = FE150,X730 | 'D4439' | = FE4020,X940 | 'SR95A' | = C2100UZ
> 'D4313' | = FE160,X735 | 'D4442' | = FE5035 | 'SR971' | = C100,D370
> 'D4314' | = u740,S740 | 'D4448' | = FE4050,X970 | 'SR973' | = C2,D230
> 'D4315' | = u750,S750 | 'D4450' | = FE5050,X985 | 'SX151' | = E100RS
> 'D4316' | = u730/S730 | 'D4454' | = u-7050 | 'SX351' | = C3000Z / C3030Z
> 'D4317' | = FE115,X715 | 'D4464' | = T10,X27 | 'SX354' | = C3040Z
> 'D4321' | = SP550UZ | 'D4470' | = FE5040,X980 | 'SX355' | = C2040Z
> 'D4322' | = SP510UZ | 'D4472' | = TG-310 | 'SX357' | = C700UZ
> 'D4324' | = FE170,X760 | 'D4474' | = TG-610 | 'SX358' | = C200Z,D510Z
> 'D4326' | = FE200 | 'D4476' | = TG-810 | 'SX374' | = C3100Z,C3020Z
> 'D4327' | = FE190/X750 | 'D4478' | = VG145,VG140,D715 | 'SX552' | = C4040Z
> 'D4328' | = u760,S760 | 'D4479' | = VG130,D710 | 'SX553' | = C40Z,D40Z
> 'D4330' | = FE180/X745 | 'D4480' | = VG120,D705 | 'SX556' | = C730UZ
> 'D4331' | = u1000/S1000 | 'D4482' | = VR310,D720 | 'SX558' | = C5050Z
> 'D4332' | = u770SW,S770SW | 'D4484' | = VR320,D725 | 'SX571' | = C120,D380
> 'D4333' | = FE240/X795 | 'D4486' | = VR330,D730 | 'SX574' | = C300Z,D550Z
> 'D4334' | = FE210,X775 | 'D4488' | = VG110,D700 | 'SX575' | = C4100Z,C4000Z
> 'D4336' | = FE230/X790 | 'D4490' | = SP-610UZ | 'SX751' | = X200,D560Z,C350Z
> 'D4337' | = FE220,X785 | 'D4492' | = SZ-10 | 'SX752' | = X300,D565Z,C450Z
> 'D4338' | = u725SW,S725SW | 'D4494' | = SZ-20 | 'SX753' | = C750UZ
> 'D4339' | = FE250/X800 | 'D4496' | = SZ-30MR | 'SX754' | = C740UZ
> 'D4341' | = u780,S780 | 'D4498' | = SP-810UZ | 'SX755' | = C755UZ
> 'D4343' | = u790SW,S790SW | 'D4500' | = SZ-11 | 'SX756' | = C5060WZ
> 'D4344' | = u1020,S1020 | 'D4504' | = TG-615 | 'SX757' | = C8080WZ
> 'D4346' | = FE15,X10 | 'D4508' | = TG-620 | 'SX758' | = X350,D575Z,C360Z
> 'D4348' | = FE280,X820,C520 | 'D4510' | = TG-820 | 'SX759' | = X400,D580Z,C460Z
> 'D4349' | = FE300,X830 | 'D4512' | = TG-1 | 'SX75A' | = AZ-2ZOOM
> 'D4350' | = u820,S820 | 'D4516' | = SH-21 | 'SX75B' | = D595Z,C500Z
> 'D4351' | = u1200,S1200 | 'D4519' | = SZ-14 | 'SX75C' | = X550,D545Z,C480Z
> 'D4352' | = FE270,X815,C510 | 'D4520' | = SZ-31MR | 'SX75D' | = IR-300
> 'D4353' | = u795SW,S795SW | 'D4521' | = SH-25MR | 'SX75F' | = C55Z,C5500Z
> 'D4354' | = u1030SW,S1030SW | 'D4523' | = SP-720UZ | 'SX75G' | = C170,D425
> 'D4355' | = SP560UZ | 'D4529' | = VG170 | 'SX75J' | = C180,D435
> 'D4356' | = u1010,S1010 | 'D4531' | = XZ-2 | 'SX771' | = C760UZ
> 'D4357' | = u830,S830 | 'D4535' | = SP-620UZ | 'SX772' | = C770UZ
> 'D4359' | = u840,S840 | 'D4536' | = TG-320 | 'SX773' | = C745UZ
> 'D4360' | = FE350WIDE,X865 | 'D4537' | = VR340,D750 | 'SX774' | = X250,D560Z,C350Z
> 'D4361' | = u850SW,S850SW | 'D4541' | = SZ-12 | 'SX775' | = X100,D540Z,C310Z
> 'D4362' | = FE340,X855,C560 | 'D4545' | = VH410 | 'SX776' | = C460ZdelSol
> 'D4363' | = FE320,X835,C540 | 'D4547' | = TG-2 | 'SX777' | = C765UZ
> 'D4364' | = SP570UZ | 'D4548' | = TG-830 | 'SX77A' | = D555Z,C315Z
> 'D4366' | = FE330,X845,C550 | 'D4562' | = SP-820UZ | 'SX851' | = C7070WZ
> 'D4368' | = FE310,X840,C530 | 'D4809' | = C2500L | 'SX852' | = C70Z,C7000Z
> 'D4370' | = u1050SW,S1050SW | 'D4842' | = E-10 | 'SX853' | = SP500UZ
> 'D4371' | = u1060,S1060 | 'D4856' | = C-1 | 'SX854' | = SP310
> 'D4372' | = FE370,X880,C575 | 'D4857' | = C-1Z,D-150Z | 'SX855' | = SP350
> 'D4374' | = SP565UZ | 'DCHC' | = D500L | 'SX873' | = SP320
> 'D4377' | = u1040,S1040 | 'DCHT' | = D600L / D620L | 'SX875' | = FE180/X745
> 'D4378' | = FE360,X875,C570 | 'S0003' | = E-330 | 'SX876' | = FE190/X750
> 'D4379' | = FE20,X15,C25 | 'S0004' | = E-500 |  |
> 'D4380' | = uT6000,ST6000 | 'S0009' | = E-400 |  |

## Olympus TextInfo Tags

This information is in text format (similar to APP12 information, but with spaces instead of linefeeds). Below are tags which have been observed, but any information found here will be extracted, even if the tag is not listed.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'Resolution' | Resolution | N |
> 'Type' | CameraType | N | --> Olympus CameraType Values

## Olympus Equipment Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | EquipmentVersion | undef[4] |
> 0x0100 | CameraType2 | string[6] | --> Olympus CameraType Values
> 0x0101 | SerialNumber | string[32] |
> 0x0102 | InternalSerialNumber | string[32] | (16 digits: 0-3=model, 4=year, 5-6=month, 8-12=unit number)
> 0x0103 | FocalPlaneDiagonal | rational64u |
> 0x0104 | BodyFirmwareVersion | int32u |
> 0x0201 | LensType | int8u[6] | --> Olympus LensType Values (6 numbers: 0. Make, 1. Unknown, 2. Model, 3. Sub-model, 4-5. Unknown. Only the Make, Model and Sub-model are used to identify the lens type)
> 0x0202 | LensSerialNumber | string[32] |
> 0x0203 | LensModel | string |
> 0x0204 | LensFirmwareVersion | int32u |
> 0x0205 | MaxApertureAtMinFocal | int16u |
> 0x0206 | MaxApertureAtMaxFocal | int16u |
> 0x0207 | MinFocalLength | int16u |
> 0x0208 | MaxFocalLength | int16u |
> 0x020a | MaxAperture | int16u |
> 0x020b | LensProperties | int16u |
> 0x0301 | Extender | int8u[6] | (6 numbers: 0. Make, 1. Unknown, 2. Model, 3. Sub-model, 4-5. Unknown. Only the Make and Model are used to identify the extender) '0 00' = None '0 04' = Olympus Zuiko Digital EC-14 1.4x Teleconverter '0 08' = Olympus EX-25 Extension Tube '0 10' = Olympus Zuiko Digital EC-20 2.0x Teleconverter
> 0x0302 | ExtenderSerialNumber | string[32] |
> 0x0303 | ExtenderModel | string |
> 0x0304 | ExtenderFirmwareVersion | int32u |
> 0x0403 | ConversionLens | string |
> 0x1000 | FlashType | int16u | 0 = None 2 = Simple E-System 3 = E-System

> 0x1001

> FlashModel

> int16u

> 0 = None 1 = FL-20 2 = FL-50 3 = RF-11 |  | 4 = TF-22 5 = FL-36 6 = FL-50R 7 = FL-36R |

> 0x1002 | FlashFirmwareVersion | int32u |
> 0x1003 | FlashSerialNumber | string[32] |

## Olympus LensType Values

The numerical values below are given in hexadecimal. (Prior to ExifTool 9.15 these were in decimal.)

> Value | LensType
> --- | ---
> '0 00 00' | = None
> '0 01 00' | = Olympus Zuiko Digital ED 50mm F2.0 Macro
> '0 01 01' | = Olympus Zuiko Digital 40-150mm F3.5-4.5
> '0 01 10' | = Olympus M.Zuiko Digital ED 14-42mm F3.5-5.6
> '0 02 00' | = Olympus Zuiko Digital ED 150mm F2.0
> '0 02 10' | = Olympus M.Zuiko Digital 17mm F2.8 Pancake
> '0 03 00' | = Olympus Zuiko Digital ED 300mm F2.8
> '0 03 10' | = Olympus M.Zuiko Digital ED 14-150mm F4.0-5.6
> '0 04 10' | = Olympus M.Zuiko Digital ED 9-18mm F4.0-5.6
> '0 05 00' | = Olympus Zuiko Digital 14-54mm F2.8-3.5
> '0 05 01' | = Olympus Zuiko Digital Pro ED 90-250mm F2.8
> '0 05 10' | = Olympus M.Zuiko Digital ED 14-42mm F3.5-5.6 L
> '0 06 00' | = Olympus Zuiko Digital ED 50-200mm F2.8-3.5
> '0 06 01' | = Olympus Zuiko Digital ED 8mm F3.5 Fisheye
> '0 06 10' | = Olympus M.Zuiko Digital ED 40-150mm F4.0-5.6
> '0 07 00' | = Olympus Zuiko Digital 11-22mm F2.8-3.5
> '0 07 01' | = Olympus Zuiko Digital 18-180mm F3.5-6.3
> '0 07 10' | = Olympus M.Zuiko Digital ED 12mm F2.0
> '0 08 01' | = Olympus Zuiko Digital 70-300mm F4.0-5.6
> '0 08 10' | = Olympus M.Zuiko Digital ED 75-300mm F4.8-6.7
> '0 09 10' | = Olympus M.Zuiko Digital 14-42mm F3.5-5.6 II
> '0 10 01' | = Kenko Tokina Reflex 300mm F6.3 MF Macro
> '0 10 10' | = Olympus M.Zuiko Digital ED 12-50mm F3.5-6.3 EZ
> '0 11 10' | = Olympus M.Zuiko Digital 45mm F1.8
> '0 12 10' | = Olympus M.Zuiko Digital ED 60mm F2.8 Macro
> '0 13 10' | = Olympus M.Zuiko Digital ED 14-42mm F3.5-5.6 II R
> '0 14 10' | = Olympus M.Zuiko Digital ED 40-150mm F4.0-5.6 R
> '0 15 00' | = Olympus Zuiko Digital ED 7-14mm F4.0
> '0 15 10' | = Olympus M.Zuiko Digital ED 75mm F1.8
> '0 16 10' | = Olympus M.Zuiko Digital 17mm F1.8
> '0 17 00' | = Olympus Zuiko Digital Pro ED 35-100mm F2.0
> '0 18 00' | = Olympus Zuiko Digital 14-45mm F3.5-5.6
> '0 18 10' | = Olympus M.Zuiko Digital ED 75-300mm F4.8-6.7 II
> '0 20 00' | = Olympus Zuiko Digital 35mm F3.5 Macro
> '0 22 00' | = Olympus Zuiko Digital 17.5-45mm F3.5-5.6
> '0 23 00' | = Olympus Zuiko Digital ED 14-42mm F3.5-5.6
> '0 24 00' | = Olympus Zuiko Digital ED 40-150mm F4.0-5.6
> '0 30 00' | = Olympus Zuiko Digital ED 50-200mm F2.8-3.5 SWD
> '0 31 00' | = Olympus Zuiko Digital ED 12-60mm F2.8-4.0 SWD
> '0 32 00' | = Olympus Zuiko Digital ED 14-35mm F2.0 SWD
> '0 33 00' | = Olympus Zuiko Digital 25mm F2.8
> '0 34 00' | = Olympus Zuiko Digital ED 9-18mm F4.0-5.6
> '0 35 00' | = Olympus Zuiko Digital 14-54mm F2.8-3.5 II
> '1 01 00' | = Sigma 18-50mm F3.5-5.6 DC
> '1 01 10' | = Sigma 30mm F2.8 EX DN
> '1 02 00' | = Sigma 55-200mm F4.0-5.6 DC
> '1 02 10' | = Sigma 19mm F2.8 EX DN
> '1 03 00' | = Sigma 18-125mm F3.5-5.6 DC
> '1 04 00' | = Sigma 18-125mm F3.5-5.6 DC
> '1 05 00' | = Sigma 30mm F1.4 EX DC HSM
> '1 06 00' | = Sigma APO 50-500mm F4.0-6.3 EX DG HSM
> '1 07 00' | = Sigma Macro 105mm F2.8 EX DG
> '1 08 00' | = Sigma APO Macro 150mm F2.8 EX DG HSM
> '1 09 00' | = Sigma 18-50mm F2.8 EX DC Macro
> '1 10 00' | = Sigma 24mm F1.8 EX DG Aspherical Macro
> '1 11 00' | = Sigma APO 135-400mm F4.5-5.6 DG
> '1 12 00' | = Sigma APO 300-800mm F5.6 EX DG HSM
> '1 13 00' | = Sigma 30mm F1.4 EX DC HSM
> '1 14 00' | = Sigma APO 50-500mm F4.0-6.3 EX DG HSM
> '1 15 00' | = Sigma 10-20mm F4.0-5.6 EX DC HSM
> '1 16 00' | = Sigma APO 70-200mm F2.8 II EX DG Macro HSM
> '1 17 00' | = Sigma 50mm F1.4 EX DG HSM
> '2 01 00' | = Leica D Vario Elmarit 14-50mm F2.8-3.5 Asph.
> '2 01 10' | = Lumix G Vario 14-45mm F3.5-5.6 Asph. Mega OIS
> '2 02 00' | = Leica D Summilux 25mm F1.4 Asph.
> '2 02 10' | = Lumix G Vario 45-200mm F4.0-5.6 Mega OIS
> '2 03 00' | = Leica D Vario Elmar 14-50mm F3.8-5.6 Asph. Mega OIS
> '2 03 01' | = Leica D Vario Elmar 14-50mm F3.8-5.6 Asph.
> '2 03 10' | = Lumix G Vario HD 14-140mm F4.0-5.8 Asph. Mega OIS
> '2 04 00' | = Leica D Vario Elmar 14-150mm F3.5-5.6
> '2 04 10' | = Lumix G Vario 7-14mm F4.0 Asph.
> '2 05 10' | = Lumix G 20mm F1.7 Asph.
> '2 06 10' | = Leica DG Macro-Elmarit 45mm F2.8 Asph. Mega OIS
> '2 07 10' | = Lumix G Vario 14-42mm F3.5-5.6 Asph. Mega OIS
> '2 08 10' | = Lumix G Fisheye 8mm F3.5
> '2 09 10' | = Lumix G Vario 100-300mm F4.0-5.6 Mega OIS
> '2 10 10' | = Lumix G 14mm F2.5 Asph.
> '2 11 10' | = Lumix G 12.5mm F12 3D
> '2 12 10' | = Leica DG Summilux 25mm F1.4 Asph.
> '2 13 10' | = Lumix G X Vario PZ 45-175mm F4.0-5.6 Asph. Power OIS
> '2 14 10' | = Lumix G X Vario PZ 14-42mm F3.5-5.6 Asph. Power OIS
> '2 15 10' | = Lumix G X Vario 12-35mm F2.8 Asph. Power OIS
> '2 16 10' | = Lumix G Vario 45-150mm F4.0-5.6 Asph. Mega OIS
> '2 17 10' | = Lumix G X Vario 35-100mm F2.8 Power OIS
> '3 01 00' | = Leica D Vario Elmarit 14-50mm F2.8-3.5 Asph.
> '3 02 00' | = Leica D Summilux 25mm F1.4 Asph.

## Olympus CameraSettings Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | CameraSettingsVersion | undef[4] |
> 0x0100 | PreviewImageValid | int32u | 0 = No 1 = Yes
> 0x0101 | PreviewImageStart | int32u* |
> 0x0102 | PreviewImageLength | int32u* |
> 0x0200 | ExposureMode | int16u | 1 = Manual 2 = Program 3 = Aperture-priority AE 4 = Shutter speed priority AE 5 = Program-shift
> 0x0201 | AELock | int16u | 0 = Off 1 = On

> 0x0202

> MeteringMode

> int16u

> 2 = Center-weighted average
> 3 = Spot
> 5 = ESP
> 261 = Pattern+AF
> 515 = Spot+Highlight control
> 1027 = Spot+Shadow control

> 0x0203 | ExposureShift | rational64s |
> 0x0300 | MacroMode | int16u | 0 = Off 1 = On 2 = Super Macro

> 0x0301

> FocusMode

> int16u[n]

> (1 or 2 values)
> [Value 0]

> 0 = Single AF
> 1 = Sequential shooting AF
> 2 = Continuous AF
> 3 = Multi AF
> 5 = Face detect
> 10 = MF

> [Value 1]

> Bit 0 = S-AF Bit 2 = C-AF Bit 4 = MF |  | Bit 5 = Face detect Bit 6 = Imager AF Bit 8 = AF sensor |

> 0x0302 | FocusProcess | int16u[n] | (1 or 2 values) [Value 0] 0 = AF Not Used 1 = AF Used
> 0x0303 | AFSearch | int16u | 0 = Not Ready 1 = Ready
> 0x0304 | AFAreas | int32u[64]~ | (coordinates range from 0 to 255)
> 0x0305 | AFPointSelected | rational64s[5]~ | (coordinates expressed as a percent)
> 0x0306 | AFFineTune | int8u | 0 = Off 1 = On
> 0x0307 | AFFineTuneAdj | int16s[3] |

> 0x0400

> FlashMode

> int16u

> 0x0 = Off Bit 0 = On Bit 1 = Fill-in Bit 2 = Red-eye |  | Bit 3 = Slow-sync Bit 4 = Forced On Bit 5 = 2nd Curtain |

> 0x0401 | FlashExposureComp | rational64s |

> 0x0403

> FlashRemoteControl

> int16u

> 0x0 = Off
> 0x1 = Channel 1, Low
> 0x2 = Channel 2, Low
> 0x3 = Channel 3, Low
> 0x4 = Channel 4, Low
> 0x9 = Channel 1, Mid
> 0xa = Channel 2, Mid

> 0xb = Channel 3, Mid
> 0xc = Channel 4, Mid
> 0x11 = Channel 1, High
> 0x12 = Channel 2, High
> 0x13 = Channel 3, High
> 0x14 = Channel 4, High

> 0x0404 | FlashControlMode | int16u[3] | [Value 0] 0 = Off 3 = TTL 4 = Auto 5 = Manual
> 0x0405 | FlashIntensity | rational64s[3] |
> 0x0406 | ManualFlashStrength | rational64s[3] |

> 0x0500

> WhiteBalance2

> int16u

> 0 = Auto
> 16 = 7500K (Fine Weather with Shade)
> 17 = 6000K (Cloudy)
> 18 = 5300K (Fine Weather)
> 20 = 3000K (Tungsten light)
> 21 = 3600K (Tungsten light-like)
> 33 = 6600K (Daylight fluorescent)
> 34 = 4500K (Neutral white fluorescent)
> 35 = 4000K (Cool white fluorescent)
> 48 = 3600K (Tungsten light-like)
> 256 = Custom WB 1
> 257 = Custom WB 2
> 258 = Custom WB 3
> 259 = Custom WB 4
> 512 = Custom WB 5400K
> 513 = Custom WB 2900K
> 514 = Custom WB 8000K

> 0x0501 | WhiteBalanceTemperature | int16u |
> 0x0502 | WhiteBalanceBracket | int16s |
> 0x0503 | CustomSaturation | int16s[3]~ | (3 numbers: 1. CS Value, 2. Min, 3. Max)
> 0x0504 | ModifiedSaturation | int16u | 0 = Off 1 = CM1 (Red Enhance) 2 = CM2 (Green Enhance) 3 = CM3 (Blue Enhance) 4 = CM4 (Skin Tones)
> 0x0505 | ContrastSetting | int16s[3] | (value, min, max)
> 0x0506 | SharpnessSetting | int16s[3] | (value, min, max)
> 0x0507 | ColorSpace | int16u | 0 = sRGB 1 = Adobe RGB 2 = Pro Photo RGB

> 0x0509

> SceneMode

> int16u

> 0 = Standard
> 6 = Auto
> 7 = Sport
> 8 = Portrait
> 9 = Landscape+Portrait
> 10 = Landscape
> 11 = Night Scene
> 12 = Self Portrait
> 13 = Panorama
> 14 = 2 in 1
> 15 = Movie
> 16 = Landscape+Portrait
> 17 = Night+Portrait
> 18 = Indoor
> 19 = Fireworks
> 20 = Sunset
> 21 = Beauty Skin
> 22 = Macro
> 23 = Super Macro
> 24 = Food
> 25 = Documents
> 26 = Museum
> 27 = Shoot & Select
> 28 = Beach & Snow
> 29 = Self Protrait+Timer
> 30 = Candle
> 31 = Available Light
> 32 = Behind Glass
> 33 = My Mode

> 34 = Pet
> 35 = Underwater Wide1
> 36 = Underwater Macro
> 37 = Shoot & Select1
> 38 = Shoot & Select2
> 39 = High Key
> 40 = Digital Image Stabilization
> 41 = Auction
> 42 = Beach
> 43 = Snow
> 44 = Underwater Wide2
> 45 = Low Key
> 46 = Children
> 47 = Vivid
> 48 = Nature Macro
> 49 = Underwater Snapshot
> 50 = Shooting Guide
> 54 = Face Portrait
> 57 = Bulb
> 59 = Smile Shot
> 60 = Quick Shutter
> 63 = Slow Shutter
> 64 = Bird Watching
> 65 = Multiple Exposure
> 66 = e-Portrait
> 67 = Soft Background Shot
> 142 = Hand-held Starlight
> 154 = HDR

> 0x050a | NoiseReduction | int16u | Bit 0 = Noise Reduction Bit 1 = Noise Filter Bit 2 = Noise Filter (ISO Boost) Bit 3 = Auto
> 0x050b | DistortionCorrection | int16u | 0 = Off 1 = On
> 0x050c | ShadingCompensation | int16u | 0 = Off 1 = On
> 0x050d | CompressionFactor | rational64u |

> 0x050f

> Gradation

> int16s[n]

> (3 or 4 values)
> [Values 0-2]
> '-1 -1 1' = Low Key
> '0 -1 1' = Normal
> '0 0 0' = n/a
> '1 -1 1' = High Key
> [Value 3]
> 0 = User-Selected
> 1 = Auto-Override

> 0x0520

> PictureMode

> int16u[n]

> (1 or 2 values)
> [Value 0]

> 1 = Vivid 2 = Natural 3 = Muted 4 = Portrait |  | 5 = i-Enhance 256 = Monotone 512 = Sepia |

> 0x0521 | PictureModeSaturation | int16s[3] | (value, min, max)
> 0x0522 | PictureModeHue? | int16s |
> 0x0523 | PictureModeContrast | int16s[3] | (value, min, max)
> 0x0524 | PictureModeSharpness | int16s[3] | (value, min, max)

> 0x0525

> PictureModeBWFilter

> int16s

> 0 = n/a 1 = Neutral 2 = Yellow |  | 3 = Orange 4 = Red 5 = Green |

> 0x0526

> PictureModeTone

> int16s

> 0 = n/a 1 = Neutral 2 = Sepia |  | 3 = Blue 4 = Purple 5 = Green |

> 0x0527 | NoiseFilter | int16s[3] | '-1 -2 1' = Low '-2 -2 1' = Off '0 -2 1' = Standard '0 0 0' = n/a '1 -2 1' = High

> 0x0529

> ArtFilter

> int16u[4]

> [Value 0]

> 0 = Off
> 1 = Soft Focus
> 2 = Pop Art
> 3 = Pale & Light Color
> 4 = Light Tone
> 5 = Pin Hole
> 6 = Grainy Film
> 9 = Diorama
> 10 = Cross Process
> 12 = Fish Eye
> 13 = Drawing
> 14 = Gentle Sepia
> 15 = Tender Light
> 16 = Pop Art II

> 17 = Pin Hole II
> 18 = Pin Hole III
> 19 = Grainy Film II
> 20 = Dramatic Tone
> 21 = Punk
> 22 = Soft Focus 2
> 23 = Sparkle
> 24 = Watercolor
> 25 = Key Line
> 27 = Miniature
> 28 = Reflection
> 29 = Fragmented
> 32 = Dramatic Tone B&W
> 33 = Watercolor II

> 0x052c

> MagicFilter

> int16u[4]

> [Value 0]

> 0 = Off
> 1 = Soft Focus
> 2 = Pop Art
> 3 = Pale & Light Color
> 4 = Light Tone
> 5 = Pin Hole
> 6 = Grainy Film
> 9 = Diorama
> 10 = Cross Process
> 12 = Fish Eye
> 13 = Drawing
> 14 = Gentle Sepia
> 15 = Tender Light
> 16 = Pop Art II

> 17 = Pin Hole II
> 18 = Pin Hole III
> 19 = Grainy Film II
> 20 = Dramatic Tone
> 21 = Punk
> 22 = Soft Focus 2
> 23 = Sparkle
> 24 = Watercolor
> 25 = Key Line
> 27 = Miniature
> 28 = Reflection
> 29 = Fragmented
> 32 = Dramatic Tone B&W
> 33 = Watercolor II

> 0x052d | PictureModeEffect | int16s[3] | '-1 -1 1' = Low '0 -1 1' = Standard '0 0 0' = n/a '1 -1 1' = High

> 0x052f

> ArtFilterEffect

> int16u[20]

> [Value 0]

> 0x0 = Off
> 0x1 = Soft Focus
> 0x2 = Pop Art
> 0x3 = Pale & Light Color
> 0x4 = Light Tone
> 0x5 = Pin Hole
> 0x6 = Grainy Film
> 0x9 = Diorama
> 0xa = Cross Process
> 0xc = Fish Eye
> 0xd = Drawing
> 0xe = Gentle Sepia
> 0xf = Tender Light
> 0x10 = Pop Art II

> 0x11 = Pin Hole II
> 0x12 = Pin Hole III
> 0x13 = Grainy Film II
> 0x14 = Dramatic Tone
> 0x15 = Punk
> 0x16 = Soft Focus 2
> 0x17 = Sparkle
> 0x18 = Watercolor
> 0x19 = Key Line
> 0x1b = Miniature
> 0x1c = Reflection
> 0x1d = Fragmented
> 0x20 = Dramatic Tone B&W
> 0x21 = Watercolor II

> [Value 4]

> 0x0 = No Effect 0x8010 = Star Light 0x8020 = Pin Hole 0x8030 = Frame |  | 0x8040 = Soft Focus 0x8050 = White Edge 0x8060 = B&W |

> 0x0600 | DriveMode | int16u[n]~ | (2 or 3 numbers: 1. Mode, 2. Shot number, 3. Mode bits)
> 0x0601 | PanoramaMode | int16u~ | (2 numbers: 1. Mode, 2. Shot number)
> 0x0603 | ImageQuality2 | int16u | 1 = SQ 2 = HQ 3 = SHQ 4 = RAW 5 = SQ (5)
> 0x0604 | ImageStabilization | int32u | 0 = Off 1 = On, Mode 1 2 = On, Mode 2 3 = On, Mode 3
> 0x0900 | ManometerPressure | int16u |
> 0x0901 | ManometerReading | int32s[2] |
> 0x0902 | ExtendedWBDetect | int16u | 0 = Off 1 = On
> 0x0903 | LevelGaugeRoll | int16u | 0 = Off 1 = On
> 0x0904 | LevelGaugePitch | int16u | 0 = Off 1 = On

## Olympus RawDevelopment Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | RawDevVersion | undef[4] |
> 0x0100 | RawDevExposureBiasValue | rational64s |
> 0x0101 | RawDevWhiteBalanceValue | int16u |
> 0x0102 | RawDevWBFineAdjustment | int16s |
> 0x0103 | RawDevGrayPoint | int16u[3] |
> 0x0104 | RawDevSaturationEmphasis | int16s[3] |
> 0x0105 | RawDevMemoryColorEmphasis | int16u |
> 0x0106 | RawDevContrastValue | int16s[3] |
> 0x0107 | RawDevSharpnessValue | int16s[3] |
> 0x0108 | RawDevColorSpace | int16u | 0 = sRGB 1 = Adobe RGB 2 = Pro Photo RGB
> 0x0109 | RawDevEngine | int16u | 0 = High Speed 1 = High Function 2 = Advanced High Speed 3 = Advanced High Function
> 0x010a | RawDevNoiseReduction | int16u | Bit 0 = Noise Reduction Bit 1 = Noise Filter Bit 2 = Noise Filter (ISO Boost)
> 0x010b | RawDevEditStatus | int16u | 0 = Original 1 = Edited (Landscape) 6 = Edited (Portrait) 8 = Edited (Portrait)

> 0x010c

> RawDevSettings

> int16u

> Bit 0 = WB Color Temp Bit 1 = WB Gray Point Bit 2 = Saturation Bit 3 = Contrast |  | Bit 4 = Sharpness Bit 5 = Color Space Bit 6 = High Function Bit 7 = Noise Reduction |

## Olympus RawDevelopment2 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | RawDevVersion | undef[4] |
> 0x0100 | RawDevExposureBiasValue | rational64s |
> 0x0101 | RawDevWhiteBalance | int16u | 1 = Color Temperature 2 = Gray Point
> 0x0102 | RawDevWhiteBalanceValue | int16u |
> 0x0103 | RawDevWBFineAdjustment | int16s |
> 0x0104 | RawDevGrayPoint | int16u[3] |
> 0x0105 | RawDevContrastValue | int16s[3] |
> 0x0106 | RawDevSharpnessValue | int16s[3] |
> 0x0107 | RawDevSaturationEmphasis | int16s[3] |
> 0x0108 | RawDevMemoryColorEmphasis | int16u |
> 0x0109 | RawDevColorSpace | int16u | 0 = sRGB 1 = Adobe RGB 2 = Pro Photo RGB
> 0x010a | RawDevNoiseReduction | int16u | Bit 0 = Noise Reduction Bit 1 = Noise Filter Bit 2 = Noise Filter (ISO Boost)
> 0x010b | RawDevEngine | int16u | 0 = High Speed 1 = High Function
> 0x010c | RawDevPictureMode | int16u | 1 = Vivid 2 = Natural 3 = Muted 256 = Monotone 512 = Sepia
> 0x010d | RawDevPMSaturation | int16s[3] |
> 0x010e | RawDevPMContrast | int16s[3] |
> 0x010f | RawDevPMSharpness | int16s[3] |
> 0x0110 | RawDevPM_BWFilter | int16u | 1 = Neutral 2 = Yellow 3 = Orange 4 = Red 5 = Green
> 0x0111 | RawDevPMPictureTone | int16u | 1 = Neutral 2 = Sepia 3 = Blue 4 = Purple 5 = Green
> 0x0112 | RawDevGradation | int16s[3] |
> 0x0113 | RawDevSaturation3 | int16s[3] |
> 0x0119 | RawDevAutoGradation | int16u | 0 = Off 1 = On
> 0x0120 | RawDevPMNoiseFilter | int16u |

## Olympus ImageProcessing Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | ImageProcessingVersion | undef[4] |
> 0x0100 | WB_RBLevels | int16u[2] |
> 0x0102 | WB_RBLevels3000K | int16u[2] |
> 0x0103 | WB_RBLevels3300K | int16u[2] |
> 0x0104 | WB_RBLevels3600K | int16u[2] |
> 0x0105 | WB_RBLevels3900K | int16u[2] |
> 0x0106 | WB_RBLevels4000K | int16u[2] |
> 0x0107 | WB_RBLevels4300K | int16u[2] |
> 0x0108 | WB_RBLevels4500K | int16u[2] |
> 0x0109 | WB_RBLevels4800K | int16u[2] |
> 0x010a | WB_RBLevels5300K | int16u[2] |
> 0x010b | WB_RBLevels6000K | int16u[2] |
> 0x010c | WB_RBLevels6600K | int16u[2] |
> 0x010d | WB_RBLevels7500K | int16u[2] |
> 0x010e | WB_RBLevelsCWB1 | int16u[2] |
> 0x010f | WB_RBLevelsCWB2 | int16u[2] |
> 0x0110 | WB_RBLevelsCWB3 | int16u[2] |
> 0x0111 | WB_RBLevelsCWB4 | int16u[2] |
> 0x0113 | WB_GLevel3000K | int16u |
> 0x0114 | WB_GLevel3300K | int16u |
> 0x0115 | WB_GLevel3600K | int16u |
> 0x0116 | WB_GLevel3900K | int16u |
> 0x0117 | WB_GLevel4000K | int16u |
> 0x0118 | WB_GLevel4300K | int16u |
> 0x0119 | WB_GLevel4500K | int16u |
> 0x011a | WB_GLevel4800K | int16u |
> 0x011b | WB_GLevel5300K | int16u |
> 0x011c | WB_GLevel6000K | int16u |
> 0x011d | WB_GLevel6600K | int16u |
> 0x011e | WB_GLevel7500K | int16u |
> 0x011f | WB_GLevel | int16u |
> 0x0200 | ColorMatrix | int16u[9] |
> 0x0300 | Enhancer | int16u |
> 0x0301 | EnhancerValues | int16u[7] |
> 0x0310 | CoringFilter | int16u |
> 0x0311 | CoringValues | int16u[7] |
> 0x0600 | BlackLevel2 | int16u[4] |
> 0x0610 | GainBase | int16u |
> 0x0611 | ValidBits | int16u[2] |
> 0x0612 | CropLeft | int16u[2] |
> 0x0613 | CropTop | int16u[2] |
> 0x0614 | CropWidth | int32u |
> 0x0615 | CropHeight | int32u |
> 0x0635 | UnknownBlock1? | undef | (large unknown data block in ORF images but not JPG images)
> 0x0636 | UnknownBlock2? | undef | (large unknown data block in ORF images but not JPG images)
> 0x1010 | NoiseReduction2 | int16u | Bit 0 = Noise Reduction Bit 1 = Noise Filter Bit 2 = Noise Filter (ISO Boost)
> 0x1011 | DistortionCorrection2 | int16u | 0 = Off 1 = On
> 0x1012 | ShadingCompensation2 | int16u | 0 = Off 1 = On
> 0x101c | MultipleExposureMode | int16u[2] | [Value 0] 0 = Off 2 = On (2 frames) 3 = On (3 frames)
> 0x1103 | UnknownBlock3? | undef | (large unknown data block in ORF images but not JPG images)
> 0x1104 | UnknownBlock4? | undef | (large unknown data block in ORF images but not JPG images)

> 0x1112

> AspectRatio

> int8u[2]

> '1 1' = 4:3 '2 2' = 3:2 '3 3' = 16:9 |  | '4 4' = 6:6 '5 5' = 5:4 '6 6' = 7:6 |  | '7 7' = 6:5 '8 8' = 7:5 '9 9' = 3:4 |

> 0x1113 | AspectFrame | int16u[4] |
> 0x1200 | FacesDetected | int32u[n] | (2 or 3 values)
> 0x1201 | FaceDetectArea | int16s[n] | (for models with 2 values in FacesDetected this gives X/Y coordinates in the FaceDetectFrame for all 4 corners of the face rectangle. For models with 3 values in FacesDetected this gives X/Y coordinates, size and rotation angle of the face detect square)
> 0x1202 | MaxFaces | int32u[3] |
> 0x1203 | FaceDetectFrameSize | int16u[6] | (width/height of the full face detect frame)
> 0x1207 | FaceDetectFrameCrop | int16s[12] | (X/Y offset and width/height of the cropped face detect frame)

## Olympus FocusInfo Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | FocusInfoVersion | undef[4] |
> 0x0209 | AutoFocus? | int16u | 0 = Off 1 = On
> 0x0210 | SceneDetect | int16u |
> 0x0211 | SceneArea? | int32u[8] |
> 0x0212 | SceneDetectData? | int32u[720] |
> 0x0300 | ZoomStepCount | int16u |
> 0x0301 | FocusStepCount | int16u |
> 0x0303 | FocusStepInfinity | int16u |
> 0x0304 | FocusStepNear | int16u |
> 0x0305 | FocusDistance | rational64u |

> 0x0308

> AFPoint

> int16u

> (for the E-3, E-5 and E-30 the value is separated into 2 parts: low 5 bits give AF point, upper bits give AF target selection mode)
> [Value 0]

> 0x0 = (none)
> 0x1 = Top-left (horizontal)
> 0x2 = Top-center (horizontal)
> 0x3 = Top-right (horizontal)
> 0x4 = Left (horizontal)
> 0x5 = Mid-left (horizontal)
> 0x6 = Center (horizontal)
> 0x7 = Mid-right (horizontal)
> 0x8 = Right (horizontal)
> 0x9 = Bottom-left (horizontal)
> 0xa = Bottom-center (horizontal)
> 0xb = Bottom-right (horizontal)

> 0xc = Top-left (vertical)
> 0xd = Top-center (vertical)
> 0xe = Top-right (vertical)
> 0xf = Left (vertical)
> 0x10 = Mid-left (vertical)
> 0x11 = Center (vertical)
> 0x12 = Mid-right (vertical)
> 0x13 = Right (vertical)
> 0x14 = Bottom-left (vertical)
> 0x15 = Bottom-center (vertical)
> 0x16 = Bottom-right (vertical)
> 0x1f = n/a

> [Value 1]

> 0x0 = Single Target 0x40 = All Target |  | 0x80 = Dynamic Single Target 0xe0 = n/a |

> (models with 7-point AF)
> [Value 0]
> 0x0 = (none)
> 0x1 = Center
> [Value 1]
> 0x0 = Single Target
> 0x40 = All Target
> (other models)
> 0 = Left (or n/a)
> 1 = Center (horizontal)
> 2 = Right
> 3 = Center (vertical)
> 255 = None

> 0x1201 | ExternalFlash | int16u[2] | '0 0' = Off '1 0' = On
> 0x1203 | ExternalFlashGuideNumber? | rational64s |
> 0x1204 | ExternalFlashBounce | int16u | 0 = Bounce or Off 1 = Direct
> 0x1205 | ExternalFlashZoom | rational64u |
> 0x1208 | InternalFlash | int16u[n] | 0 = Off 1 = On '0 0' = Off '1 0' = On
> 0x1209 | ManualFlash | int16u[2]~ | (2 numbers: 1. 0=Off, 1=On, 2. Flash strength)
> 0x120a | MacroLED | int16u | 0 = Off 1 = On
> 0x1500 | SensorTemperature | int16s | (approximately Celsius for E-1, unknown calibration for E-3/410/420/510, and always zero for E-300/330/400/500, divide by 10 for E-P1?)
> 0x1600 | ImageStabilization | undef~ |

## Olympus FE Tags

Some FE models write a large number of tags here, but most of this information remains unknown.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0100 | BodyFirmwareVersion | string |

## Olympus RawInfo Tags

These tags are found only in ORF images of some models (ie. C8080WZ).

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | RawInfoVersion | undef[4] |
> 0x0100 | WB_RBLevelsUsed | int16u[2] |
> 0x0110 | WB_RBLevelsAuto | int16u[2] |
> 0x0120 | WB_RBLevelsShade | int16u[2] |
> 0x0121 | WB_RBLevelsCloudy | int16u[2] |
> 0x0122 | WB_RBLevelsFineWeather | int16u[2] |
> 0x0123 | WB_RBLevelsTungsten | int16u[2] |
> 0x0124 | WB_RBLevelsEveningSunlight | int16u[2] |
> 0x0130 | WB_RBLevelsDaylightFluor | int16u[2] |
> 0x0131 | WB_RBLevelsDayWhiteFluor | int16u[2] |
> 0x0132 | WB_RBLevelsCoolWhiteFluor | int16u[2] |
> 0x0133 | WB_RBLevelsWhiteFluorescent | int16u[2] |
> 0x0200 | ColorMatrix2 | int16u[9] |
> 0x0310 | CoringFilter | int16u |
> 0x0311 | CoringValues | int16u[11] |
> 0x0600 | BlackLevel2 | int16u[4] |
> 0x0601 | YCbCrCoefficients | N | (stored as int16u[6], but extracted as rational32u[3])
> 0x0611 | ValidPixelDepth | int16u[2] |
> 0x0612 | CropLeft | int16u |
> 0x0613 | CropTop | int16u |
> 0x0614 | CropWidth | int32u |
> 0x0615 | CropHeight | int32u |

> 0x1000

> LightSource

> int16u

> 0 = Unknown
> 16 = Shade
> 17 = Cloudy
> 18 = Fine Weather
> 20 = Tungsten (Incandescent)
> 22 = Evening Sunlight
> 33 = Daylight Fluorescent
> 34 = Day White Fluorescent
> 35 = Cool White Fluorescent
> 36 = White Fluorescent
> 256 = One Touch White Balance
> 512 = Custom 1-4

> 0x1001 | WhiteBalanceComp | int16s[3] |
> 0x1010 | SaturationSetting | int16s[3] |
> 0x1011 | HueSetting | int16s[3] |
> 0x1012 | ContrastSetting | int16s[3] |
> 0x1013 | SharpnessSetting | int16s[3] |
> 0x2000 | CMExposureCompensation | rational64s |
> 0x2001 | CMWhiteBalance | int16u |
> 0x2002 | CMWhiteBalanceComp | int16s |
> 0x2010 | CMWhiteBalanceGrayPoint | int16u[3] |
> 0x2020 | CMSaturation | int16s[3] |
> 0x2021 | CMHue | int16s[3] |
> 0x2022 | CMContrast | int16s[3] |
> 0x2023 | CMSharpness | int16s[3] |

## Olympus UnknownInfo Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Olympus MOV1 Tags

This information is found in MOV videos from Olympus models such as the D540Z, D595Z, FE100, FE110, FE115, FE170 and FE200.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N | --> Olympus CameraType Values
> 38 | ExposureUnknown? | N |
> 42 | FNumber | N |
> 50 | ExposureCompensation | N |
> 72 | FocalLength | N |

## Olympus MOV2 Tags

This information is found in MOV videos from Olympus models such as the FE120, FE140 and FE190.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N | (the actual model name, no decoding necessary)
> 54 | ExposureTime | N |
> 58 | FNumber | N |
> 66 | ExposureCompensation | N |
> 88 | FocalLength | N |
> 193 | ISO | N |

## Olympus MP4 Tags

This information is found in MP4 videos from Olympus models such as the u7040 and u9010.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |

> 24

> Model

> N

> (oddly different than CameraType values in JPEG images by the same camera)

> 'SG472' = u7040,S7040 'SG473' = u9010,S9010 'SG475' = SP800UZ 'SG551' = SZ-30MR 'SG553' = SP-610UZ |  | 'SG554' = SZ-10 'SG555' = SZ-20 'SG573' = SZ-14 'SG575' = SP-620UZ |

> 40 | FNumber | N |
> 48 | ExposureCompensation | N |
> 104 | MovableInfo | - | --> Olympus MovableInfo Tags
> 114 | MovableInfo | - | --> Olympus MovableInfo Tags

## Olympus MovableInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | ISO | N |
> 44 | EncoderVersion | N |
> 60 | DecoderVersion | N |
> 131 | Thumbnail | - | --> Olympus Thumbnail Tags

## Olympus Thumbnail Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | ThumbnailWidth | N |
> 2 | ThumbnailHeight | N |
> 3 | ThumbnailLength | N |
> 4 | ThumbnailOffset | N |

## Olympus MOV3 Tags

QuickTime information found in the TAGS atom of MOV videos from the E-M5.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'OLYM' | OlympusAtom | - | --> Olympus OLYM2 Tags

## Olympus OLYM2 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'prms' | MakerNotes | - | --> Olympus prms Tags
> 'scrn' | PreviewInfo | - | --> Olympus scrn2 Tags
> 'thmb' | ThumbInfo | - | --> Olympus thmb2 Tags

## Olympus prms Tags

Information extracted from the "prms" atom in MOV videos from Olympus models such as the OM E-M5.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 18 | Make | N |
> 44 | Model | N | --> Olympus CameraType Values
> 131 | DateTime1 | N |
> 157 | DateTime2 | N |

## Olympus scrn2 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | OlympusPreview | - | --> Olympus scrn Tags

## Olympus scrn Tags

Information extracted from the "scrn" atom of Olympus MP4 videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PreviewImageLength | N |
> 4 | PreviewImage | N | (640x480 JPEG preview image)

## Olympus thmb2 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ThumbnailWidth | N |
> 2 | ThumbnailHeight | N |
> 4 | ThumbnailLength | N |
> 8 | ThumbnailImage | N | (160x120 JPEG thumbnail image)

## Olympus thmb Tags

Information extracted from the "thmb" atom of Olympus MP4 videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ThumbnailLength | N |
> 4 | ThumbnailImage | N | (160x120 JPEG thumbnail image)

## Olympus OLYM Tags

Tags found in the OLYM atom of MP4 videos from the TG-810.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 14 | Make | N |
> 40 | Model | N | --> Olympus CameraType Values
> 90 | FNumber | N |
> 127 | DateTimeOriginal | N |
> 153 | DateTime2 | N |
> 265 | ThumbnailWidth | N |
> 267 | ThumbnailHeight | N |

## Olympus AVI Tags

This information is found in Olympus AVI videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 18 | Make | N |
> 44 | Model | N | --> Olympus CameraType Values
> 94 | FNumber | N |
> 131 | DateTime1 | N |
> 157 | DateTime2 | N |
> 297 | ThumbInfo | - | --> Olympus thmb2 Tags

## Olympus WAV Tags

This information is found in WAV files from Olympus PCM linear recorders like the LS-5, LS-10, LS-11.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | Model | N |
> 28 | FileNumber | N |
> 38 | DateTimeOriginal | N | (time at start of recording)
> 50 | DateTimeEnd | N | (time at end of recording)
> 62 | RecordingTime | N |
> 512 | Duration | N |
> 522 | Index01 | N |
> 532 | Index02 | N |
> 542 | Index03 | N |
> 552 | Index04 | N |
> 562 | Index05 | N |
> 572 | Index06 | N |
> 582 | Index07 | N |
> 592 | Index08 | N |
> 602 | Index09 | N |
> 612 | Index10 | N |
> 622 | Index11 | N |
> 632 | Index12 | N |
> 642 | Index13 | N |
> 652 | Index14 | N |
> 662 | Index15 | N |
> 672 | Index16 | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Apr 5, 2013

<-- ExifTool Tag Names