NikonCustom Tags

## NikonCustom SettingsD40 Tags

Custom settings for the Nikon D40.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | Beep | int8u | [Mask 0x80] 0x0 = On 0x80 = Off
> 0.2 | AFAssist | int8u | [Mask 0x40] 0x0 = On 0x40 = Off
> 0.3 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 0.4 | ImageReview | int8u | [Mask 0x10] 0x0 = On 0x10 = Off
> 1.1 | AutoISO | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 1.2 | AutoISOMax | int8u | [Mask 0x30] 0x10 = 400 0x20 = 800 0x30 = 1600

> 1.3

> AutoISOMinShutterSpeed

> int8u

> [Mask 0x07]

> 0x0 = 1/125 s 0x1 = 1/60 s 0x2 = 1/30 s 0x3 = 1/15 s |  | 0x4 = 1/8 s 0x5 = 1/4 s 0x6 = 1/2 s 0x7 = 1 s |

> 2.1

> ImageReviewTime

> int8u

> [Mask 0x07]
> 0x0 = 4 s
> 0x1 = 8 s
> 0x2 = 20 s
> 0x3 = 1 min
> 0x4 = 10 min

> 3.1

> MonitorOffTime

> int8u

> [Mask 0xe0]
> 0x0 = 4 s
> 0x20 = 8 s
> 0x40 = 20 s
> 0x60 = 1 min
> 0x80 = 10 min

> 3.2

> MeteringTime

> int8u

> [Mask 0x1c]
> 0x0 = 4 s
> 0x4 = 8 s
> 0x8 = 20 s
> 0xc = 1 min
> 0x10 = 30 min

> 3.3 | SelfTimerTime | int8u | [Mask 0x03] 0x0 = 2 s 0x1 = 5 s 0x2 = 10 s 0x3 = 20 s
> 3.4 | RemoteOnDuration | int8u | [Mask 0xc0] 0x0 = 1 min 0x40 = 5 min 0x80 = 10 min 0xc0 = 15 min

> 4.1

> AELockButton

> int8u

> [Mask 0x0e]
> 0x0 = AE/AF Lock
> 0x2 = AE Lock Only
> 0x4 = AF Lock Only
> 0x6 = AE Lock (hold)
> 0x8 = AF-ON

> 4.2 | AELock | int8u | [Mask 0x01] 0x0 = Off 0x1 = On

> 5.1

> ShootingModeSetting

> int8u

> [Mask 0x70]
> 0x0 = Single Frame
> 0x10 = Continuous
> 0x20 = Self-timer
> 0x30 = Delayed Remote
> 0x40 = Quick-response Remote

> 5.2

> TimerFunctionButton

> int8u

> [Mask 0x07]
> 0x0 = Shooting Mode
> 0x1 = Image Quality/Size
> 0x2 = ISO
> 0x3 = White Balance
> 0x4 = Self-timer

> 6.1 | Metering | int8u | [Mask 0x03] 0x0 = Matrix 0x1 = Center-weighted 0x2 = Spot
> 8.1 | InternalFlash | int8u | [Mask 0x10] 0x0 = TTL 0x10 = Manual
> 8.2 | ManualFlashOutput | int8u | [Mask 0x07]
> 9 | FlashLevel | int8s |
> 10.1 | FocusModeSetting | int8u | [Mask 0xc0] 0x0 = Manual 0x40 = AF-S 0x80 = AF-C 0xc0 = AF-A
> 11.1 | AFAreaModeSetting | int8u | [Mask 0x30] 0x0 = Single Area 0x10 = Dynamic Area 0x20 = Closest Subject

## NikonCustom SettingsD80 Tags

Custom settings for the Nikon D80.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | Beep | int8u | [Mask 0x80] 0x0 = On 0x80 = Off
> 0.2 | AFAssist | int8u | [Mask 0x40] 0x0 = On 0x40 = Off
> 0.3 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 0.4 | ImageReview | int8u | [Mask 0x10] 0x0 = On 0x10 = Off
> 0.5 | Illumination | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 0.6 | MainDialExposureComp | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 0.7 | EVStepSize | int8u | [Mask 0x01] 0x0 = 1/3 EV 0x1 = 1/2 EV
> 1.1 | AutoISO | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 1.2 | AutoISOMax | int8u | [Mask 0x30] 0x0 = 200 0x10 = 400 0x20 = 800 0x30 = 1600

> 1.3

> AutoISOMinShutterSpeed

> int8u

> [Mask 0x0f]

> 0x0 = 1/125 s
> 0x1 = 1/100 s
> 0x2 = 1/80 s
> 0x3 = 1/60 s
> 0x4 = 1/40 s
> 0x5 = 1/30 s

> 0x6 = 1/15 s
> 0x7 = 1/8 s
> 0x8 = 1/4 s
> 0x9 = 1/2 s
> 0xa = 1 s

> 2.1 | AutoBracketSet | int8u | [Mask 0xc0] 0x0 = AE & Flash 0x40 = AE Only 0x80 = Flash Only 0xc0 = WB Bracketing
> 2.2 | AutoBracketOrder | int8u | [Mask 0x20] 0x0 = 0,-,+ 0x20 = -,0,+

> 3.1

> MonitorOffTime

> int8u

> [Mask 0xe0]

> 0x0 = 5 s 0x20 = 10 s 0x40 = 20 s |  | 0x60 = 1 min 0x80 = 5 min 0xa0 = 10 min |

> 3.2

> MeteringTime

> int8u

> [Mask 0x1c]

> 0x0 = 4 s 0x4 = 6 s 0x8 = 8 s |  | 0xc = 16 s 0x10 = 30 s 0x14 = 30 min |

> 3.3 | SelfTimerTime | int8u | [Mask 0x03] 0x0 = 2 s 0x1 = 5 s 0x2 = 10 s 0x3 = 20 s

> 4.1

> AELockButton

> int8u

> [Mask 0x1e]

> 0x0 = AE/AF Lock
> 0x2 = AE Lock Only
> 0x4 = AF Lock Only
> 0x6 = AE Lock (hold)
> 0x8 = AF-ON
> 0xa = FV Lock
> 0xc = Focus Area Selection
> 0xe = AE-L/AF-L/AF Area
> 0x10 = AE-L/AF Area
> 0x12 = AF-L/AF Area
> 0x14 = AF-ON/AF Area

> 4.2 | AELock | int8u | [Mask 0x01] 0x0 = Off 0x1 = On
> 4.3 | RemoteOnDuration | int8u | [Mask 0xc0] 0x0 = 1 min 0x40 = 5 min 0x80 = 10 min 0xc0 = 15 min
> 5.1 | CommandDials | int8u | [Mask 0x80] 0x0 = Standard (Main Shutter, Sub Aperture) 0x80 = Reversed (Main Aperture, Sub Shutter)

> 5.2

> FunctionButton

> int8u

> [Mask 0x78]

> 0x0 = ISO Display 0x8 = Framing Grid 0x10 = AF-area Mode 0x18 = Center AF Area 0x20 = FV Lock |  | 0x28 = Flash Off 0x30 = Matrix Metering 0x38 = Center-weighted 0x40 = Spot Metering |

> 6.1 | GridDisplay | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 6.2 | ViewfinderWarning | int8u | [Mask 0x40] 0x0 = On 0x40 = Off
> 6.3 | CenterWeightedAreaSize | int8u | [Mask 0x0c] 0x0 = 6 mm 0x4 = 8 mm 0x8 = 10 mm
> 6.4 | ExposureDelayMode | int8u | [Mask 0x20] 0x0 = Off 0x20 = On
> 6.5 | MB-D80Batteries | int8u | [Mask 0x03] 0x0 = LR6 (AA Alkaline) 0x1 = HR6 (AA Ni-MH) 0x2 = FR6 (AA Lithium) 0x3 = ZR6 (AA Ni-Mg)
> 7.1 | FlashWarning | int8u | [Mask 0x80] 0x0 = On 0x80 = Off
> 7.2 | FlashShutterSpeed | int8u | [Mask 0x78]
> 7.3 | AutoFP | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 7.4 | ModelingFlash | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 8.1 | InternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Repeating Flash 0xc0 = Commander Mode
> 8.2 | ManualFlashOutput | int8u | [Mask 0x07]
> 9.1 | RepeatingFlashOutput | int8u | [Mask 0x70]
> 9.2 | RepeatingFlashCount | int8u | [Mask 0x0f]
> 10.1 | RepeatingFlashRate | int8u | [Mask 0xf0]
> 10.2 | CommanderChannel | int8u | [Mask 0x03]
> 11.1 | CommanderInternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Off
> 11.2 | CommanderGroupAMode | int8u | [Mask 0x30] 0x0 = TTL 0x10 = Auto Aperture 0x20 = Manual 0x30 = Off
> 11.3 | CommanderGroupBMode | int8u | [Mask 0x0c] 0x0 = TTL 0x4 = Auto Aperture 0x8 = Manual 0xc = Off
> 12.1 | CommanderInternalTTLComp | int8u | [Mask 0x1f]
> 12.2 | CommanderInternalManualOutput | int8u | [Mask 0xe0]
> 13.1 | CommanderGroupA_TTL-AAComp | int8u | [Mask 0x1f]
> 13.2 | CommanderGroupAManualOutput | int8u | [Mask 0xe0]
> 14.1 | CommanderGroupB_TTL-AAComp | int8u | [Mask 0x1f]
> 14.2 | CommanderGroupBManualOutput | int8u | [Mask 0xe0]
> 15.1 | CenterAFArea | int8u | [Mask 0x80] 0x0 = Normal Zone 0x80 = Wide Zone
> 15.2 | FocusAreaSelection | int8u | [Mask 0x04] 0x0 = No Wrap 0x4 = Wrap
> 15.3 | AFAreaIllumination | int8u | [Mask 0x03] 0x0 = Auto 0x1 = Off 0x2 = On
> 16.1 | AFAreaModeSetting | int8u | [Mask 0xc0] 0x0 = Single Area 0x40 = Dynamic Area 0x80 = Auto-area

## NikonCustom SettingsD90 Tags

Custom settings for the D90.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | LightSwitch | int8u | [Mask 0x08] 0x0 = LCD Backlight 0x8 = LCD Backlight and Shooting Information
> 2.1 | AFAreaModeSetting | int8u | [Mask 0x60] 0x0 = Single Area 0x20 = Dynamic Area 0x40 = Auto-area 0x60 = 3D-tracking (11 points)
> 2.2 | CenterFocusPoint | int8u | [Mask 0x10] 0x0 = Normal Zone 0x10 = Wide Zone
> 2.3 | AFAssist | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 2.4 | AFPointIllumination | int8u | [Mask 0x06] 0x0 = Auto 0x2 = On 0x4 = Off
> 2.5 | FocusPointWrap | int8u | [Mask 0x08] 0x0 = No Wrap 0x8 = Wrap

> 3.1

> AELockForMB-D80

> int8u

> [Mask 0x1c]

> 0x0 = AE Lock Only
> 0x4 = AF Lock Only
> 0x8 = AE Lock (hold)
> 0xc = AF-On
> 0x10 = FV Lock
> 0x14 = Focus Point Selection
> 0x1c = AE/AF Lock

> 3.2 | MB-D80BatteryType | int8u | [Mask 0x03] 0x0 = LR6 (AA alkaline) 0x1 = HR6 (AA Ni-MH) 0x2 = FR6 (AA lithium) 0x3 = ZR6 (AA Ni-Mn)
> 4.1 | Beep | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 4.2 | GridDisplay | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 4.3 | ISODisplay | int8u | [Mask 0x0c] 0x0 = Show ISO/Easy ISO 0x4 = Show ISO Sensitivity 0xc = Show Frame Count
> 4.4 | ViewfinderWarning | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 4.5 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 5.1 | ScreenTips | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 5.2 | FileNumberSequence | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 5.3 | ShootingInfoDisplay | int8u | [Mask 0xc0] 0x0 = Auto 0x80 = Manual (dark on light) 0xc0 = Manual (light on dark)
> 5.4 | LCDIllumination | int8u | [Mask 0x20] 0x0 = Off 0x20 = On
> 6.1 | EasyExposureComp | int8u | [Mask 0x01] 0x0 = Off 0x1 = On
> 6.2 | ReverseIndicators | int8u | [Mask 0x80] 0x0 = + 0 - 0x80 = - 0 +
> 7.1 | ExposureControlStepSize | int8u | [Mask 0x40] 0x0 = 1/3 EV 0x40 = 1/2 EV
> 8.1 | CenterWeightedAreaSize | int8u | [Mask 0x60] 0x0 = 6 mm 0x20 = 8 mm 0x40 = 10 mm
> 8.2 | FineTuneOptMatrixMetering | int8u | [Mask 0x0f]
> 9.1 | FineTuneOptCenterWeighted | int8u | [Mask 0xf0]
> 9.2 | FineTuneOptSpotMetering | int8u | [Mask 0x0f]
> 11.1 | CLModeShootingSpeed | int8u | [Mask 0x07]
> 11.2 | ExposureDelayMode | int8u | [Mask 0x40] 0x0 = Off 0x40 = On

> 13.1

> AutoBracketSet

> int8u

> [Mask 0xe0]
> 0x0 = AE & Flash
> 0x20 = AE Only
> 0x40 = Flash Only
> 0x60 = WB Bracketing
> 0x80 = Active D-Lighting

> 13.2 | AutoBracketOrder | int8u | [Mask 0x10] 0x0 = 0,-,+ 0x10 = -,0,+

> 14.1

> FuncButton

> int8u

> [Mask 0x78]

> 0x8 = Framing Grid
> 0x10 = AF-area Mode
> 0x18 = Center Focus Point
> 0x20 = FV Lock
> 0x28 = Flash Off
> 0x30 = Matrix Metering
> 0x38 = Center-weighted Metering
> 0x40 = Spot Metering
> 0x48 = My Menu Top
> 0x50 = + NEF (RAW)

> 16.1 | OKButton | int8u | [Mask 0x18] 0x0 = Not Used 0x8 = Select Center Focus Point 0x10 = Highlight Active Focus Point 0x18 = Not Used

> 17.1

> AELockButton

> int8u

> [Mask 0x38]

> 0x0 = AE/AF Lock 0x8 = AE Lock Only 0x10 = AF Lock Only |  | 0x18 = AE Lock (hold) 0x20 = AF-ON 0x28 = FV Lock |

> 18.1 | CommandDialsReverseRotation | int8u | [Mask 0x80] 0x0 = No 0x80 = Yes
> 18.2 | ShutterReleaseButtonAE-L | int8u | [Mask 0x02] 0x0 = Off 0x2 = On

> 19.1

> MeteringTime

> int8u

> [Mask 0xf0]

> 0x0 = 4 s 0x10 = 6 s 0x20 = 8 s 0x30 = 16 s 0x40 = 30 s |  | 0x50 = 1 min 0x60 = 5 min 0x70 = 10 min 0x80 = 30 min |

> 19.2 | RemoteOnDuration | int8u | [Mask 0x03] 0x0 = 1 min 0x1 = 5 min 0x2 = 10 min 0x3 = 15 min
> 20.1 | SelfTimerTime | int8u | [Mask 0xc0] 0x0 = 2 s 0x40 = 5 s 0x80 = 10 s 0xc0 = 20 s
> 20.2 | SelfTimerShotCount | int8u | [Mask 0x1e]

> 21.1

> PlaybackMonitorOffTime

> int8u

> [Mask 0x1c]

> 0x0 = 4 s 0x4 = 10 s 0x8 = 20 s |  | 0xc = 1 min 0x10 = 5 min 0x14 = 10 min |

> 21.2

> ImageReviewTime

> int8u

> [Mask 0xe0]

> 0x0 = 4 s 0x20 = 10 s 0x40 = 20 s |  | 0x60 = 1 min 0x80 = 5 min 0xa0 = 10 min |

> 22.1

> MenuMonitorOffTime

> int8u

> [Mask 0xe0]

> 0x0 = 4 s 0x20 = 10 s 0x40 = 20 s |  | 0x60 = 1 min 0x80 = 5 min 0xa0 = 10 min |

> 22.2

> ShootingInfoMonitorOffTime

> int8u

> [Mask 0x1c]

> 0x0 = 4 s 0x4 = 10 s 0x8 = 20 s |  | 0xc = 1 min 0x10 = 5 min 0x14 = 10 min |

> 23.1

> FlashShutterSpeed

> int8u

> [Mask 0x0f]

> 0x0 = 1/60 s
> 0x1 = 1/30 s
> 0x2 = 1/15 s
> 0x3 = 1/8 s
> 0x4 = 1/4 s
> 0x5 = 1/2 s

> 0x6 = 1 s
> 0x7 = 2 s
> 0x8 = 4 s
> 0x9 = 8 s
> 0xa = 15 s
> 0xb = 30 s

> 24.1 | InternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Repeating Flash 0xc0 = Commander Mode
> 24.2 | ManualFlashOutput | int8u | [Mask 0x1f]
> 25.1 | RepeatingFlashOutput | int8u | [Mask 0x70]
> 25.2 | RepeatingFlashCount | int8u | [Mask 0x0f]
> 26.1 | RepeatingFlashRate | int8u | [Mask 0xf0]
> 31.1 | FlashWarning | int8u | [Mask 0x80] 0x0 = On 0x80 = Off
> 31.2 | CommanderInternalTTLComp | int8u | [Mask 0x1f]
> 31.3 | ModelingFlash | int8u | [Mask 0x20] 0x0 = On 0x20 = Off
> 31.4 | AutoFP | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 32.1 | CommanderGroupA_TTLComp | int8u | [Mask 0x1f]
> 33.1 | CommanderGroupB_TTLComp | int8u | [Mask 0x1f]
> 34.1 | LiveViewAF | int8u | [Mask 0xc0] 0x0 = Face Priority 0x40 = Wide Area 0x80 = Normal Area

## NikonCustom SettingsD3 Tags

Custom settings for the D3, D3S, D3X, D300 and D300S.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [Mask 0x03] 0x0 = A 0x1 = B 0x2 = C 0x3 = D
> 0.2 | CustomSettingsAllDefault | int8u | ("No" if any custom setting for this bank was changed from the default) [Mask 0x80] 0x0 = Yes 0x80 = No
> 1.1 | AF-CPrioritySelection | int8u | [Mask 0xc0] 0x0 = Release 0x40 = Release + Focus 0x80 = Focus
> 1.2 | AF-SPrioritySelection | int8u | [Mask 0x20] 0x0 = Focus 0x20 = Release
> 1.3 | AFPointSelection | int8u | [Mask 0x10] 0x0 = 51 Points 0x10 = 11 Points
> 1.4 | DynamicAFArea | int8u | [Mask 0x0c] 0x0 = 9 Points 0x4 = 21 Points 0x8 = 51 Points 0xc = 51 Points (3D-tracking)

> 1.5

> FocusTrackingLockOn

> int8u

> (not D3S)
> [Mask 0x03]
> 0x0 = Long
> 0x1 = Normal
> 0x2 = Short
> 0x3 = Off

> 2.1 | AFActivation | int8u | [Mask 0x80] 0x0 = Shutter/AF-On 0x80 = AF-On Only
> 2.2 | FocusPointWrap | int8u | [Mask 0x08] 0x0 = No Wrap 0x8 = Wrap

> 2.3

> AFPointIllumination

> int8u

> (D3)
> [Mask 0x60]
> 0x0 = On in Continuous Shooting and Manual Focusing
> 0x20 = On During Manual Focusing
> 0x40 = On in Continuous Shooting Modes
> 0x60 = Off
> (D300)
> [Mask 0x06]
> 0x0 = Auto
> 0x2 = Off
> 0x4 = On

> 2.4

> AFPointBrightness

> int8u

> (D3 only)
> [Mask 0x06]
> 0x0 = Low
> 0x2 = Normal
> 0x4 = High
> 0x6 = Extra High

> 2.5 | AFAssist | int8u | (D300 only) [Mask 0x01] 0x0 = On 0x1 = Off

> 3.1

> AFOnButton

> int8u

> (D3 only)
> [Mask 0x07]

> 0x0 = AF On
> 0x1 = AE/AF Lock
> 0x2 = AE Lock Only
> 0x3 = AE Lock (reset on release)
> 0x4 = AE Lock (hold)
> 0x5 = AF Lock Only

> 3.2

> VerticalAFOnButton

> int8u

> (D3 only)
> [Mask 0x70]

> 0x0 = AF On
> 0x10 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x30 = AE Lock (reset on release)
> 0x40 = AE Lock (hold)
> 0x50 = AF Lock Only
> 0x70 = Same as AF On

> 3.3

> AF-OnForMB-D10

> int8u

> (D300 only)
> [Mask 0x70]

> 0x0 = AF-On
> 0x10 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x30 = AE Lock (reset on release)
> 0x40 = AE Lock (hold)
> 0x50 = AF Lock Only
> 0x60 = Same as FUNC Button

> 4.1

> FocusTrackingLockOn

> int8u

> (D3S only)
> [Mask 0x07]

> 0x0 = 5 (Long) 0x1 = 4 0x2 = 3 (Normal) |  | 0x3 = 2 0x4 = 1 (Short) 0x5 = Off |

> 4.2 | AssignBktButton | int8u | (D3S only) [Mask 0x08] 0x0 = Auto Bracketing 0x8 = Multiple Exposure

> 4.3

> MultiSelectorLiveView

> int8u

> (D3S only)
> [Mask 0xc0]
> 0x0 = Reset
> 0x40 = Zoom On/Off
> 0x80 = Start Movie Recording
> 0xc0 = Not Used

> 4.4 | InitialZoomLiveView | int8u | (D3S only) [Mask 0x30] 0x0 = Low Magnification 0x10 = Medium Magnification 0x20 = High Magnification
> 6.1 | ISOStepSize | int8u | [Mask 0xc0] 0x0 = 1/3 EV 0x40 = 1/2 EV 0x80 = 1 EV
> 6.2 | ExposureControlStepSize | int8u | [Mask 0x30] 0x0 = 1/3 EV 0x10 = 1/2 EV 0x20 = 1 EV
> 6.3 | ExposureCompStepSize | int8u | [Mask 0x0c] 0x0 = 1/3 EV 0x4 = 1/2 EV 0x8 = 1 EV
> 6.4 | EasyExposureCompensation | int8u | [Mask 0x03] 0x0 = Off 0x1 = On 0x2 = On (auto reset)

> 7.1

> CenterWeightedAreaSize

> int8u

> (D3)
> [Mask 0xe0]
> 0x0 = 8 mm
> 0x20 = 12 mm
> 0x40 = 15 mm
> 0x60 = 20 mm
> 0x80 = Average
> (D300)
> [Mask 0xe0]
> 0x0 = 6 mm
> 0x20 = 8 mm
> 0x40 = 10 mm
> 0x60 = 13 mm
> 0x80 = Average

> 7.2 | FineTuneOptCenterWeighted | int8u | [Mask 0x0f]
> 8.1 | FineTuneOptMatrixMetering | int8u | [Mask 0xf0]
> 8.2 | FineTuneOptSpotMetering | int8u | [Mask 0x0f]
> 9.1 | MultiSelectorShootMode | int8u | [Mask 0xc0] 0x0 = Select Center Focus Point 0x40 = Highlight Active Focus Point 0x80 = Not Used

> 9.2

> MultiSelectorPlaybackMode

> int8u

> (all models except D3S)
> [Mask 0x30]
> 0x0 = Thumbnail On/Off
> 0x10 = View Histograms
> 0x20 = Zoom On/Off
> 0x30 = Choose Folder

> 9.3

> InitialZoomSetting

> int8u

> (D3)
> [Mask 0x0c]
> 0x0 = High Magnification
> 0x4 = Medium Magnification
> 0x8 = Low Magnification
> (D300)
> [Mask 0x0c]
> 0x0 = Low Magnification
> 0x4 = Medium Magnification
> 0x8 = High Magnification

> 9.4 | MultiSelector | int8u | [Mask 0x01] 0x0 = Do Nothing 0x1 = Reset Meter-off Delay
> 10.1 | ExposureDelayMode | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 10.2 | CLModeShootingSpeed | int8u | [Mask 0x07]
> 10.3 | CHModeShootingSpeed | int8u | (D3 only) [Mask 0x30] 0x0 = 9 fps 0x10 = 10 fps 0x20 = 11 fps
> 11 | MaxContinuousRelease | int8u |
> 12.1 | ReverseIndicators | int8u | [Mask 0x20] 0x0 = + 0 - 0x20 = - 0 +

> 12.2

> FileNumberSequence

> int8u

> (D3)
> [Mask 0x02]
> 0x0 = On
> 0x2 = Off
> (D300)
> [Mask 0x08]
> 0x0 = On
> 0x8 = Off

> 12.3 | RearDisplay | int8u | (D3 only) [Mask 0x80] 0x0 = ISO 0x80 = Exposures Remaining
> 12.4 | ViewfinderDisplay | int8u | (D3 only) [Mask 0x40] 0x0 = Frame Count 0x40 = Exposures Remaining
> 12.5 | BatteryOrder | int8u | (D300 only) [Mask 0x04] 0x0 = MB-D10 First 0x4 = Camera Battery First

> 12.6

> MB-D10Batteries

> int8u

> (D300 only)
> [Mask 0x03]
> 0x0 = LR6 (AA alkaline)
> 0x1 = HR6 (AA Ni-MH)
> 0x2 = FR6 (AA lithium)
> 0x3 = ZR6 (AA Ni-Mn)

> 12.7 | ScreenTips | int8u | [Mask 0x10] 0x0 = On 0x10 = Off
> 13.1 | Beep | int8u | [Mask 0xc0] 0x0 = High 0x40 = Low 0x80 = Off
> 13.2 | ShootingInfoDisplay | int8u | [Mask 0x30] 0x0 = Auto 0x10 = Auto 0x20 = Manual (dark on light) 0x30 = Manual (light on dark)
> 13.3 | GridDisplay | int8u | (D300 only) [Mask 0x02] 0x0 = Off 0x2 = On
> 13.4 | ViewfinderWarning | int8u | (D300 only) [Mask 0x01] 0x0 = On 0x1 = Off
> 13.5 | MultiSelectorPlaybackMode | int8u | (D3S only) [Mask 0x03] 0x0 = Thumbnail On/Off 0x1 = View Histograms 0x2 = Zoom On/Off

> 14.1

> PreviewButton
> FuncButton

> int8u
> int8u

> (D3)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x40 = Flash Off
> 0x48 = Bracketing Burst
> 0x50 = Matrix Metering
> 0x58 = Center-weighted Metering
> 0x60 = Spot Metering
> 0x68 = Virtual Horizon
> 0x78 = Playback
> 0x80 = My Menu Top

> (D300)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x48 = Flash Off
> 0x50 = Bracketing Burst
> 0x58 = Matrix Metering
> 0x60 = Center-weighted Metering
> 0x68 = Spot Metering
> 0x70 = Playback
> 0x78 = My Menu Top
> 0x80 = + NEF (RAW)

> 14.2

> PreviewButtonPlusDials
> FuncButtonPlusDials

> int8u
> int8u

> (D3)
> [Mask 0x07]

> 0x0 = None
> 0x1 = Choose Image Area (FX/DX/5:4)
> 0x2 = One Step Speed/Aperture
> 0x3 = Choose Non-CPU Lens Number
> 0x5 = Choose Image Area (FX/DX)
> 0x6 = Shooting Bank Menu
> 0x7 = Dynamic AF Area

> (D300)
> [Mask 0x07]
> 0x0 = None
> 0x2 = One Step Speed/Aperture
> 0x3 = Choose Non-CPU Lens Number
> 0x5 = Auto Bracketing
> 0x6 = Dynamic AF Area

> 15.1

> FuncButton
> PreviewButton

> int8u
> int8u

> (D3)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x40 = Flash Off
> 0x48 = Bracketing Burst
> 0x50 = Matrix Metering
> 0x58 = Center-weighted Metering
> 0x60 = Spot Metering
> 0x68 = Virtual Horizon
> 0x78 = Playback
> 0x80 = My Menu Top

> (D300)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x48 = Flash Off
> 0x50 = Bracketing Burst
> 0x58 = Matrix Metering
> 0x60 = Center-weighted Metering
> 0x68 = Spot Metering
> 0x70 = Playback
> 0x78 = My Menu Top
> 0x80 = + NEF (RAW)

> 15.2

> FuncButtonPlusDials
> PreviewButtonPlusDials

> int8u
> int8u

> (D3)
> [Mask 0x07]

> 0x0 = None
> 0x1 = Choose Image Area (FX/DX/5:4)
> 0x2 = One Step Speed/Aperture
> 0x3 = Choose Non-CPU Lens Number
> 0x4 = Focus Point Selection
> 0x5 = Choose Image Area (FX/DX)
> 0x6 = Shooting Bank Menu
> 0x7 = Dynamic AF Area

> (D300)
> [Mask 0x07]
> 0x0 = None
> 0x2 = One Step Speed/Aperture
> 0x3 = Choose Non-CPU Lens Number
> 0x5 = Auto Bracketing
> 0x6 = Dynamic AF Area

> 16.1

> AELockButton

> int8u

> (D3)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x40 = Flash Off
> 0x48 = Bracketing Burst
> 0x50 = Matrix Metering
> 0x58 = Center-weighted Metering
> 0x60 = Spot Metering
> 0x68 = Virtual Horizon
> 0x70 = AF On
> 0x78 = Playback
> 0x80 = My Menu Top

> (D300)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x40 = AF On
> 0x48 = Flash Off
> 0x50 = Bracketing Burst
> 0x58 = Matrix Metering
> 0x60 = Center-weighted Metering
> 0x68 = Spot Metering
> 0x70 = Playback
> 0x78 = My Menu Top
> 0x80 = + NEF (RAW)

> 16.2

> AELockButtonPlusDials

> int8u

> (D3)
> [Mask 0x07]

> 0x0 = None
> 0x1 = Choose Image Area (FX/DX/5:4)
> 0x2 = One Step Speed/Aperture
> 0x3 = Choose Non-CPU Lens Number
> 0x5 = Choose Image Area (FX/DX)
> 0x6 = Shooting Bank Menu
> 0x7 = Dynamic AF Area

> (D300)
> [Mask 0x07]
> 0x0 = None
> 0x3 = Choose Non-CPU Lens Number
> 0x5 = Auto Bracketing
> 0x6 = Dynamic AF Area

> 17.1 | CommandDialsReverseRotation | int8u | [Mask 0x80] 0x0 = No 0x80 = Yes
> 17.2 | CommandDialsChangeMainSub | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 17.3 | CommandDialsApertureSetting | int8u | [Mask 0x20] 0x0 = Sub-command Dial 0x20 = Aperture Ring
> 17.4 | CommandDialsMenuAndPlayback | int8u | [Mask 0x10] 0x0 = Off 0x10 = On
> 17.5 | LCDIllumination | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 17.6 | PhotoInfoPlayback | int8u | [Mask 0x04] 0x0 = Info Up-down, Playback Left-right 0x4 = Info Left-right, Playback Up-down
> 17.7 | ShutterReleaseButtonAE-L | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 17.8 | ReleaseButtonToUseDial | int8u | [Mask 0x01] 0x0 = No 0x1 = Yes
> 18.1 | SelfTimerTime | int8u | [Mask 0x18] 0x0 = 2 s 0x8 = 5 s 0x10 = 10 s 0x18 = 20 s

> 18.2

> MonitorOffTime

> int8u

> [Mask 0x07]
> 0x0 = 10 s
> 0x1 = 20 s
> 0x2 = 1 min
> 0x3 = 5 min
> 0x4 = 10 min

> 20.1

> FlashSyncSpeed

> int8u

> (D3)
> [Mask 0xe0]

> 0x0 = 1/250 s (auto FP) 0x20 = 1/250 s 0x40 = 1/200 s 0x60 = 1/160 s |  | 0x80 = 1/125 s 0xa0 = 1/100 s 0xc0 = 1/80 s 0xe0 = 1/60 s |

> (D300)
> [Mask 0xf0]

> 0x0 = 1/320 s (auto FP)
> 0x10 = 1/250 s (auto FP)
> 0x20 = 1/250 s
> 0x30 = 1/200 s
> 0x40 = 1/160 s
> 0x50 = 1/125 s
> 0x60 = 1/100 s
> 0x70 = 1/80 s
> 0x80 = 1/60 s

> 20.2

> FlashShutterSpeed

> int8u

> [Mask 0x0f]

> 0x0 = 1/60 s
> 0x1 = 1/30 s
> 0x2 = 1/15 s
> 0x3 = 1/8 s
> 0x4 = 1/4 s
> 0x5 = 1/2 s

> 0x6 = 1 s
> 0x7 = 2 s
> 0x8 = 4 s
> 0x9 = 8 s
> 0xa = 15 s
> 0xb = 30 s

> 21.1 | AutoBracketSet | int8u | [Mask 0xc0] 0x0 = AE & Flash 0x40 = AE Only 0x80 = Flash Only 0xc0 = WB Bracketing
> 21.2 | AutoBracketModeM | int8u | [Mask 0x30] 0x0 = Flash/Speed 0x10 = Flash/Speed/Aperture 0x20 = Flash/Aperture 0x30 = Flash Only
> 21.3 | AutoBracketOrder | int8u | [Mask 0x08] 0x0 = 0,-,+ 0x8 = -,0,+
> 21.4 | ModelingFlash | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 22.1 | NoMemoryCard | int8u | [Mask 0x80] 0x0 = Release Locked 0x80 = Enable Release

> 22.2

> MeteringTime

> int8u

> [Mask 0x0f]

> 0x0 = 4 s 0x1 = 6 s 0x2 = 8 s 0x3 = 16 s 0x4 = 30 s |  | 0x5 = 1 min 0x6 = 5 min 0x7 = 10 min 0x8 = 30 min 0x9 = No Limit |

> 23.1 | InternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Repeating Flash 0xc0 = Commander Mode

## NikonCustom SettingsD700 Tags

Custom settings for the D700.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [Mask 0x03] 0x0 = A 0x1 = B 0x2 = C 0x3 = D
> 0.2 | CustomSettingsAllDefault | int8u | ("No" if any custom setting for this bank was changed from the default) [Mask 0x80] 0x0 = Yes 0x80 = No
> 1.1 | AF-CPrioritySelection | int8u | [Mask 0xc0] 0x0 = Release 0x40 = Release + Focus 0x80 = Focus
> 1.2 | AF-SPrioritySelection | int8u | [Mask 0x20] 0x0 = Focus 0x20 = Release
> 1.3 | AFPointSelection | int8u | [Mask 0x10] 0x0 = 51 Points 0x10 = 11 Points
> 1.4 | DynamicAFArea | int8u | [Mask 0x0c] 0x0 = 9 Points 0x4 = 21 Points 0x8 = 51 Points 0xc = 51 Points (3D-tracking)
> 2.1 | AFActivation | int8u | [Mask 0x80] 0x0 = Shutter/AF-On 0x80 = AF-On Only
> 2.2 | FocusPointWrap | int8u | [Mask 0x08] 0x0 = No Wrap 0x8 = Wrap
> 2.3 | AFPointIllumination | int8u | [Mask 0x06] 0x0 = Auto 0x2 = Off 0x4 = On
> 2.4 | AFAssist | int8u | [Mask 0x01] 0x0 = On 0x1 = Off

> 3.1

> FocusTrackingLockOn

> int8u

> [Mask 0x07]

> 0x0 = 3 Normal 0x1 = 4 0x2 = 5 Long |  | 0x3 = 2 0x4 = 1 Short 0x5 = Off |

> 3.2

> AF-OnForMB-D10

> int8u

> [Mask 0x70]

> 0x0 = AF-On
> 0x10 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x30 = AE Lock (reset on release)
> 0x40 = AE Lock (hold)
> 0x50 = AF Lock Only
> 0x60 = Same as FUNC Button

> 4.1 | ISOStepSize | int8u | [Mask 0xc0] 0x0 = 1/3 EV 0x40 = 1/2 EV 0x80 = 1 EV
> 4.2 | ExposureControlStepSize | int8u | [Mask 0x30] 0x0 = 1/3 EV 0x10 = 1/2 EV 0x20 = 1 EV
> 4.3 | ExposureCompStepSize | int8u | [Mask 0x0c] 0x0 = 1/3 EV 0x4 = 1/2 EV 0x8 = 1 EV
> 4.4 | EasyExposureCompensation | int8u | [Mask 0x03] 0x0 = Off 0x1 = On 0x2 = On (auto reset)

> 5.1

> CenterWeightedAreaSize

> int8u

> [Mask 0x70]
> 0x0 = 8 mm
> 0x10 = 12 mm
> 0x20 = 15 mm
> 0x30 = 20 mm
> 0x40 = Average

> 6.1 | FineTuneOptMatrixMetering | int8u | [Mask 0xf0]
> 6.2 | FineTuneOptSpotMetering | int8u | [Mask 0x0f]
> 7.1 | ShutterReleaseButtonAE-L | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 7.2 | SelfTimerTime | int8u | [Mask 0x30] 0x0 = 2 s 0x10 = 5 s 0x20 = 10 s 0x30 = 20 s

> 7.3

> MeteringTime

> int8u

> [Mask 0x0f]

> 0x0 = 4 s 0x1 = 6 s 0x2 = 8 s 0x3 = 16 s 0x4 = 30 s |  | 0x5 = 1 min 0x6 = 5 min 0x7 = 10 min 0x8 = 30 min 0x9 = No Limit |

> 8.1

> PlaybackMonitorOffTime

> int8u

> [Mask 0x38]

> 0x0 = 4 s 0x8 = 10 s 0x10 = 20 s |  | 0x18 = 1 min 0x20 = 5 min 0x28 = 10 min |

> 8.2

> MenuMonitorOffTime

> int8u

> [Mask 0x07]

> 0x0 = 4 s 0x1 = 10 s 0x2 = 20 s |  | 0x3 = 1 min 0x4 = 5 min 0x5 = 10 min |

> 9.1

> ShootingInfoMonitorOffTime

> int8u

> [Mask 0x38]

> 0x0 = 4 s 0x8 = 10 s 0x10 = 20 s |  | 0x18 = 1 min 0x20 = 5 min 0x28 = 10 min |

> 9.2

> ImageReviewTime

> int8u

> [Mask 0x07]

> 0x0 = 4 s 0x1 = 10 s 0x2 = 20 s |  | 0x3 = 1 min 0x4 = 5 min 0x5 = 10 min |

> 10.1 | Beep | int8u | [Mask 0xc0] 0x0 = High 0x40 = Low 0x80 = Off
> 10.2 | ShootingInfoDisplay | int8u | [Mask 0x30] 0x0 = Auto 0x10 = Auto 0x20 = Manual (dark on light) 0x30 = Manual (light on dark)
> 10.3 | LCDIllumination | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 10.4 | ExposureDelayMode | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 10.5 | GridDisplay | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 11.1 | FileNumberSequence | int8u | [Mask 0x40] 0x0 = On 0x40 = Off
> 11.2 | CLModeShootingSpeed | int8u | [Mask 0x07]
> 12 | MaxContinuousRelease | int8u |
> 13.1 | ScreenTips | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 13.2 | BatteryOrder | int8u | [Mask 0x04] 0x0 = MB-D10 First 0x4 = Camera Battery First
> 13.3 | MB-D10BatteryType | int8u | [Mask 0x03] 0x0 = LR6 (AA alkaline) 0x1 = HR6 (AA Ni-MH) 0x2 = FR6 (AA lithium) 0x3 = ZR6 (AA Ni-Mn)

> 15.1

> FlashSyncSpeed

> int8u

> [Mask 0xf0]

> 0x0 = 1/320 s (auto FP)
> 0x10 = 1/250 s (auto FP)
> 0x20 = 1/250 s
> 0x30 = 1/200 s
> 0x40 = 1/160 s
> 0x50 = 1/125 s
> 0x60 = 1/100 s
> 0x70 = 1/80 s
> 0x80 = 1/60 s

> 15.2

> FlashShutterSpeed

> int8u

> [Mask 0x0f]

> 0x0 = 1/60 s
> 0x1 = 1/30 s
> 0x2 = 1/15 s
> 0x3 = 1/8 s
> 0x4 = 1/4 s
> 0x5 = 1/2 s

> 0x6 = 1 s
> 0x7 = 2 s
> 0x8 = 4 s
> 0x9 = 8 s
> 0xa = 15 s
> 0xb = 30 s

> 16.1 | FlashControlBuilt-in | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Repeating Flash 0xc0 = Commander Mode
> 16.2 | ManualFlashOutput | int8u | [Mask 0x1f]
> 17.1 | RepeatingFlashOutput | int8u | [Mask 0x70]
> 17.2 | RepeatingFlashCount | int8u | [Mask 0x0f]
> 18.1 | RepeatingFlashRate | int8u | [Mask 0xf0]
> 18.2 | CommanderInternalTTLChannel | int8u | [Mask 0x03] 0x0 = 1 ch 0x1 = 2 ch 0x2 = 3 ch 0x3 = 4 ch
> 20.1 | CommanderInternalTTLCompBuiltin | int8u | [Mask 0x1f]
> 21.1 | CommanderInternalTTLCompGroupA | int8u | [Mask 0x1f]
> 22.1 | CommanderInternalTTLCompGroupB | int8u | [Mask 0x1f]
> 26.1 | AutoBracketSet | int8u | [Mask 0xc0] 0x0 = AE & Flash 0x40 = AE Only 0x80 = Flash Only 0xc0 = WB Bracketing
> 26.2 | AutoBracketModeM | int8u | [Mask 0x30] 0x0 = Flash/Speed 0x10 = Flash/Speed/Aperture 0x20 = Flash/Aperture 0x30 = Flash Only
> 26.3 | AutoBracketOrder | int8u | [Mask 0x08] 0x0 = 0,-,+ 0x8 = -,0,+
> 26.4 | ModelingFlash | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 27.1 | MultiSelectorShootMode | int8u | [Mask 0xc0] 0x0 = Select Center Focus Point 0x40 = Highlight Active Focus Point 0x80 = Not Used
> 27.2 | MultiSelectorPlaybackMode | int8u | [Mask 0x30] 0x0 = Thumbnail On/Off 0x10 = View Histograms 0x20 = Zoom On/Off 0x30 = Choose Folder
> 27.3 | InitialZoomSetting | int8u | [Mask 0x0c] 0x0 = Low Magnification 0x4 = Medium Magnification 0x8 = High Magnification
> 27.4 | MultiSelector | int8u | [Mask 0x01] 0x0 = Do Nothing 0x1 = Reset Meter-off Delay

> 28.1

> FuncButton

> int8u

> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x48 = Flash Off
> 0x50 = Bracketing Burst
> 0x58 = Matrix Metering
> 0x60 = Center-weighted Metering
> 0x68 = Spot Metering
> 0x70 = My Menu Top
> 0x78 = Live View
> 0x80 = + NEF (RAW)
> 0x88 = Virtual Horizon

> 29.1

> PreviewButton

> int8u

> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x40 = AF-ON
> 0x48 = Flash Off
> 0x50 = Bracketing Burst
> 0x58 = Matrix Metering
> 0x60 = Center-weighted Metering
> 0x68 = Spot Metering
> 0x70 = My Menu Top
> 0x78 = Live View
> 0x80 = + NEF (RAW)
> 0x88 = Virtual Horizon

> 30.1

> AELockButton

> int8u

> (D300)
> [Mask 0xf8]

> 0x0 = None
> 0x8 = Preview
> 0x10 = FV Lock
> 0x18 = AE/AF Lock
> 0x20 = AE Lock Only
> 0x28 = AE Lock (reset on release)
> 0x30 = AE Lock (hold)
> 0x38 = AF Lock Only
> 0x40 = AF-ON
> 0x48 = Flash Off
> 0x50 = Bracketing Burst
> 0x58 = Matrix Metering
> 0x60 = Center-weighted Metering
> 0x68 = Spot Metering
> 0x70 = My Menu Top
> 0x78 = Live View
> 0x80 = + NEF (RAW)
> 0x88 = Virtual Horizon

> 31.1

> FuncButtonPlusDials

> int8u

> [Mask 0x70]

> 0x0 = None
> 0x10 = Choose Image Area
> 0x20 = One Step Speed/Aperture
> 0x30 = Choose Non-CPU Lens Number
> 0x50 = Auto bracketing
> 0x60 = Dynamic AF Area
> 0x70 = Shutter speed & Aperture lock

> 31.2

> PreviewButtonPlusDials

> int8u

> [Mask 0x07]

> 0x0 = None
> 0x1 = Choose Image Area
> 0x2 = One Step Speed/Aperture
> 0x3 = Choose Non-CPU Lens Number
> 0x5 = Auto bracketing
> 0x6 = Dynamic AF Area
> 0x7 = Shutter speed & Aperture lock

> 32.1

> AELockButtonPlusDials

> int8u

> [Mask 0x70]

> 0x0 = None
> 0x10 = Choose Image Area
> 0x20 = One Step Speed/Aperture
> 0x30 = Choose Non-CPU Lens Number
> 0x50 = Auto bracketing
> 0x60 = Dynamic AF Area
> 0x70 = Shutter speed & Aperture lock

> 33.1 | CommandDialsReverseRotation | int8u | [Mask 0x80] 0x0 = No 0x80 = Yes
> 33.2 | CommandDialsChangeMainSub | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 33.3 | CommandDialsApertureSetting | int8u | [Mask 0x20] 0x0 = Sub-command Dial 0x20 = Aperture Ring
> 33.4 | CommandDialsMenuAndPlayback | int8u | [Mask 0x10] 0x0 = Off 0x10 = On
> 33.5 | ReverseIndicators | int8u | [Mask 0x08] 0x0 = + 0 - 0x8 = - 0 +
> 33.6 | PhotoInfoPlayback | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 33.7 | NoMemoryCard | int8u | [Mask 0x02] 0x0 = Release Locked 0x2 = Enable Release
> 33.8 | ReleaseButtonToUseDial | int8u | [Mask 0x01] 0x0 = No 0x1 = Yes

## NikonCustom SettingsD800 Tags

Custom settings for the D800.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 12.1

> AutoBracketingSet

> int8u

> [Mask 0xe0]
> 0x0 = AE & Flash
> 0x20 = AE Only
> 0x40 = Flash Only
> 0x60 = WB Bracketing
> 0x80 = Active D-Lighting

> 12.2 | AutoBracketOrder | int8u | [Mask 0x10] 0x0 = 0,-,+ 0x10 = -,0,+
> 12.3 | AutoBracketingMode | int8u | [Mask 0x0c] 0x0 = Flash/Speed 0x4 = Flash/Speed/Aperture 0x8 = Flash/Aperture 0xc = Flash Only

> 22.1

> FlashSyncSpeed

> int8u

> [Mask 0xf0]

> 0x0 = 1/320 s (auto FP)
> 0x10 = 1/250 s (auto FP)
> 0x20 = 1/250 s
> 0x30 = 1/200 s
> 0x40 = 1/160 s
> 0x50 = 1/125 s
> 0x60 = 1/100 s
> 0x70 = 1/80 s
> 0x80 = 1/60 s

> 22.2

> FlashShutterSpeed

> int8u

> [Mask 0x0f]

> 0x0 = 1/60 s
> 0x1 = 1/30 s
> 0x2 = 1/15 s
> 0x3 = 1/8 s
> 0x4 = 1/4 s
> 0x5 = 1/2 s

> 0x6 = 1 s
> 0x7 = 2 s
> 0x8 = 4 s
> 0x9 = 8 s
> 0xa = 15 s
> 0xb = 30 s

> 23.1 | FlashControlBuilt-in | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Repeating Flash 0xc0 = Commander Mode
> 23.2 | ManualFlashOutput | int8u | [Mask 0x1f]
> 24.1 | RepeatingFlashOutput | int8u | [Mask 0x70]
> 24.2 | RepeatingFlashCount | int8u | [Mask 0x0f]
> 25.1 | RepeatingFlashRate | int8u | [Mask 0xf0]
> 25.2 | CommanderChannel | int8u | [Mask 0x03]
> 27.1 | CommanderInternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Off
> 27.2 | CommanderInternalManualOutput | int8u | [Mask 0x1f]
> 28.1 | CommanderGroupAMode | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Auto Aperture 0x80 = Manual 0xc0 = Off
> 28.2 | CommanderGroupAManualOutput | int8u | [Mask 0x1f]
> 29.1 | CommanderGroupBMode | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Auto Aperture 0x80 = Manual 0xc0 = Off
> 29.2 | CommanderGroupBManualOutput | int8u | [Mask 0x1f]
> 30.1 | ModelingFlash | int8u | [Mask 0x20] 0x0 = On 0x20 = Off
> 30.2 | CommanderInternalTTLComp | int8u | [Mask 0x1f]
> 31.1 | CommanderGroupA_TTL-AAComp | int8u | [Mask 0x1f]
> 32.1 | CommanderGroupB_TTL-AAComp | int8u | [Mask 0x1f]

## NikonCustom SettingsD5000 Tags

Custom settings for the D5000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AFAreaModeSetting | int8u | [Mask 0x60] 0x0 = Single Area 0x20 = Dynamic Area 0x40 = Auto-area 0x60 = 3D-tracking (11 points)
> 0.2 | AFAssist | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 2.1 | Beep | int8u | [Mask 0xc0] 0x0 = Off 0x40 = Low 0x80 = High
> 2.2 | GridDisplay | int8u | [Mask 0x02] 0x0 = On 0x2 = Off
> 2.3 | ISODisplay | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 2.4 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 3.1 | FileNumberSequence | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 4.1 | RangeFinder | int8u | [Mask 0x10] 0x0 = Off 0x10 = On
> 4.2 | DateImprint | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 4.3 | ReverseIndicators | int8u | [Mask 0x80] 0x0 = + 0 - 0x80 = - 0 +
> 5.1 | EVStepSize | int8u | [Mask 0x40] 0x0 = 1/3 EV 0x40 = 1/2 EV
> 9.1 | ExposureDelayMode | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 11.1 | AutoBracketSet | int8u | [Mask 0xc0] 0x0 = Exposure 0x40 = Active D-Lighting 0x80 = WB Bracketing

> 12.1

> TimerFunctionButton

> int8u

> [Mask 0x38]

> 0x0 = Self-timer
> 0x8 = Release Mode
> 0x10 = Image Quality/Size
> 0x18 = ISO
> 0x20 = White Balance
> 0x28 = Active D-Lighting
> 0x30 = + NEF (RAW)
> 0x38 = Auto Bracketing

> 15.1

> AELockButton

> int8u

> [Mask 0x38]
> 0x0 = AE/AF Lock
> 0x8 = AE Lock Only
> 0x10 = AF Lock Only
> 0x18 = AE Lock (hold)
> 0x20 = AF-ON

> 16.1 | ShutterReleaseButtonAE-L | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 16.2 | CommandDialsReverseRotation | int8u | [Mask 0x80] 0x0 = No 0x80 = Yes

> 17.1

> MeteringTime

> int8u

> [Mask 0x70]
> 0x0 = 4 s
> 0x10 = 8 s
> 0x20 = 20 s
> 0x30 = 1 min
> 0x40 = 30 min

> 17.2 | RemoteOnDuration | int8u | [Mask 0x03] 0x0 = 1 min 0x1 = 5 min 0x2 = 10 min 0x3 = 15 min
> 18.1 | SelfTimerTime | int8u | [Mask 0xc0] 0x0 = 2 s 0x40 = 5 s 0x80 = 10 s 0xc0 = 20 s
> 18.2 | SelfTimerShotCount | int8u | [Mask 0x1e]

> 19.1

> ImageReviewTime

> int8u

> [Mask 0xe0]
> 0x0 = 4 s
> 0x20 = 8 s
> 0x40 = 20 s
> 0x60 = 1 min
> 0x80 = 10 min

> 20.1

> PlaybackMenusTime

> int8u

> [Mask 0xe0]
> 0x0 = 8 s
> 0x20 = 12 s
> 0x40 = 20 s
> 0x60 = 1 min
> 0x80 = 10 min

> 22.1 | InternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual
> 22.2 | ManualFlashOutput | int8u | [Mask 0x1f]
> 32.1 | LiveViewAF | int8u | [Mask 0x60] 0x0 = Face Priority 0x20 = Wide Area 0x40 = Normal Area 0x60 = Subject Tracking

## NikonCustom SettingsD5100 Tags

Custom settings for the D5100.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [Mask 0x80] 0x0 = Release 0x80 = Focus
> 1.1 | AFAssist | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 3.1 | Beep | int8u | [Mask 0xc0] 0x0 = Off 0x40 = Low 0x80 = High
> 3.2 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 3.3 | ISODisplay | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 4.1 | FileNumberSequence | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 5.1 | RangeFinder | int8u | [Mask 0x10] 0x0 = Off 0x10 = On
> 5.2 | ReverseIndicators | int8u | [Mask 0x80] 0x0 = + 0 - 0x80 = - 0 +
> 6.1 | EVStepSize | int8u | [Mask 0x40] 0x0 = 1/3 EV 0x40 = 1/2 EV
> 10.1 | ExposureDelayMode | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 12.1 | AutoBracketSet | int8u | [Mask 0xc0] 0x0 = Exposure 0x40 = WB Bracketing 0x80 = Active D-Lighting

> 13.1

> TimerFunctionButton

> int8u

> [Mask 0x38]

> 0x0 = Self-timer
> 0x8 = Release Mode
> 0x10 = Image Quality/Size
> 0x18 = ISO
> 0x20 = White Balance
> 0x28 = Active D-Lighting
> 0x30 = + NEF (RAW)
> 0x38 = Auto Bracketing

> 16.1

> AELockButton

> int8u

> [Mask 0x38]
> 0x0 = AE/AF Lock
> 0x8 = AE Lock Only
> 0x10 = AF Lock Only
> 0x18 = AE Lock (hold)
> 0x20 = AF-ON

> 17.1 | ShutterReleaseButtonAE-L | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 17.2 | CommandDialsReverseRotation | int8u | [Mask 0x80] 0x0 = No 0x80 = Yes

> 18.1

> MeteringTime

> int8u

> [Mask 0x70]
> 0x0 = 4 s
> 0x10 = 8 s
> 0x20 = 20 s
> 0x30 = 1 min
> 0x40 = 30 min

> 18.2 | RemoteOnDuration | int8u | [Mask 0x03] 0x0 = 1 min 0x1 = 5 min 0x2 = 10 min 0x3 = 20 min
> 19.1 | SelfTimerTime | int8u | [Mask 0xc0] 0x0 = 2 s 0x40 = 5 s 0x80 = 10 s 0xc0 = 20 s
> 19.2 | SelfTimerShotCount | int8u | [Mask 0x0f]

> 20.1

> ImageReviewTime

> int8u

> [Mask 0xe0]
> 0x0 = 4 s
> 0x20 = 8 s
> 0x40 = 20 s
> 0x60 = 1 min
> 0x80 = 10 min

> 20.2

> LiveViewMonitorOffTime

> int8u

> [Mask 0x1c]

> 0x0 = 3 min 0x4 = 5 min 0x8 = 10 min |  | 0xc = 15 min 0x10 = 20 min 0x14 = 30 min |

> 21.1

> PlaybackMenusTime

> int8u

> [Mask 0xe0]
> 0x0 = 8 s
> 0x20 = 12 s
> 0x40 = 20 s
> 0x60 = 1 min
> 0x80 = 10 min

> 23.1 | ManualFlashOutput | int8u | [Mask 0x1f]

## NikonCustom SettingsD5200 Tags

Custom settings for the D5200.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [Mask 0x80] 0x0 = Release 0x80 = Focus
> 0.2 | NumberOfFocusPoints | int8u | [Mask 0x10] 0x0 = 39 Points 0x10 = 11 Points
> 1.1 | AFAssist | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 3.1 | Beep | int8u | [Mask 0xc0] 0x0 = Off 0x40 = Low 0x80 = High
> 3.2 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 3.3 | ISODisplay | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 4.1 | FileNumberSequence | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 5.1 | RangeFinder | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 5.2 | ReverseExposureCompDial | int8u | [Mask 0x10] 0x0 = No 0x10 = Yes
> 5.3 | ReverseShutterSpeedAperture | int8u | [Mask 0x08] 0x0 = No 0x8 = Yes
> 5.4 | ReverseIndicators | int8u | [Mask 0x80] 0x0 = + 0 - 0x80 = - 0 +
> 6.1 | EVStepSize | int8u | [Mask 0x40] 0x0 = 1/3 EV 0x40 = 1/2 EV
> 10.1 | ExposureDelayMode | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 12.1 | AutoBracketSet | int8u | [Mask 0xc0] 0x0 = Exposure 0x40 = WB Bracketing 0x80 = Active D-Lighting

> 13.1

> FunctionButton

> int8u

> [Mask 0x1f]

> 0x3 = AE/AF Lock
> 0x4 = AE Lock Only
> 0x6 = AE Lock (hold)
> 0x7 = AF Lock Only
> 0x8 = AF-ON
> 0x10 = + NEF (RAW)
> 0x12 = Active D-Lighting
> 0x19 = Live View
> 0x1a = Image Quality
> 0x1b = ISO
> 0x1c = White Balance
> 0x1d = HDR
> 0x1e = Auto Bracketing
> 0x1f = AF-area Mode

> 16.1

> AELockButton

> int8u

> [Mask 0x0f]
> 0x3 = AE/AF Lock
> 0x4 = AE Lock Only
> 0x6 = AE Lock (hold)
> 0x7 = AF Lock Only
> 0x8 = AF-ON

> 17.1 | ShutterReleaseButtonAE-L | int8u | [Mask 0x02] 0x0 = Off 0x2 = On

> 18.1

> StandbyTimer

> int8u

> [Mask 0xe0]
> 0x0 = 4 s
> 0x20 = 8 s
> 0x40 = 20 s
> 0x60 = 1 min
> 0x80 = 30 min

> 18.2 | RemoteOnDuration | int8u | [Mask 0x03] 0x0 = 1 min 0x1 = 5 min 0x2 = 10 min 0x3 = 15 min
> 19.1 | SelfTimerTime | int8u | [Mask 0xc0] 0x0 = 2 s 0x40 = 5 s 0x80 = 10 s 0xc0 = 20 s
> 19.2 | SelfTimerShotCount | int8u | [Mask 0x0f]

> 20.1

> ImageReviewTime

> int8u

> [Mask 0xe0]
> 0x20 = 4 s
> 0x40 = 8 s
> 0x80 = 20 s
> 0xa0 = 1 min
> 0xe0 = 10 min

> 20.2

> LiveViewMonitorOffTime

> int8u

> [Mask 0x1c]
> 0x4 = 5 min
> 0x8 = 10 min
> 0xc = 15 min
> 0x10 = 20 min
> 0x14 = 30 min

> 21.1

> PlaybackMenusTime

> int8u

> [Mask 0xe0]
> 0x20 = 8 s
> 0x80 = 20 s
> 0xa0 = 1 min
> 0xc0 = 5 min
> 0xe0 = 10 min

> 23.1 | InternalFlash | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual
> 23.2 | ManualFlashOutput | int8u | [Mask 0x1f]

## NikonCustom SettingsD7000 Tags

Custom settings for the D7000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [Mask 0x80] 0x0 = Release 0x80 = Focus
> 0.2 | AF-SPrioritySelection | int8u | [Mask 0x20] 0x0 = Focus 0x20 = Release
> 0.3 | NumberOfFocusPoints | int8u | [Mask 0x10] 0x0 = 39 Points 0x10 = 11 Points

> 0.4

> FocusTrackingLockOn

> int8u

> [Mask 0x07]

> 0x0 = Off 0x1 = 1 Short 0x2 = 2 |  | 0x3 = 3 Normal 0x4 = 4 0x5 = 5 Long |

> 1.2 | FocusPointWrap | int8u | [Mask 0x08] 0x0 = No Wrap 0x8 = Wrap
> 1.3 | AFPointIllumination | int8u | [Mask 0x06] 0x0 = Auto 0x2 = On 0x4 = Off
> 1.4 | AFAssist | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 2.1 | BatteryOrder | int8u | [Mask 0x40] 0x0 = MB-D11 First 0x40 = Camera Battery First

> 2.2

> AF-OnForMB-D11

> int8u

> [Mask 0x1c]

> 0x0 = AE/AF Lock
> 0x4 = AE Lock Only
> 0x8 = AF Lock Only
> 0xc = AE Lock (hold)
> 0x10 = AF-ON
> 0x14 = FV Lock
> 0x18 = Same as FUNC Button

> 2.3 | MB-D11BatteryType | int8u | [Mask 0x03] 0x0 = LR6 (AA alkaline) 0x1 = Ni-MH (AA Ni-MH) 0x2 = FR6 (AA lithium)
> 3.1 | BeepPitch | int8u | [Mask 0xc0] 0x0 = Off 0x40 = Low 0x80 = High
> 3.2 | NoMemoryCard | int8u | [Mask 0x20] 0x0 = Release Locked 0x20 = Enable Release
> 3.3 | ISODisplay | int8u | [Mask 0x0c] 0x0 = Show ISO/Easy ISO 0x4 = Show ISO Sensitivity 0xc = Show Frame Count
> 3.4 | GridDisplay | int8u | [Mask 0x02] 0x0 = On 0x2 = Off
> 3.5 | ViewfinderWarning | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 4.1 | ShootingInfoDisplay | int8u | [Mask 0xc0] 0x0 = Auto 0x80 = Manual (dark on light) 0xc0 = Manual (light on dark)
> 4.2 | LCDIllumination | int8u | [Mask 0x20] 0x0 = Off 0x20 = On
> 4.3 | FileNumberSequence | int8u | [Mask 0x08] 0x0 = On 0x8 = Off
> 4.4 | ScreenTips | int8u | [Mask 0x04] 0x0 = Off 0x4 = On
> 4.5 | BeepVolume | int8u | [Mask 0x03] 0x0 = Off 0x1 = 1 0x2 = 2 0x3 = 3
> 5.1 | ReverseIndicators | int8u | [Mask 0x80] 0x0 = + 0 - 0x80 = - 0 +
> 5.2 | EasyExposureCompensation | int8u | [Mask 0x03] 0x0 = Off 0x1 = On 0x2 = On Auto Reset
> 6.1 | ExposureControlStep | int8u | [Mask 0x40] 0x0 = 1/3 EV 0x40 = 1/2 EV
> 6.2 | ISOSensitivityStep | int8u | [Mask 0x10] 0x0 = 1/3 EV 0x10 = 1/2 EV

> 7.1

> CenterWeightedAreaSize

> int8u

> [Mask 0xe0]
> 0x0 = 6 mm
> 0x20 = 8 mm
> 0x40 = 10 mm
> 0x60 = 13 mm
> 0x80 = Average

> 10.1 | ExposureDelayMode | int8u | [Mask 0x40] 0x0 = Off 0x40 = On
> 10.2 | CLModeShootingSpeed | int8u | [Mask 0x07]
> 11 | MaxContinuousRelease | int8u |

> 12.1

> AutoBracketSet

> int8u

> [Mask 0xe0]
> 0x0 = AE & Flash
> 0x20 = AE Only
> 0x40 = Flash Only
> 0x60 = WB Bracketing
> 0x80 = Active D-Lighting

> 12.2 | AutoBracketOrder | int8u | [Mask 0x10] 0x0 = 0,-,+ 0x10 = -,0,+

> 13.1

> FuncButton

> int8u

> [Mask 0xf8]

> 0x0 = Grid Display
> 0x8 = FV Lock
> 0x10 = Flash Off
> 0x18 = Matrix Metering
> 0x20 = Center-weighted Metering
> 0x28 = Spot Metering
> 0x30 = My Menu Top
> 0x38 = + NEF (RAW)
> 0x40 = Active D-Lighting
> 0x48 = Preview
> 0x50 = AE/AF Lock
> 0x58 = AE Lock Only
> 0x60 = AF Lock Only
> 0x68 = AE Lock (hold)
> 0x70 = Bracketing Burst
> 0x78 = Playback
> 0x80 = 1EV Step Speed/Aperture
> 0x88 = Choose Non-CPU Lens
> 0x90 = Virtual Horizon
> 0x98 = Start Movie Recording

> 14.1

> PreviewButton

> int8u

> [Mask 0xf8]

> 0x0 = Grid Display
> 0x8 = FV Lock
> 0x10 = Flash Off
> 0x18 = Matrix Metering
> 0x20 = Center-weighted Metering
> 0x28 = Spot Metering
> 0x30 = My Menu Top
> 0x38 = + NEF (RAW)
> 0x40 = Active D-Lighting
> 0x48 = Preview
> 0x50 = AE/AF Lock
> 0x58 = AE Lock Only
> 0x60 = AF Lock Only
> 0x68 = AE Lock (hold)
> 0x70 = Bracketing Burst
> 0x78 = Playback
> 0x80 = 1EV Step Speed/Aperture
> 0x88 = Choose Non-CPU Lens
> 0x90 = Virtual Horizon
> 0x98 = Start Movie Recording

> 15.1 | OKButton | int8u | [Mask 0x18] 0x0 = Off 0x8 = Select Center Focus Point 0x10 = Highlight Active Focus Point 0x18 = Not Used

> 16.1

> AELockButton

> int8u

> [Mask 0x38]

> 0x0 = AE/AF Lock 0x8 = AE Lock Only 0x10 = AF Lock Only |  | 0x18 = AE Lock (hold) 0x20 = AF-ON 0x28 = FV Lock |

> 17.1 | CommandDialsReverseRotation | int8u | [Mask 0x80] 0x0 = No 0x80 = Yes
> 17.2 | CommandDialsChangeMainSub | int8u | [Mask 0x60] 0x0 = Off 0x20 = On 0x40 = On (A mode only)
> 17.3 | CommandDialsApertureSetting | int8u | [Mask 0x04] 0x0 = Sub-command Dial 0x4 = Aperture Ring
> 17.4 | CommandDialsMenuAndPlayback | int8u | [Mask 0x18] 0x0 = On 0x8 = Off 0x10 = On (Image Review Exclude)
> 17.5 | ShutterReleaseButtonAE-L | int8u | [Mask 0x02] 0x0 = Off 0x2 = On
> 17.6 | ReleaseButtonToUseDial | int8u | [Mask 0x01] 0x0 = No 0x1 = Yes

> 18.1

> MeteringTime

> int8u

> [Mask 0xf0]

> 0x0 = 4 s 0x10 = 6 s 0x20 = 8 s 0x30 = 16 s 0x40 = 30 s |  | 0x50 = 1 min 0x60 = 5 min 0x70 = 10 min 0x80 = 30 min 0x90 = No Limit |

> 18.2 | RemoteOnDuration | int8u | [Mask 0x03] 0x0 = 1 min 0x1 = 5 min 0x2 = 10 min 0x3 = 15 min
> 19.1 | SelfTimerTime | int8u | [Mask 0xc0] 0x0 = 2 s 0x40 = 5 s 0x80 = 10 s 0xc0 = 20 s
> 19.2 | SelfTimerInterval | int8u | [Mask 0x30] 0x0 = 0.5 s 0x10 = 1 s 0x20 = 2 s 0x30 = 3 s
> 19.3 | SelfTimerShotCount | int8u | [Mask 0x0f]

> 20.1

> ImageReviewTime

> int8u

> [Mask 0xe0]

> 0x0 = 4 s 0x20 = 10 s 0x40 = 20 s |  | 0x60 = 1 min 0x80 = 5 min 0xa0 = 10 min |

> 20.2

> LiveViewMonitorOffTime

> int8u

> [Mask 0x1c]

> 0x0 = 4 s 0x4 = 10 s 0x8 = 20 s |  | 0xc = 1 min 0x10 = 5 min 0x14 = 10 min |

> 21.1

> MenuMonitorOffTime

> int8u

> [Mask 0xe0]

> 0x0 = 4 s 0x20 = 10 s 0x40 = 20 s |  | 0x60 = 1 min 0x80 = 5 min 0xa0 = 10 min |

> 21.2

> ShootingInfoMonitorOffTime

> int8u

> [Mask 0x1c]

> 0x0 = 4 s 0x4 = 10 s 0x8 = 20 s |  | 0xc = 1 min 0x10 = 5 min 0x14 = 10 min |

> 22.1

> FlashSyncSpeed

> int8u

> [Mask 0xf0]

> 0x0 = 1/320 s (auto FP)
> 0x10 = 1/250 s (auto FP)
> 0x20 = 1/250 s
> 0x30 = 1/200 s
> 0x40 = 1/160 s
> 0x50 = 1/125 s
> 0x60 = 1/100 s
> 0x70 = 1/80 s
> 0x80 = 1/60 s

> 22.2

> FlashShutterSpeed

> int8u

> [Mask 0x0f]

> 0x0 = 1/60 s
> 0x1 = 1/30 s
> 0x2 = 1/15 s
> 0x3 = 1/8 s
> 0x4 = 1/4 s
> 0x5 = 1/2 s

> 0x6 = 1 s
> 0x7 = 2 s
> 0x8 = 4 s
> 0x9 = 8 s
> 0xa = 15 s
> 0xb = 30 s

> 23.1 | FlashControlBuilt-in | int8u | [Mask 0xc0] 0x0 = TTL 0x40 = Manual 0x80 = Repeating Flash 0xc0 = Commander Mode
> 23.2 | ManualFlashOutput | int8u | [Mask 0x1f]
> 24.1 | RepeatingFlashOutput | int8u | [Mask 0x70]
> 24.2 | RepeatingFlashCount | int8u | [Mask 0x0f]
> 25.1 | RepeatingFlashRate | int8u | [Mask 0xf0]
> 26.1 | CommanderInternalTTLCompBuiltin | int8u | [Mask 0x1f]
> 27.1 | CommanderInternalTTLCompGroupA | int8u | [Mask 0x1f]
> 28.1 | CommanderInternalTTLCompGroupB | int8u | [Mask 0x1f]
> 30.1 | FlashWarning | int8u | [Mask 0x80] 0x0 = On 0x80 = Off
> 30.2 | ModelingFlash | int8u | [Mask 0x20] 0x0 = On 0x20 = Off
> 34.1 | LiveViewAFAreaMode | int8u | [Mask 0x60] 0x0 = Face-Priority 0x20 = NormalArea 0x40 = WideArea 0x60 = SubjectTracking
> 34.2 | LiveViewAFMode | int8u | [Mask 0x02] 0x0 = AF-C 0x2 = AF-F

> 35.1

> PlaybackMonitorOffTime

> int8u

> [Mask 0xe0]

> 0x0 = 4 s 0x20 = 10 s 0x40 = 20 s |  | 0x60 = 1 min 0x80 = 5 min 0xa0 = 10 min |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Mar 23, 2013

<-- ExifTool Tag Names