## Pentax Tags

These tags are used in Pentax/Asahi cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | PentaxVersion | int8u[4] |
> 0x0001 | PentaxModelType | int16u |
> 0x0002 | PreviewImageSize | int16u[2]~ |
> 0x0003 | PreviewImageLength | int32u* |
> 0x0004 | PreviewImageStart | int32u* |
> 0x0005 | PentaxModelID | int32u | --> Pentax PentaxModelID Values
> 0x0006 | Date | undef[4] | (changing either Date or Time will affect ShutterCount decryption)
> 0x0007 | Time | undef[3] |

> 0x0008

> Quality

> int16u

> 0 = Good 1 = Better 2 = Best 3 = TIFF |  | 4 = RAW 5 = Premium 65535 = n/a |

> 0x0009

> PentaxImageSize

> int16u

> 0 = 640x480
> 1 = Full
> 2 = 1024x768
> 3 = 1280x960
> 4 = 1600x1200
> 5 = 2048x1536
> 8 = 2560x1920 or 2304x1728
> 9 = 3072x2304
> 10 = 3264x2448
> 19 = 320x240
> 20 = 2288x1712
> 21 = 2592x1944
> 22 = 2304x1728 or 2592x1944
> 23 = 3056x2296
> 25 = 2816x2212 or 2816x2112
> 27 = 3648x2736

> 29 = 4000x3000
> 30 = 4288x3216
> 31 = 4608x3456
> 129 = 1920x1080
> 135 = 4608x2592
> 257 = 3216x3216
> '0 0' = 2304x1728
> '4 0' = 1600x1200
> '5 0' = 2048x1536
> '8 0' = 2560x1920
> '32 2' = 960x640
> '33 2' = 1152x768
> '34 2' = 1536x1024
> '35 1' = 2400x1600
> '36 0' = 3008x2008 or 3040x2024
> '37 0' = 3008x2000

> 0x000b

> PictureMode

> int16u[n]

> (1 or 2 values. Decimal values differentiate Optio 555 modes which are different from other models)
> [Value 0]

> 0 = Program
> 0.1 = Av
> 1 = Shutter Speed Priority
> 1.1 = M
> 2 = Program AE
> 2.1 = Tv
> 3 = Manual
> 3.1 = USER
> 5 = Portrait
> 6 = Landscape
> 8 = Sport
> 9 = Night Scene
> 11 = Soft
> 12 = Surf & Snow
> 13 = Candlelight
> 14 = Autumn
> 15 = Macro
> 17 = Fireworks
> 18 = Text
> 19 = Panorama
> 20 = 3-D
> 21 = Black & White
> 22 = Sepia
> 23 = Red
> 24 = Pink
> 25 = Purple
> 26 = Blue
> 27 = Green
> 28 = Yellow

> 30 = Self Portrait
> 31 = Illustrations
> 33 = Digital Filter
> 35 = Night Scene Portrait
> 37 = Museum
> 38 = Food
> 39 = Underwater
> 40 = Green Mode
> 49 = Light Pet
> 50 = Dark Pet
> 51 = Medium Pet
> 53 = Underwater
> 54 = Candlelight
> 55 = Natural Skin Tone
> 56 = Synchro Sound Record
> 58 = Frame Composite
> 59 = Report
> 60 = Kids
> 61 = Blur Reduction
> 63 = Panorama 2
> 65 = Half-length Portrait
> 66 = Portrait 2
> 75 = Blue Sky
> 80 = Miniature
> 81 = HDR
> 83 = Fisheye
> 221 = P
> 255 = PICT

> 0x000c

> FlashMode

> int16u[n]

> [Value 0]

> 0x0 = Auto, Did not fire
> 0x1 = Off, Did not fire
> 0x2 = On, Did not fire
> 0x3 = Auto, Did not fire, Red-eye reduction
> 0x5 = On, Did not fire, Wireless (Master)
> 0x100 = Auto, Fired
> 0x102 = On, Fired
> 0x103 = Auto, Fired, Red-eye reduction
> 0x104 = On, Red-eye reduction
> 0x105 = On, Wireless (Master)
> 0x106 = On, Wireless (Control)
> 0x108 = On, Soft
> 0x109 = On, Slow-sync
> 0x10a = On, Slow-sync, Red-eye reduction
> 0x10b = On, Trailing-curtain Sync

> [Value 1]

> 0x0 = n/a - Off-Auto-Aperture
> 0x3f = Internal
> 0x100 = External, Auto
> 0x23f = External, Flash Problem
> 0x300 = External, Manual
> 0x304 = External, P-TTL Auto
> 0x305 = External, Contrast-control Sync
> 0x306 = External, High-speed Sync
> 0x30c = External, Wireless
> 0x30d = External, Wireless, High-speed Sync

> 0x000d

> FocusMode

> int16u

> (Pentax models)

> 0 = Normal
> 1 = Macro
> 2 = Infinity
> 3 = Manual
> 4 = Super Macro
> 5 = Pan Focus

> 16 = AF-S
> 17 = AF-C
> 18 = AF-A
> 32 = Contrast-detect
> 33 = Tracking Contrast-detect
> 288 = Face Detect

> (Asahi models)
> 0 = Normal
> 1 = Macro (1)
> 2 = Macro (2)
> 3 = Infinity

> 0x000e

> AFPointSelected

> int16u

> [Value 0]

> 0 = None
> 1 = Upper-left
> 2 = Top
> 3 = Upper-right
> 4 = Left
> 5 = Mid-left
> 6 = Center
> 7 = Mid-right
> 8 = Right

> 9 = Lower-left
> 10 = Bottom
> 11 = Lower-right
> 65531 = AF Select
> 65532 = Face Detect AF
> 65533 = Automatic Tracking AF
> 65534 = Fixed Center
> 65535 = Auto

> 0x000f

> AFPointsInFocus

> int16u

> 0x0 = Fixed Center or Multiple
> 0x1 = Top-left
> 0x2 = Top-center
> 0x3 = Top-right
> 0x4 = Left
> 0x5 = Center
> 0x6 = Right
> 0x7 = Bottom-left
> 0x8 = Bottom-center
> 0x9 = Bottom-right
> 0xffff = None

> 0x0010 | FocusPosition | int16u | (related to focus distance but affected by focal length)
> 0x0012 | ExposureTime | int32u |
> 0x0013 | FNumber | int16u |

> 0x0014

> ISO

> int16u

> (may be different than EXIF:ISO, which can round to the nearest full stop)

> 3 = 50
> 4 = 64
> 5 = 80
> 6 = 100
> 7 = 125
> 8 = 160
> 9 = 200
> 10 = 250
> 11 = 320
> 12 = 400
> 13 = 500
> 14 = 640
> 15 = 800
> 16 = 1000
> 17 = 1250

> 18 = 1600
> 19 = 2000
> 20 = 2500
> 21 = 3200
> 22 = 4000
> 23 = 5000
> 24 = 6400
> 25 = 8000
> 26 = 10000
> 27 = 12800
> 28 = 16000
> 29 = 20000
> 30 = 25600
> 31 = 32000
> 32 = 40000

> 33 = 51200
> 50 = 50
> 100 = 100
> 200 = 200
> 258 = 50
> 259 = 70
> 260 = 100
> 261 = 140
> 262 = 200
> 263 = 280
> 264 = 400
> 265 = 560
> 266 = 800
> 267 = 1100
> 268 = 1600

> 269 = 2200
> 270 = 3200
> 271 = 4500
> 272 = 6400
> 273 = 9000
> 274 = 12800
> 275 = 18000
> 276 = 25600
> 277 = 36000
> 278 = 51200
> 400 = 400
> 800 = 800
> 1600 = 1600
> 3200 = 3200

> 0x0015 | LightReading | int16u | (calibrated differently for different models. For the Optio WP, add 6 to get approximate Light Value. May not be valid for some models, ie. Optio S)
> 0x0016 | ExposureCompensation | int16u |
> 0x0017 | MeteringMode | int16u | 0 = Multi-segment 1 = Center-weighted average 2 = Spot
> 0x0018 | AutoBracketing | int16u[n] | (1 or 2 values: exposure bracket step in EV, then extended bracket if available. Extended bracket values are printed as 'WB-BA', 'WB-GM', 'Saturation', 'Sharpness', 'Contrast', 'Hue' or 'HighLowKey' followed by '+1', '+2' or '+3' for step size)

> 0x0019

> WhiteBalance

> int16u

> 0 = Auto
> 1 = Daylight
> 2 = Shade
> 3 = Fluorescent
> 4 = Tungsten
> 5 = Manual
> 6 = Daylight Fluorescent
> 7 = Day White Fluorescent

> 8 = White Fluorescent
> 9 = Flash
> 10 = Cloudy
> 15 = Color Temperature Enhancement
> 17 = Kelvin
> 65534 = Unknown
> 65535 = User-Selected

> 0x001a

> WhiteBalanceMode

> int16u

> 1 = Auto (Daylight)
> 2 = Auto (Shade)
> 3 = Auto (Flash)
> 4 = Auto (Tungsten)
> 6 = Auto (Daylight Fluorescent)
> 7 = Auto (Day White Fluorescent)
> 8 = Auto (White Fluorescent)
> 10 = Auto (Cloudy)
> 65534 = Unknown
> 65535 = User-Selected

> 0x001b | BlueBalance | int16u |
> 0x001c | RedBalance | int16u |
> 0x001d | FocalLength | int32u |
> 0x001e | DigitalZoom | int16u |

> 0x001f

> Saturation

> int16u[n]

> (1 or 2 values)
> [Value 0]

> 0 = Low 1 = Normal 2 = High 3 = Med Low 4 = Med High |  | 5 = Very Low 6 = Very High 7 = -4 8 = +4 65535 = None |

> 0x0020

> Contrast

> int16u[n]

> (1 or 2 values)
> [Value 0]

> 0 = Low 1 = Normal 2 = High 3 = Med Low 4 = Med High |  | 5 = Very Low 6 = Very High 7 = -4 8 = +4 |

> 0x0021

> Sharpness

> int16u[n]

> (1 or 2 values)
> [Value 0]

> 0 = Soft 1 = Normal 2 = Hard 3 = Med Soft 4 = Med Hard |  | 5 = Very Soft 6 = Very Hard 7 = -4 8 = +4 |

> 0x0022 | WorldTimeLocation | int16u | 0 = Hometown 1 = Destination
> 0x0023 | HometownCity | int16u | --> Pentax City Values
> 0x0024 | DestinationCity | int16u | --> Pentax City Values
> 0x0025 | HometownDST | int16u | 0 = No 1 = Yes
> 0x0026 | DestinationDST | int16u | 0 = No 1 = Yes
> 0x0027 | DSPFirmwareVersion | undef |
> 0x0028 | CPUFirmwareVersion | undef |
> 0x0029 | FrameNumber | int32u |
> 0x002d | EffectiveLV EffectiveLV | int16u int32u | (camera-calculated light value, but includes exposure compensation)

> 0x0032

> ImageEditing

> undef[4]

> '0 0' = None
> '0 0 0 0' = None
> '0 0 0 4' = Digital Filter
> '1 0 0 0' = Resized
> '2 0 0 0' = Cropped
> '4 0 0 0' = Digital Filter 4
> '6 0 0 0' = Digital Filter 6
> '16 0 0 0' = Frame Synthesis?

> 0x0033

> PictureMode

> int8u[3]

> [Values 0-1]

> '0 0' = Program
> '0 1' = Hi-speed Program
> '0 2' = DOF Program
> '0 3' = MTF Program
> '0 4' = Standard
> '0 5' = Portrait
> '0 6' = Landscape
> '0 7' = Macro
> '0 8' = Sport
> '0 9' = Night Scene Portrait
> '0 10' = No Flash
> '0 11' = Night Scene
> '0 12' = Surf & Snow
> '0 13' = Text
> '0 14' = Sunset
> '0 15' = Kids
> '0 16' = Pet
> '0 17' = Candlelight
> '0 18' = Museum
> '0 19' = Food
> '0 20' = Stage Lighting
> '0 21' = Night Snap
> '0 23' = Blue Sky
> '0 24' = Sunset
> '0 26' = Night Scene HDR
> '0 27' = HDR
> '0 28' = Quick Macro
> '0 29' = Forest
> '0 30' = Backlight Silhouette
> '1 4' = Auto PICT (Standard)
> '1 5' = Auto PICT (Portrait)

> '1 6' = Auto PICT (Landscape)
> '1 7' = Auto PICT (Macro)
> '1 8' = Auto PICT (Sport)
> '2 0' = Program (HyP)
> '2 1' = Hi-speed Program (HyP)
> '2 2' = DOF Program (HyP)
> '2 3' = MTF Program (HyP)
> '2 22' = Shallow DOF (HyP)
> '3 0' = Green Mode
> '4 0' = Shutter Speed Priority
> '5 0' = Aperture Priority
> '6 0' = Program Tv Shift
> '7 0' = Program Av Shift
> '8 0' = Manual
> '9 0' = Bulb
> '10 0' = Aperture Priority, Off-Auto-Aperture
> '11 0' = Manual, Off-Auto-Aperture
> '12 0' = Bulb, Off-Auto-Aperture
> '13 0' = Shutter & Aperture Priority AE
> '15 0' = Sensitivity Priority AE
> '16 0' = Flash X-Sync Speed AE
> '18 0' = Auto Program (Normal)
> '18 1' = Auto Program (Hi-speed)
> '18 2' = Auto Program (DOF)
> '18 3' = Auto Program (MTF)
> '18 22' = Auto Program (Shallow DOF)
> '20 22' = Blur Control
> '254 0' = Video
> '255 0' = Video (Auto Aperture)
> '255 4' = Video (4)

> [Value 2]

> 0 = 1/2 EV steps |  | 1 = 1/3 EV steps |

> 0x0034

> DriveMode

> int8u[4]

> [Value 0]
> 0 = Single-frame
> 1 = Continuous
> 2 = Continuous (Lo)
> 3 = Burst
> 255 = Video
> [Value 1]

> 0 = No Timer 1 = Self-timer (12 s) 2 = Self-timer (2 s) |  | 15 = Video 16 = Mirror Lock-up 255 = n/a |

> [Value 2]
> 0 = Shutter Button
> 1 = Remote Control (3 s delay)
> 2 = Remote Control
> 4 = Remote Continuous Shooting
> [Value 3]

> 0 = Single Exposure 1 = Multiple Exposure 15 = Interval Movie 16 = HDR 32 = HDR Strong 1 |  | 48 = HDR Strong 2 64 = HDR Strong 3 224 = HDR Auto 255 = Video |

> 0x0035 | SensorSize | int16u[2] | (includes masked pixels)
> 0x0037 | ColorSpace | int16u | 0 = sRGB 1 = Adobe RGB
> 0x0038 | ImageAreaOffset | int16u[2] |
> 0x0039 | RawImageSize | int16u[2]~ |

> 0x003c

> AFPointsInFocus

> N

> (*istD only)

> Bit 0 = Upper-left
> Bit 1 = Top
> Bit 2 = Upper-right
> Bit 3 = Left
> Bit 4 = Mid-left
> Bit 5 = Center

> Bit 6 = Mid-right
> Bit 7 = Right
> Bit 8 = Lower-left
> Bit 9 = Bottom
> Bit 10 = Lower-right

> 0x003e | PreviewImageBorders | int8u[4] | (top, bottom, left, right)
> 0x003f | LensRec | - | --> Pentax LensRec Tags
> 0x0040 | SensitivityAdjust | int16u |
> 0x0041 | ImageEditCount | int16u |
> 0x0047 | CameraTemperature | int8s |
> 0x0048 | AELock | int16u | 0 = Off 1 = On
> 0x0049 | NoiseReduction | int16u | 0 = Off 1 = On
> 0x004d | FlashExposureComp | int32s |

> 0x004f

> ImageTone

> int16u

> 0 = Natural 1 = Bright 2 = Portrait 3 = Landscape 4 = Vibrant |  | 5 = Monochrome 6 = Muted 7 = Reversal Film 8 = Bleach Bypass 9 = Radiant |

> 0x0050 | ColorTemperature | int16u |
> 0x0053 | ColorTempDaylight | undef[4] | (0x0053-0x005a are 3 numbers: Kelvin, shift AB, shift GM)
> 0x0054 | ColorTempShade | undef[4] |
> 0x0055 | ColorTempCloudy | undef[4] |
> 0x0056 | ColorTempTungsten | undef[4] |
> 0x0057 | ColorTempFluorescentD | undef[4] |
> 0x0058 | ColorTempFluorescentN | undef[4] |
> 0x0059 | ColorTempFluorescentW | undef[4] |
> 0x005a | ColorTempFlash | undef[4] |
> 0x005c | ShakeReductionInfo | - | --> Pentax SRInfo Tags
> 0x005d | ShutterCount | undef[4] | (Note: May be reset by servicing! Also, does not include shutter actuations for live view or video recording)
> 0x0060 | FaceInfo | - | --> Pentax FaceInfo Tags

> 0x0062

> RawDevelopmentProcess

> int16u

> 1 = 1 (K10D,K200D,K2000,K-m)
> 3 = 3 (K20D)
> 4 = 4 (K-7)
> 5 = 5 (K-x)
> 6 = 6 (645D)
> 7 = 7 (K-r)
> 8 = 8 (K-5,K-5II,K-5IIs)
> 9 = 9 (Q)
> 10 = 10 (K-01,K-30)
> 11 = 11 (Q10)
> 12 = 12 (MX-1)

> 0x0067

> Hue

> int16u

> 0 = -2 1 = Normal 2 = 2 3 = -1 4 = 1 |  | 5 = -3 6 = 3 7 = -4 8 = 4 65535 = None |

> 0x0068 | AWBInfo | - | --> Pentax AWBInfo Tags

> 0x0069

> DynamicRangeExpansion

> undef[4]

> (called highlight correction by Pentax for the K20D, K-5, K-01 and maybe other models)

> '0 0 0 0' = Off
> '0 1 0 0' = Off (enabled)
> '0 2 0 0' = Off (auto)
> '1 0 0 0' = On
> '1 1 0 0' = On (enabled)
> '1 2 0 0' = On (auto)

> 0x006b | TimeInfo | - | --> Pentax TimeInfo Tags

> 0x006c

> HighLowKeyAdj

> int16s[2]

> '-1 0' = -1 '-2 0' = -2 '-3 0' = -3 |  | '-4 0' = -4 '0 0' = 0 '1 0' = 1 |  | '2 0' = 2 '3 0' = 3 '4 0' = 4 |

> 0x006d

> ContrastHighlight

> int16s[2]

> '-1 0' = -1 '-2 0' = -2 '-3 0' = -3 |  | '-4 0' = -4 '0 0' = 0 '1 0' = 1 |  | '2 0' = 2 '3 0' = 3 '4 0' = 4 |

> 0x006e

> ContrastShadow

> int16s[2]

> '-1 0' = -1 '-2 0' = -2 '-3 0' = -3 |  | '-4 0' = -4 '0 0' = 0 '1 0' = 1 |  | '2 0' = 2 '3 0' = 3 '4 0' = 4 |

> 0x006f | ContrastHighlightShadowAdj | int8u | 0 = Off 1 = On

> 0x0070

> FineSharpness

> int8u[n]

> [Value 0]
> 0 = Off
> 1 = On
> [Value 1]
> 0 = Normal
> 2 = Extra fine

> 0x0071

> HighISONoiseReduction

> int8u

> [Value 0]

> 0 = Off 1 = Weakest 2 = Weak |  | 3 = Strong 4 = Medium 255 = Auto |

> [Value 1]
> 0 = Inactive
> 1 = Active
> 2 = Active (Weak)
> 3 = Active (Strong)
> 4 = Active (Medium)
> [Value 2]
> 48 = ISO>400
> 56 = ISO>800
> 64 = ISO>1600
> 72 = ISO>3200

> 0x0072 | AFAdjustment | int16s |

> 0x0073

> MonochromeFilterEffect

> int16u

> 1 = Green 2 = Yellow 3 = Orange 4 = Red 5 = Magenta |  | 6 = Blue 7 = Cyan 8 = Infrared 65535 = None |

> 0x0074

> MonochromeToning

> int16u

> 0 = -4 1 = -3 2 = -2 3 = -1 4 = 0 |  | 5 = 1 6 = 2 7 = 3 8 = 4 65535 = None |

> 0x0076 | FaceDetect | int8u[2] |
> 0x0077 | FaceDetectFrameSize | int16u[2] |

> 0x0079

> ShadowCorrection

> int8u[n]

> 0 = Off 1 = On '0 0' = Off '1 1' = Weak |  | '1 2' = Normal '1 3' = Strong '2 4' = Auto |

> 0x007a | ISOAutoParameters | int8u[2] | '1 0' = Slow '2 0' = Standard '3 0' = Fast

> 0x007b

> CrossProcess

> int8u

> 0 = Off 1 = Random 2 = Preset 1 3 = Preset 2 |  | 4 = Preset 3 33 = Favorite 1 34 = Favorite 2 35 = Favorite 3 |

> 0x007d | LensCorr | - | --> Pentax LensCorr Tags

> 0x007f

> BleachBypassToning

> int16u

> 1 = Green 2 = Yellow 3 = Orange 4 = Red 5 = Magenta |  | 6 = Purple 7 = Blue 8 = Cyan 65535 = Off |

> 0x0080 | AspectRatio | Y | 0 = 4:3 1 = 3:2 2 = 16:9 3 = 1:1
> 0x0082 | BlurControl | int8u[4] | [Value 0] 0 = Off 1 = Low 2 = Medium 3 = High
> 0x0088 | NeutralDensityFilter | int8u | 0 = Off 1 = On
> 0x008b | ISO | int32u |
> 0x0200 | BlackPoint | int16u[4] |
> 0x0201 | WhitePoint | int16u[4] |
> 0x0203 | ColorMatrixA | int16s[9] |
> 0x0204 | ColorMatrixB | int16s[9] |
> 0x0205 | CameraSettings CameraSettingsUnknown | - - | --> Pentax CameraSettings Tags --> Pentax CameraSettingsUnknown Tags
> 0x0206 | AEInfo AEInfo2 AEInfo3 AEInfoUnknown | - - - - | --> Pentax AEInfo Tags --> Pentax AEInfo2 Tags --> Pentax AEInfo3 Tags --> Pentax AEInfoUnknown Tags
> 0x0207 | LensInfo | - | --> Pentax LensInfo Tags --> Pentax LensInfo2 Tags --> Pentax LensInfo3 Tags --> Pentax LensInfo4 Tags --> Pentax LensInfo5 Tags
> 0x0208 | FlashInfo FlashInfoUnknown | - - | --> Pentax FlashInfo Tags --> Pentax FlashInfoUnknown Tags
> 0x0209 | AEMeteringSegments | int8u[n] | (measurements from each of the 16 AE metering segments for models such as the K10D, and 77 metering segments for models such as the K-5, converted to LV)
> 0x020a | FlashMeteringSegments | int8u[n] |
> 0x020b | SlaveFlashMeteringSegments | int8u[n] | (used in wireless control mode)
> 0x020d | WB_RGGBLevelsDaylight | int16u[4] |
> 0x020e | WB_RGGBLevelsShade | int16u[4] |
> 0x020f | WB_RGGBLevelsCloudy | int16u[4] |
> 0x0210 | WB_RGGBLevelsTungsten | int16u[4] |
> 0x0211 | WB_RGGBLevelsFluorescentD | int16u[4] |
> 0x0212 | WB_RGGBLevelsFluorescentN | int16u[4] |
> 0x0213 | WB_RGGBLevelsFluorescentW | int16u[4] |
> 0x0214 | WB_RGGBLevelsFlash | int16u[4] |
> 0x0215 | CameraInfo | - | --> Pentax CameraInfo Tags
> 0x0216 | BatteryInfo | - | --> Pentax BatteryInfo Tags
> 0x021b | SaturationInfo? | N | (only in PEF and DNG images)
> 0x021f | AFInfo | - | --> Pentax AFInfo Tags
> 0x0220 | HuffmanTable? | N | (found in K10D, K20D and K2000D PEF images)
> 0x0221 | KelvinWB | - | --> Pentax KelvinWB Tags
> 0x0222 | ColorInfo | - | --> Pentax ColorInfo Tags
> 0x0224 | EVStepInfo | - | --> Pentax EVStepInfo Tags
> 0x0226 | ShotInfo | - | --> Pentax ShotInfo Tags
> 0x0227 | FacePos | - | --> Pentax FacePos Tags
> 0x0228 | FaceSize | - | --> Pentax FaceSize Tags
> 0x0229 | SerialNumber | string | (left blank by some cameras)
> 0x022a | FilterInfo | - | --> Pentax FilterInfo Tags
> 0x022b | LevelInfo | - | --> Pentax LevelInfo Tags
> 0x022d | WBLevels | - | --> Pentax WBLevels Tags
> 0x022e | Artist | string |
> 0x022f | Copyright | string |
> 0x0230 | FirmwareVersion | string | (only in AVI videos)
> 0x0231 | ContrastDetectAFArea | int16u[4] | (AF area of the most recent contrast-detect focus operation. Coordinates are left, top, width and height in a 720x480 frame, with Y downwards)
> 0x0235 | CrossProcessParams | undef[10] |
> 0x0239 | LensInfoQ | - | --> Pentax LensInfoQ Tags
> 0x03fe | DataDump | N |
> 0x03ff | TempInfoK5 UnknownInfo | - - | --> Pentax TempInfoK5 Tags --> Pentax UnknownInfo Tags
> 0x0402 | ToneCurve | Y~ |
> 0x0403 | ToneCurves | Y~ |
> 0x0405 | UnknownBlock? | undef | (large unknown data block in PEF/DNG images but not JPG images)
> 0x0e00 | PrintIM | - | --> PrintIM Tags

## Pentax PentaxModelID Values

> Value | PentaxModelID | Value | PentaxModelID | Value | PentaxModelID
> --- | --- | --- | --- | --- | ---
> 0xd | = Optio 330/430 | 0x12b9c | = K100D | 0x12d72 | = K2000
> 0x12926 | = Optio 230 | 0x12b9d | = K110D | 0x12d73 | = K-m
> 0x12958 | = Optio 330GS | 0x12ba2 | = K100D Super | 0x12d86 | = Optio P70
> 0x12962 | = Optio 450/550 | 0x12bb0 | = Optio T10/T20 | 0x12d90 | = Optio L70
> 0x1296c | = Optio S | 0x12be2 | = Optio W10 | 0x12d9a | = Optio E70
> 0x12971 | = Optio S V1.01 | 0x12bf6 | = Optio M10 | 0x12dae | = X70
> 0x12994 | = *ist D | 0x12c1e | = K10D | 0x12db8 | = K-7
> 0x129b2 | = Optio 33L | 0x12c20 | = Samsung GX10 | 0x12dcc | = Optio W80
> 0x129bc | = Optio 33LF | 0x12c28 | = Optio S7 | 0x12dea | = Optio P80
> 0x129c6 | = Optio 33WR/43WR/555 | 0x12c2d | = Optio L20 | 0x12df4 | = Optio WS80
> 0x129d5 | = Optio S4 | 0x12c32 | = Optio M20 | 0x12dfe | = K-x
> 0x12a02 | = Optio MX | 0x12c3c | = Optio W20 | 0x12e08 | = 645D
> 0x12a0c | = Optio S40 | 0x12c46 | = Optio A20 | 0x12e12 | = Optio E80
> 0x12a16 | = Optio S4i | 0x12c78 | = Optio E30 | 0x12e30 | = Optio W90
> 0x12a34 | = Optio 30 | 0x12c7d | = Optio E35 | 0x12e3a | = Optio I-10
> 0x12a52 | = Optio S30 | 0x12c82 | = Optio T30 | 0x12e44 | = Optio H90
> 0x12a66 | = Optio 750Z | 0x12c8c | = Optio M30 | 0x12e4e | = Optio E90
> 0x12a70 | = Optio SV | 0x12c91 | = Optio L30 | 0x12e58 | = X90
> 0x12a75 | = Optio SVi | 0x12c96 | = Optio W30 | 0x12e6c | = K-r
> 0x12a7a | = Optio X | 0x12ca0 | = Optio A30 | 0x12e76 | = K-5
> 0x12a8e | = Optio S5i | 0x12cb4 | = Optio E40 | 0x12e8a | = Optio RS1000 / RS1500
> 0x12a98 | = Optio S50 | 0x12cbe | = Optio M40 | 0x12e94 | = Optio RZ10
> 0x12aa2 | = *ist DS | 0x12cc3 | = Optio L40 | 0x12e9e | = Optio LS1000
> 0x12ab6 | = Optio MX4 | 0x12cc5 | = Optio L36 | 0x12ebc | = Optio WG-1 GPS
> 0x12ac0 | = Optio S5n | 0x12cc8 | = Optio Z10 | 0x12ed0 | = Optio S1
> 0x12aca | = Optio WP | 0x12cd2 | = K20D | 0x12ee4 | = Q
> 0x12afc | = Optio S55 | 0x12cd4 | = Samsung GX20 | 0x12ef8 | = K-01
> 0x12b10 | = Optio S5z | 0x12cdc | = Optio S10 | 0x12f0c | = Optio RZ18
> 0x12b1a | = *ist DL | 0x12ce6 | = Optio A40 | 0x12f16 | = Optio VS20
> 0x12b24 | = Optio S60 | 0x12cf0 | = Optio V10 | 0x12f2a | = Optio WG-2 GPS
> 0x12b2e | = Optio S45 | 0x12cfa | = K200D | 0x12f48 | = Optio LS465
> 0x12b38 | = Optio S6 | 0x12d04 | = Optio S12 | 0x12f52 | = K-30
> 0x12b4c | = Optio WPi | 0x12d0e | = Optio E50 | 0x12f5c | = X-5
> 0x12b56 | = BenQ DC X600 | 0x12d18 | = Optio M50 | 0x12f66 | = Q10
> 0x12b60 | = *ist DS2 | 0x12d22 | = Optio L50 | 0x12f70 | = K-5 II
> 0x12b62 | = Samsung GX-1S | 0x12d2c | = Optio V20 | 0x12f71 | = K-5 II s
> 0x12b6a | = Optio A10 | 0x12d40 | = Optio W60 | 0x12f84 | = MX-1
> 0x12b7e | = *ist DL2 | 0x12d4a | = Optio M60 |  |
> 0x12b80 | = Samsung GX-1L | 0x12d68 | = Optio E60/M90 |  |

## Pentax City Values

> Value | City | Value | City | Value | City | Value | City | Value | City
> --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
> 0 | = Pago Pago | 15 | = Halifax | 30 | = Jeddah | 45 | = Phnom Penh | 60 | = Wellington
> 1 | = Honolulu | 16 | = Buenos Aires | 31 | = Tehran | 46 | = Ho Chi Minh | 61 | = Auckland
> 2 | = Anchorage | 17 | = Sao Paulo | 32 | = Dubai | 47 | = Jakarta | 62 | = Lima
> 3 | = Vancouver | 18 | = Rio de Janeiro | 33 | = Karachi | 48 | = Hong Kong | 63 | = Dakar
> 4 | = San Francisco | 19 | = Madrid | 34 | = Kabul | 49 | = Perth | 64 | = Algiers
> 5 | = Los Angeles | 20 | = London | 35 | = Male | 50 | = Beijing | 65 | = Helsinki
> 6 | = Calgary | 21 | = Paris | 36 | = Delhi | 51 | = Shanghai | 66 | = Athens
> 7 | = Denver | 22 | = Milan | 37 | = Colombo | 52 | = Manila | 67 | = Nairobi
> 8 | = Mexico City | 23 | = Rome | 38 | = Kathmandu | 53 | = Taipei | 68 | = Amsterdam
> 9 | = Chicago | 24 | = Berlin | 39 | = Dacca | 54 | = Seoul | 69 | = Stockholm
> 10 | = Miami | 25 | = Johannesburg | 40 | = Yangon | 55 | = Adelaide | 70 | = Lisbon
> 11 | = Toronto | 26 | = Istanbul | 41 | = Bangkok | 56 | = Tokyo | 71 | = Copenhagen
> 12 | = New York | 27 | = Cairo | 42 | = Kuala Lumpur | 57 | = Guam | 72 | = Warsaw
> 13 | = Santiago | 28 | = Jerusalem | 43 | = Vientiane | 58 | = Sydney | 73 | = Prague
> 14 | = Caracus | 29 | = Moscow | 44 | = Singapore | 59 | = Noumea | 74 | = Budapest

## Pentax LensRec Tags

This record stores the LensType, plus one or two unknown bytes for some models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensType | int8u[2] | --> Pentax LensType Values

## Pentax LensType Values

The first number gives the series of the lens, and the second identifies the lens model. Note that newer series numbers may not always be properly identified by cameras running older firmware versions. Decimal values have been added to differentiate lenses which would otherwise have the same LensType, and are used by the Composite LensID tag when attempting to identify the specific lens model.

> Value | LensType
> --- | ---
> '0 0' | = M-42 or No Lens
> '1 0' | = K or M Lens
> '2 0' | = A Series Lens
> '3 0' | = Sigma
> '3 17' | = smc PENTAX-FA SOFT 85mm F2.8
> '3 18' | = smc PENTAX-F 1.7X AF ADAPTER
> '3 19' | = smc PENTAX-F 24-50mm F4
> '3 20' | = smc PENTAX-F 35-80mm F4-5.6
> '3 21' | = smc PENTAX-F 80-200mm F4.7-5.6
> '3 22' | = smc PENTAX-F FISH-EYE 17-28mm F3.5-4.5
> '3 23' | = smc PENTAX-F 100-300mm F4.5-5.6 or Sigma Lens
> '3 23.1' | = Sigma AF 28-300mm F3.5-5.6 DL IF
> '3 23.2' | = Sigma AF 28-300mm F3.5-6.3 DG IF Macro
> '3 24' | = smc PENTAX-F 35-135mm F3.5-4.5
> '3 25' | = smc PENTAX-F 35-105mm F4-5.6 or Sigma or Tokina Lens
> '3 25.1' | = Sigma AF 28-300mm F3.5-5.6 DL IF
> '3 25.2' | = Sigma 55-200mm F4-5.6 DC
> '3 25.3' | = Sigma AF 28-300mm F3.5-5.6 DL IF
> '3 25.4' | = Sigma AF 28-300mm F3.5-6.3 DG IF Macro
> '3 25.5' | = Tokina 80-200mm F2.8 ATX-Pro
> '3 26' | = smc PENTAX-F* 250-600mm F5.6 ED[IF]
> '3 27' | = smc PENTAX-F 28-80mm F3.5-4.5 or Tokina Lens
> '3 27.1' | = Tokina AT-X Pro AF 28-70mm F2.6-2.8
> '3 28' | = smc PENTAX-F 35-70mm F3.5-4.5 or Tokina Lens
> '3 28.1' | = Tokina 19-35mm F3.5-4.5 AF
> '3 28.2' | = Tokina AT-X AF 400mm F5.6
> '3 29' | = PENTAX-F 28-80mm F3.5-4.5 or Sigma or Tokina Lens
> '3 29.1' | = Sigma AF 18-125mm F3.5-5.6 DC
> '3 29.2' | = Tokina AT-X PRO 28-70mm F2.6-2.8
> '3 30' | = PENTAX-F 70-200mm F4-5.6
> '3 31' | = smc PENTAX-F 70-210mm F4-5.6 or Tokina or Takumar Lens
> '3 31.1' | = Tokina AF 730 75-300mm F4.5-5.6
> '3 31.2' | = Takumar-F 70-210mm F4-5.6
> '3 32' | = smc PENTAX-F 50mm F1.4
> '3 33' | = smc PENTAX-F 50mm F1.7
> '3 34' | = smc PENTAX-F 135mm F2.8 [IF]
> '3 35' | = smc PENTAX-F 28mm F2.8
> '3 36' | = Sigma 20mm F1.8 EX DG Aspherical RF
> '3 38' | = smc PENTAX-F* 300mm F4.5 ED[IF]
> '3 39' | = smc PENTAX-F* 600mm F4 ED[IF]
> '3 40' | = smc PENTAX-F Macro 100mm F2.8
> '3 41' | = smc PENTAX-F Macro 50mm F2.8 or Sigma Lens
> '3 41.1' | = Sigma 50mm F2.8 Macro
> '3 44' | = Sigma or Tamron Lens (3 44)
> '3 44.1' | = Sigma AF 10-20mm F4-5.6 EX DC
> '3 44.2' | = Sigma 12-24mm F4.5 EX DG
> '3 44.3' | = Sigma 17-70mm F2.8-4.5 DC Macro
> '3 44.4' | = Sigma 18-50mm F3.5-5.6 DC
> '3 44.5' | = Tamron 35-90mm F4 AF
> '3 46' | = Sigma Lens (3 46)
> '3 46.1' | = Sigma APO 70-200mm F2.8 EX
> '3 46.2' | = Sigma EX APO 100-300mm F4 IF
> '3 50' | = smc PENTAX-FA 28-70mm F4 AL
> '3 51' | = Sigma 28mm F1.8 EX DG Aspherical Macro
> '3 52' | = smc PENTAX-FA 28-200mm F3.8-5.6 AL[IF] or Tamron Lens
> '3 52.1' | = Tamron AF LD 28-200mm F3.8-5.6 [IF] Aspherical (171D)
> '3 53' | = smc PENTAX-FA 28-80mm F3.5-5.6 AL
> '3 247' | = smc PENTAX-DA FISH-EYE 10-17mm F3.5-4.5 ED[IF]
> '3 248' | = smc PENTAX-DA 12-24mm F4 ED AL[IF]
> '3 250' | = smc PENTAX-DA 50-200mm F4-5.6 ED
> '3 251' | = smc PENTAX-DA 40mm F2.8 Limited
> '3 252' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL
> '3 253' | = smc PENTAX-DA 14mm F2.8 ED[IF]
> '3 254' | = smc PENTAX-DA 16-45mm F4 ED AL
> '3 255' | = Sigma Lens (3 255)
> '3 255.1' | = Sigma 18-200mm F3.5-6.3 DC
> '3 255.2' | = Sigma DL-II 35-80mm F4-5.6
> '3 255.3' | = Sigma DL Zoom 75-300mm F4-5.6
> '3 255.4' | = Sigma DF EX Aspherical 28-70mm F2.8
> '3 255.5' | = Sigma AF Tele 400mm F5.6 Multi-coated
> '3 255.6' | = Sigma 24-60mm F2.8 EX DG
> '3 255.7' | = Sigma 70-300mm F4-5.6 Macro
> '3 255.8' | = Sigma 55-200mm F4-5.6 DC
> '3 255.9' | = Sigma 18-50mm F2.8 EX DC
> '4 1' | = smc PENTAX-FA SOFT 28mm F2.8
> '4 2' | = smc PENTAX-FA 80-320mm F4.5-5.6
> '4 3' | = smc PENTAX-FA 43mm F1.9 Limited
> '4 6' | = smc PENTAX-FA 35-80mm F4-5.6
> '4 12' | = smc PENTAX-FA 50mm F1.4
> '4 15' | = smc PENTAX-FA 28-105mm F4-5.6 [IF]
> '4 16' | = Tamron AF 80-210mm F4-5.6 (178D)
> '4 19' | = Tamron SP AF 90mm F2.8 (172E)
> '4 20' | = smc PENTAX-FA 28-80mm F3.5-5.6
> '4 21' | = Cosina AF 100-300mm F5.6-6.7
> '4 22' | = Tokina 28-80mm F3.5-5.6
> '4 23' | = smc PENTAX-FA 20-35mm F4 AL
> '4 24' | = smc PENTAX-FA 77mm F1.8 Limited
> '4 25' | = Tamron SP AF 14mm F2.8
> '4 26' | = smc PENTAX-FA Macro 100mm F3.5 or Cosina Lens
> '4 26.1' | = Cosina 100mm F3.5 Macro
> '4 27' | = Tamron AF 28-300mm F3.5-6.3 LD Aspherical[IF] Macro (185D/285D)
> '4 28' | = smc PENTAX-FA 35mm F2 AL
> '4 29' | = Tamron AF 28-200mm F3.8-5.6 LD Super II Macro (371D)
> '4 34' | = smc PENTAX-FA 24-90mm F3.5-4.5 AL[IF]
> '4 35' | = smc PENTAX-FA 100-300mm F4.7-5.8
> '4 36' | = Tamron AF70-300mm F4-5.6 LD Macro
> '4 37' | = Tamron SP AF 24-135mm F3.5-5.6 AD AL (190D)
> '4 38' | = smc PENTAX-FA 28-105mm F3.2-4.5 AL[IF]
> '4 39' | = smc PENTAX-FA 31mm F1.8 AL Limited
> '4 41' | = Tamron AF 28-200mm Super Zoom F3.8-5.6 Aspherical XR [IF] Macro (A03)
> '4 43' | = smc PENTAX-FA 28-90mm F3.5-5.6
> '4 44' | = smc PENTAX-FA J 75-300mm F4.5-5.8 AL
> '4 45' | = Tamron Lens (4 45)
> '4 45.1' | = Tamron 28-300mm F3.5-6.3 Ultra zoom XR
> '4 45.2' | = Tamron AF 28-300mm F3.5-6.3 XR Di LD Aspherical [IF] Macro
> '4 46' | = smc PENTAX-FA J 28-80mm F3.5-5.6 AL
> '4 47' | = smc PENTAX-FA J 18-35mm F4-5.6 AL
> '4 49' | = Tamron SP AF 28-75mm F2.8 XR Di (A09)
> '4 51' | = smc PENTAX-D FA 50mm F2.8 Macro
> '4 52' | = smc PENTAX-D FA 100mm F2.8 Macro
> '4 56' | = Samsung D-XENON 100mm F2.8 Macro
> '4 75' | = Tamron SP AF 70-200mm F2.8 Di LD [IF] Macro (A001)
> '4 214' | = smc PENTAX-DA 35mm F2.4 AL
> '4 229' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL II
> '4 230' | = Tamron SP AF 17-50mm F2.8 XR Di II
> '4 231' | = smc PENTAX-DA 18-250mm F3.5-6.3 ED AL [IF]
> '4 237' | = Samsung/Schneider D-XENOGON 10-17mm F3.5-4.5
> '4 239' | = Samsung D-XENON 12-24mm F4 ED AL [IF]
> '4 242' | = smc PENTAX-DA* 16-50mm F2.8 ED AL [IF] SDM (SDM unused)
> '4 243' | = smc PENTAX-DA 70mm F2.4 Limited
> '4 244' | = smc PENTAX-DA 21mm F3.2 AL Limited
> '4 245' | = Schneider D-XENON 50-200mm F4-5.6
> '4 246' | = Schneider D-XENON 18-55mm F3.5-5.6
> '4 247' | = smc PENTAX-DA FISH-EYE 10-17mm F3.5-4.5 ED[IF]
> '4 248' | = smc PENTAX-DA 12-24mm F4 ED AL [IF]
> '4 249' | = Tamron XR DiII 18-200mm F3.5-6.3 (A14)
> '4 250' | = smc PENTAX-DA 50-200mm F4-5.6 ED
> '4 251' | = smc PENTAX-DA 40mm F2.8 Limited
> '4 252' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL
> '4 253' | = smc PENTAX-DA 14mm F2.8 ED[IF]
> '4 254' | = smc PENTAX-DA 16-45mm F4 ED AL
> '5 1' | = smc PENTAX-FA* 24mm F2 AL[IF]
> '5 2' | = smc PENTAX-FA 28mm F2.8 AL
> '5 3' | = smc PENTAX-FA 50mm F1.7
> '5 4' | = smc PENTAX-FA 50mm F1.4
> '5 5' | = smc PENTAX-FA* 600mm F4 ED[IF]
> '5 6' | = smc PENTAX-FA* 300mm F4.5 ED[IF]
> '5 7' | = smc PENTAX-FA 135mm F2.8 [IF]
> '5 8' | = smc PENTAX-FA Macro 50mm F2.8
> '5 9' | = smc PENTAX-FA Macro 100mm F2.8
> '5 10' | = smc PENTAX-FA* 85mm F1.4 [IF]
> '5 11' | = smc PENTAX-FA* 200mm F2.8 ED[IF]
> '5 12' | = smc PENTAX-FA 28-80mm F3.5-4.7
> '5 13' | = smc PENTAX-FA 70-200mm F4-5.6
> '5 14' | = smc PENTAX-FA* 250-600mm F5.6 ED[IF]
> '5 15' | = smc PENTAX-FA 28-105mm F4-5.6
> '5 16' | = smc PENTAX-FA 100-300mm F4.5-5.6
> '5 98' | = smc PENTAX-FA 100-300mm F4.5-5.6
> '6 1' | = smc PENTAX-FA* 85mm F1.4 [IF]
> '6 2' | = smc PENTAX-FA* 200mm F2.8 ED[IF]
> '6 3' | = smc PENTAX-FA* 300mm F2.8 ED[IF]
> '6 4' | = smc PENTAX-FA* 28-70mm F2.8 AL
> '6 5' | = smc PENTAX-FA* 80-200mm F2.8 ED[IF]
> '6 6' | = smc PENTAX-FA* 28-70mm F2.8 AL
> '6 7' | = smc PENTAX-FA* 80-200mm F2.8 ED[IF]
> '6 8' | = smc PENTAX-FA 28-70mm F4AL
> '6 9' | = smc PENTAX-FA 20mm F2.8
> '6 10' | = smc PENTAX-FA* 400mm F5.6 ED[IF]
> '6 13' | = smc PENTAX-FA* 400mm F5.6 ED[IF]
> '6 14' | = smc PENTAX-FA* Macro 200mm F4 ED[IF]
> '7 0' | = smc PENTAX-DA 21mm F3.2 AL Limited
> '7 58' | = smc PENTAX-D FA Macro 100mm F2.8 WR
> '7 75' | = Tamron SP AF 70-200mm F2.8 Di LD [IF] Macro (A001)
> '7 212' | = smc PENTAX-DA 50mm F1.8
> '7 213' | = smc PENTAX-DA 40mm F2.8 XS
> '7 214' | = smc PENTAX-DA 35mm F2.4 AL
> '7 216' | = smc PENTAX-DA L 55-300mm F4-5.8 ED
> '7 217' | = smc PENTAX-DA 50-200mm F4-5.6 ED WR
> '7 218' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL WR
> '7 220' | = Tamron SP AF 10-24mm F3.5-4.5 Di II LD Aspherical [IF]
> '7 221' | = smc PENTAX-DA L 50-200mm F4-5.6 ED
> '7 222' | = smc PENTAX-DA L 18-55mm F3.5-5.6
> '7 223' | = Samsung D-XENON 18-55mm F3.5-5.6 II
> '7 224' | = smc PENTAX-DA 15mm F4 ED AL Limited
> '7 225' | = Samsung D-XENON 18-250mm F3.5-6.3
> '7 226' | = smc PENTAX-DA* 55mm F1.4 SDM (SDM unused)
> '7 227' | = smc PENTAX-DA* 60-250mm F4 [IF] SDM (SDM unused)
> '7 229' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL II
> '7 230' | = Tamron AF 17-50mm F2.8 XR Di-II LD (Model A16)
> '7 231' | = smc PENTAX-DA 18-250mm F3.5-6.3 ED AL [IF]
> '7 233' | = smc PENTAX-DA 35mm F2.8 Macro Limited
> '7 234' | = smc PENTAX-DA* 300mm F4 ED [IF] SDM (SDM unused)
> '7 235' | = smc PENTAX-DA* 200mm F2.8 ED [IF] SDM (SDM unused)
> '7 236' | = smc PENTAX-DA 55-300mm F4-5.8 ED
> '7 238' | = Tamron AF 18-250mm F3.5-6.3 Di II LD Aspherical [IF] Macro
> '7 241' | = smc PENTAX-DA* 50-135mm F2.8 ED [IF] SDM (SDM unused)
> '7 242' | = smc PENTAX-DA* 16-50mm F2.8 ED AL [IF] SDM (SDM unused)
> '7 243' | = smc PENTAX-DA 70mm F2.4 Limited
> '7 244' | = smc PENTAX-DA 21mm F3.2 AL Limited
> '8 4' | = Sigma 50mm F1.4 EX DG HSM
> '8 8' | = Sigma 18-250mm F3.5-6.3 DC OS HSM
> '8 11' | = Sigma 10-20mm F3.5 EX DC HSM
> '8 12' | = Sigma 70-300mm F4-5.6 DG OS
> '8 13' | = Sigma 120-400mm F4.5-5.6 APO DG OS HSM
> '8 14' | = Sigma 17-70mm F2.8-4.0 DC Macro OS HSM
> '8 15' | = Sigma 150-500mm F5-6.3 APO DG OS HSM
> '8 16' | = Sigma 70-200mm F2.8 EX DG Macro HSM II
> '8 17' | = Sigma 50-500mm F4.5-6.3 DG OS HSM
> '8 18' | = Sigma 8-16mm F4.5-5.6 DC HSM
> '8 21' | = Sigma 17-50mm F2.8 EX DC OS HSM
> '8 22' | = Sigma 85mm F1.4 EX DG HSM
> '8 23' | = Sigma 70-200mm F2.8 APO EX DG OS HSM
> '8 27' | = Sigma 18-200mm F3.5-6.3 II DC HSM
> '8 28' | = Sigma 18-250mm F3.5-6.3 DC Macro HSM
> '8 210' | = smc PENTAX-DA 18-270mm F3.5-6.3 ED SDM
> '8 211' | = HD PENTAX-DA 560mm F5.6 ED AW
> '8 215' | = smc PENTAX-DA 18-135mm F3.5-5.6 ED AL [IF] DC WR
> '8 226' | = smc PENTAX-DA* 55mm F1.4 SDM
> '8 227' | = smc PENTAX-DA* 60-250mm F4 [IF] SDM
> '8 232' | = smc PENTAX-DA 17-70mm F4 AL [IF] SDM
> '8 234' | = smc PENTAX-DA* 300mm F4 ED [IF] SDM
> '8 235' | = smc PENTAX-DA* 200mm F2.8 ED [IF] SDM
> '8 241' | = smc PENTAX-DA* 50-135mm F2.8 ED [IF] SDM
> '8 242' | = smc PENTAX-DA* 16-50mm F2.8 ED AL [IF] SDM
> '8 255' | = Sigma Lens (8 255)
> '8 255.1' | = Sigma 70-200mm F2.8 EX DG Macro HSM II
> '8 255.2' | = Sigma APO 150-500mm F5-6.3 DG OS HSM
> '8 255.3' | = Sigma 4.5mm F2.8 EX DC HSM Circular Fisheye
> '8 255.4' | = Sigma 50-200mm F4-5.6 DC OS
> '9 0' | = 645 Manual Lens
> '10 0' | = 645 A Series Lens
> '11 1' | = smc PENTAX-FA 645 75mm F2.8
> '11 2' | = smc PENTAX-FA 645 45mm F2.8
> '11 3' | = smc PENTAX-FA* 645 300mm F4 ED [IF]
> '11 4' | = smc PENTAX-FA 645 45-85mm F4.5
> '11 5' | = smc PENTAX-FA 645 400mm F5.6 ED [IF]
> '11 7' | = smc PENTAX-FA 645 Macro 120mm F4
> '11 8' | = smc PENTAX-FA 645 80-160mm F4.5
> '11 9' | = smc PENTAX-FA 645 200mm F4 [IF]
> '11 10' | = smc PENTAX-FA 645 150mm F2.8 [IF]
> '11 11' | = smc PENTAX-FA 645 35mm F3.5 AL [IF]
> '11 14' | = smc PENTAX-FA 645 55-110mm F5.6
> '11 16' | = smc PENTAX-FA 645 33-55mm F4.5 AL
> '11 17' | = smc PENTAX-FA 645 150-300mm F5.6 ED [IF]
> '13 18' | = smc PENTAX-D FA 645 55mm F2.8 AL [IF] SDM AW
> '13 19' | = smc PENTAX-D FA 645 25mm F4 AL [IF] SDM AW
> '13 20' | = HD PENTAX-D FA 645 90mm F2.8 ED AW SR
> '21 0' | = Pentax Q Manual Lens
> '21 1' | = 01 Standard Prime 8.5mm F1.9
> '21 2' | = 02 Standard Zoom 5-15mm F2.8-4.5
> '21 6' | = 06 Telephoto Zoom 15-45mm F2.8
> '22 3' | = 03 Fish-eye 3.2mm F5.6
> '22 4' | = 04 Toy Lens Wide 6.3mm F7.1
> '22 5' | = 05 Toy Lens Telephoto 18mm F8

## Pentax SRInfo Tags

Shake reduction information.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SRResult | int8u | 0x0 = Not stabilized Bit 0 = Stabilized Bit 6 = Not ready

> 1

> ShakeReduction

> int8u

> 0 = Off 1 = On 4 = Off (4) 5 = On but Disabled 6 = On (Video) |  | 7 = On (7) 15 = On (15) 39 = On (mode 2) 135 = On (135) 167 = On (mode 1) |

> 2 | SRHalfPressTime | int8u | (time from when the shutter button was half pressed to when the shutter was released, including time for focusing)
> 3 | SRFocalLength | int8u |

## Pentax FaceInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FacesDetected | int8u |
> 2 | FacePosition | int8u[2] | (X/Y coordinates of the center of the main face in percent of frame size, with positive Y downwards)

## Pentax AWBInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WhiteBalanceAutoAdjustment | int8u | 0 = Off 1 = On
> 1 | TungstenAWB | int8u | 0 = Subtle Correction 1 = Strong Correction

## Pentax TimeInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | WorldTimeLocation | int8u | [Mask 0x01] 0x0 = Hometown 0x1 = Destination
> 0.2 | HometownDST | int8u | [Mask 0x02] 0x0 = No 0x2 = Yes
> 0.3 | DestinationDST | int8u | [Mask 0x04] 0x0 = No 0x4 = Yes
> 2 | HometownCity | int8u | --> Pentax City Values
> 3 | DestinationCity | int8u | --> Pentax City Values

## Pentax LensCorr Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DistortionCorrection | int8u | 0 = Off 1 = On
> 1 | ChromaticAberrationCorrection | int8u | 0 = Off 1 = On

## Pentax CameraSettings Tags

Camera settings information written by Pentax DSLR cameras.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0

> PictureMode2

> int8u

> 0 = Scene Mode
> 1 = Auto PICT
> 2 = Program AE
> 3 = Green Mode
> 4 = Shutter Speed Priority
> 5 = Aperture Priority
> 6 = Program Tv Shift
> 7 = Program Av Shift
> 8 = Manual
> 9 = Bulb
> 10 = Aperture Priority, Off-Auto-Aperture
> 11 = Manual, Off-Auto-Aperture
> 12 = Bulb, Off-Auto-Aperture
> 13 = Shutter & Aperture Priority AE
> 15 = Sensitivity Priority AE
> 16 = Flash X-Sync Speed AE

> 1.1 | ProgramLine | int8u | [Mask 0x03] 0x0 = Normal 0x1 = Hi Speed 0x2 = Depth 0x3 = MTF
> 1.2 | EVSteps | int8u | [Mask 0x20] 0x0 = 1/2 EV Steps 0x20 = 1/3 EV Steps
> 1.3 | E-DialInProgram | int8u | [Mask 0x40] 0x0 = Tv or Av 0x40 = P Shift
> 1.4 | ApertureRingUse | int8u | [Mask 0x80] 0x0 = Prohibited 0x80 = Permitted

> 2

> FlashOptions

> int8u

> (the camera flash options settings, set even if the flash is off)
> [Mask 0xf0]

> 0x0 = Normal
> 0x1 = Red-eye reduction
> 0x2 = Auto
> 0x3 = Auto, Red-eye reduction
> 0x5 = Wireless (Master)
> 0x6 = Wireless (Control)
> 0x8 = Slow-sync
> 0x9 = Slow-sync, Red-eye reduction
> 0xa = Trailing-curtain Sync

> 2.1 | MeteringMode2 | int8u | (may not be valid for some models, ie. *ist D) [Mask 0x0f] 0x0 = Multi-segment Bit 0 = Center-weighted average Bit 1 = Spot
> 3 | AFPointMode | int8u | [Mask 0xf0] 0x0 = Auto Bit 4 = Select Bit 5 = Fixed Center
> 3.1 | FocusMode2 | int8u | [Mask 0x0f] 0x0 = Manual 0x1 = AF-S 0x2 = AF-C 0x3 = AF-A

> 4

> AFPointSelected2

> int16u

> 0x0 = Auto
> Bit 0 = Upper-left
> Bit 1 = Top
> Bit 2 = Upper-right
> Bit 3 = Left
> Bit 4 = Mid-left

> Bit 5 = Center
> Bit 6 = Mid-right
> Bit 7 = Right
> Bit 8 = Lower-left
> Bit 9 = Bottom
> Bit 10 = Lower-right

> 6 | ISOFloor | int8u |

> 7

> DriveMode2

> int8u

> 0x0 = Single-frame
> Bit 0 = Continuous
> Bit 1 = Continuous (Lo)
> Bit 2 = Self-timer (12 s)
> Bit 3 = Self-timer (2 s)
> Bit 4 = Remote Control (3 s delay)
> Bit 5 = Remote Control
> Bit 6 = Exposure Bracket
> Bit 7 = Multiple Exposure

> 8

> ExposureBracketStepSize

> int8u

> 3 = 0.3 4 = 0.5 5 = 0.7 8 = 1.0 |  | 11 = 1.3 12 = 1.5 13 = 1.7 16 = 2.0 |

> 9

> BracketShotNumber

> int8u

> 0x0 = n/a 0x2 = 1 of 2 0x3 = 1 of 3 0x5 = 1 of 5 |  | 0x12 = 2 of 2 0x13 = 2 of 3 0x15 = 2 of 5 0x23 = 3 of 3 |  | 0x25 = 3 of 5 0x35 = 4 of 5 0x45 = 5 of 5 |

> 10

> WhiteBalanceSet

> int8u

> [Mask 0xf0]

> 0x0 = Auto
> 0x10 = Daylight
> 0x20 = Shade
> 0x30 = Cloudy
> 0x40 = Daylight Fluorescent
> 0x50 = Day White Fluorescent
> 0x60 = White Fluorescent
> 0x70 = Tungsten
> 0x80 = Flash
> 0x90 = Manual
> 0xc0 = Set Color Temperature 1
> 0xd0 = Set Color Temperature 2
> 0xe0 = Set Color Temperature 3

> 10.1 | MultipleExposureSet | int8u | [Mask 0x0f] 0x0 = Off 0x1 = On

> 13

> RawAndJpgRecording

> int8u

> (K10D only)

> 0x1 = JPEG (Best)
> 0x4 = RAW (PEF, Best)
> 0x5 = RAW+JPEG (PEF, Best)
> 0x8 = RAW (DNG, Best)
> 0x9 = RAW+JPEG (DNG, Best)
> 0x21 = JPEG (Better)
> 0x24 = RAW (PEF, Better)
> 0x25 = RAW+JPEG (PEF, Better)
> 0x28 = RAW (DNG, Better)
> 0x29 = RAW+JPEG (DNG, Better)
> 0x41 = JPEG (Good)
> 0x44 = RAW (PEF, Good)
> 0x45 = RAW+JPEG (PEF, Good)
> 0x48 = RAW (DNG, Good)
> 0x49 = RAW+JPEG (DNG, Good)

> 14.1 | JpgRecordedPixels | int8u | (K10D only) [Mask 0x03] 0x0 = 10 MP 0x1 = 6 MP 0x2 = 2 MP
> 14.2 | LinkAEToAFPoint | int8u | (K-5 only) [Mask 0x01] 0x0 = Off 0x1 = On
> 14.3 | SensitivitySteps | int8u | (K-5 only) [Mask 0x02] 0x0 = 1 EV Steps 0x2 = As EV Steps
> 14.4 | ISOAuto | int8u | (K-5 only) [Mask 0x04] 0x0 = Off 0x4 = On

> 16

> FlashOptions2

> int8u

> (K10D only; set even if the flash is off)
> [Mask 0xf0]

> 0x0 = Normal
> 0x10 = Red-eye reduction
> 0x20 = Auto
> 0x30 = Auto, Red-eye reduction
> 0x50 = Wireless (Master)
> 0x60 = Wireless (Control)
> 0x80 = Slow-sync
> 0x90 = Slow-sync, Red-eye reduction
> 0xa0 = Trailing-curtain Sync

> 16.1 | MeteringMode3 | int8u | (K10D only) [Mask 0x0f] 0x0 = Multi-segment Bit 0 = Center-weighted average Bit 1 = Spot
> 17.1 | SRActive | int8u | (K10D only; SR is active only when ShakeReduction is On, DriveMode is not Remote or Self-timer, and Internal/ExternalFlashMode is not "On, Wireless") [Mask 0x80] 0x0 = No 0x80 = Yes

> 17.2

> Rotation

> int8u

> (K10D only)
> [Mask 0x60]
> 0x0 = Horizontal (normal)
> 0x20 = Rotate 180
> 0x40 = Rotate 90 CW
> 0x60 = Rotate 270 CW

> 17.3 | ISOSetting | int8u | (K10D only) [Mask 0x04] 0x0 = Manual 0x4 = Auto
> 17.4 | SensitivitySteps | int8u | (K10D only) [Mask 0x02] 0x0 = 1 EV Steps 0x2 = As EV Steps
> 18 | TvExposureTimeSetting | int8u | (K10D only)
> 19 | AvApertureSetting | int8u | (K10D only)
> 20 | SvISOSetting | int8u | (K10D only)
> 21 | BaseExposureCompensation | int8u | (K10D only; exposure compensation without auto bracketing)

## Pentax CameraSettingsUnknown Tags

This information has not yet been decoded for models such as the K-01.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Pentax AEInfo Tags

Auto-exposure information for most Pentax models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AEExposureTime | int8u | (val = 24 * 2**((32-raw)/8))
> 1 | AEAperture | int8u | (val = 2**((raw-68)/16))
> 2 | AE_ISO | int8u | (val = 100 * 2**((raw-32)/8))
> 3 | AEXv | int8u | (val = (raw-64)/8)
> 4 | AEBXv | int8s | (val = raw / 8)
> 5 | AEMinExposureTime | int8u | (val = 24 * 2**((32-raw)/8))

> 6

> AEProgramMode

> int8u

> 0 = M, P or TAv
> 1 = Av, B or X
> 2 = Tv
> 3 = Sv or Green Mode
> 8 = Hi-speed Program
> 11 = Hi-speed Program (P-Shift)
> 16 = DOF Program
> 19 = DOF Program (P-Shift)
> 24 = MTF Program
> 27 = MTF Program (P-Shift)
> 35 = Standard
> 43 = Portrait
> 51 = Landscape
> 59 = Macro
> 67 = Sport

> 75 = Night Scene Portrait
> 83 = No Flash
> 91 = Night Scene
> 99 = Surf & Snow
> 104 = Night Snap
> 107 = Text
> 115 = Sunset
> 123 = Kids
> 131 = Pet
> 139 = Candlelight
> 144 = SCN
> 147 = Museum
> 160 = Program
> 184 = Shallow DOF Program
> 216 = HDR

> 7 | AEFlags? | N | Bit 3 = AE lock Bit 4 = Flash recommended? Bit 7 = Aperture wide open
> 8 | AEUnknown | N | (indices after this are incremented by 1 for some models)
> 9 | AEMaxAperture | int8u | (val = 2**((raw-68)/16))
> 10 | AEMaxAperture2 | int8u | (val = 2**((raw-68)/16))
> 11 | AEMinAperture | int8u | (val = 2**((raw-68)/16))
> 12 | AEMeteringMode | int8u | 0x0 = Multi-segment Bit 4 = Center-weighted average Bit 5 = Spot
> 14 | FlashExposureCompSet | int8s | (reports the camera setting, unlike tag 0x004d which reports 0 in Green mode or if flash was on but did not fire. Both this tag and 0x004d report the setting even if the flash is off)

## Pentax AEInfo2 Tags

Auto-exposure information for the K-01.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | AEExposureTime | int8u | (val = 24 * 2**((32-raw)/8))
> 3 | AEAperture | int8u | (val = 2**((raw-68)/16))
> 4 | AE_ISO | int8u | (val = 100 * 2**((raw-32)/8))
> 5 | AEXv | int8u | (val = (raw-64)/8)
> 6 | AEBXv | int8s | (val = raw / 8)
> 8 | AEError | int8s |

> 15

> SceneMode

> int8u

> 0 = Off
> 1 = HDR
> 4 = Auto PICT
> 5 = Portrait
> 6 = Landscape
> 7 = Macro
> 8 = Sport
> 9 = Night Scene Portrait
> 10 = No Flash
> 11 = Night Scene
> 12 = Surf & Snow
> 14 = Sunset

> 15 = Kids
> 16 = Pet
> 17 = Candlelight
> 18 = Museum
> 20 = Food
> 21 = Stage Lighting
> 22 = Night Snap
> 25 = Night Scene HDR
> 26 = Blue Sky
> 27 = Forest
> 29 = Backlight Silhouette

> 16 | AEMaxAperture | int8u | (val = 2**((raw-68)/16))
> 17 | AEMaxAperture2 | int8u | (val = 2**((raw-68)/16))
> 18 | AEMinAperture | int8u | (val = 2**((raw-68)/16))
> 19 | AEMinExposureTime | int8u | (val = 24 * 2**((32-raw)/8))

## Pentax AEInfo3 Tags

Auto-exposure information for the K-30

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 16 | AEExposureTime | int8u | (val = 24 * 2**((32-raw)/8))
> 17 | AEAperture | int8u | (val = 2**((raw-68)/16))
> 18 | AE_ISO | int8u | (val = 100 * 2**((raw-32)/8))
> 28 | AEMaxAperture | int8u | (val = 2**((raw-68)/16))
> 29 | AEMaxAperture2 | int8u | (val = 2**((raw-68)/16))
> 30 | AEMinAperture | int8u | (val = 2**((raw-68)/16))
> 31 | AEMinExposureTime | int8u | (val = 24 * 2**((32-raw)/8))

## Pentax AEInfoUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Pentax LensInfo Tags

Pentax lens information structure for models such as the *istD.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensType | int8u[2] | --> Pentax LensType Values
> 3 | LensData | - | --> Pentax LensData Tags

## Pentax LensInfo2 Tags

Pentax lens information structure for models such as the K10D and K20D.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensType | int8u[4] | --> Pentax LensType Values
> 4 | LensData | - | --> Pentax LensData Tags

## Pentax LensData Tags

Pentax lens data information. Some of these tags require interesting binary gymnastics to decode them into useful values.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AutoAperture | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 0.2 | MinAperture | int8u | [Mask 0x06] 0x0 = 22 0x2 = 32 0x4 = 45 0x6 = 16
> 0.3 | LensFStops | int8u | [Mask 0x70]
> 1 | LensKind? | int8u |
> 2 | LC1? | int8u |
> 3 | LC2? | int8u |
> 4 | LC3? | int8u |
> 5 | LC4? | int8u |
> 6 | LC5? | int8u |
> 7 | LC6? | int8u |
> 8 | LC7? | int8u |
> 9 | FocalLength | int8u |
> 10 | NominalMaxAperture | int8u | [Mask 0xf0]
> 10.1 | NominalMinAperture | int8u | [Mask 0x0f]
> 11 | LC10? | int8u |
> 12 | LC11? | int8u |
> 13 | LC12? | int8u |
> 14.1 | MaxAperture | int8u | (effective wide open aperture for current focal length. Not valid for K-5) [Mask 0x7f]
> 15 | LC14? | int8u |
> 16 | LC15? | int8u |

## Pentax LensInfo3 Tags

Pentax lens information structure for 645D.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | LensType | int8u[4] | --> Pentax LensType Values
> 13 | LensData | - | --> Pentax LensData Tags

## Pentax LensInfo4 Tags

Pentax lens information structure for models such as the K-5 and K-r.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | LensType | int8u[4] | --> Pentax LensType Values
> 12 | LensData | - | --> Pentax LensData Tags

## Pentax LensInfo5 Tags

Pentax lens information structure for the K-01.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | LensType | int8u[5] | --> Pentax LensType Values
> 15 | LensData | - | --> Pentax LensData Tags

## Pentax FlashInfo Tags

Flash information tags for the K10D, K20D and K200D.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0

> FlashStatus

> int8u

> 0x0 = Off
> 0x1 = Off (1)
> 0x2 = External, Did not fire
> 0x6 = External, Fired
> 0x8 = Internal, Did not fire (0x08)
> 0x9 = Internal, Did not fire
> 0xd = Internal, Fired

> 1

> InternalFlashMode

> int8u

> 0x0 = n/a - Off-Auto-Aperture
> 0x86 = Fired, Wireless (Control)
> 0x95 = Fired, Wireless (Master)
> 0xc0 = Fired
> 0xc1 = Fired, Red-eye reduction
> 0xc2 = Fired, Auto
> 0xc3 = Fired, Auto, Red-eye reduction
> 0xc6 = Fired, Wireless (Control), Fired normally not as control
> 0xc8 = Fired, Slow-sync
> 0xc9 = Fired, Slow-sync, Red-eye reduction
> 0xca = Fired, Trailing-curtain Sync
> 0xf0 = Did not fire, Normal
> 0xf1 = Did not fire, Red-eye reduction
> 0xf2 = Did not fire, Auto
> 0xf3 = Did not fire, Auto, Red-eye reduction
> 0xf4 = Did not fire, (Unknown 0xf4)
> 0xf5 = Did not fire, Wireless (Master)
> 0xf6 = Did not fire, Wireless (Control)
> 0xf8 = Did not fire, Slow-sync
> 0xf9 = Did not fire, Slow-sync, Red-eye reduction
> 0xfa = Did not fire, Trailing-curtain Sync

> 2

> ExternalFlashMode

> int8u

> 0x0 = n/a - Off-Auto-Aperture
> 0x3f = Off
> 0x40 = On, Auto
> 0xbf = On, Flash Problem
> 0xc0 = On, Manual
> 0xc4 = On, P-TTL Auto
> 0xc5 = On, Contrast-control Sync
> 0xc6 = On, High-speed Sync
> 0xcc = On, Wireless
> 0xcd = On, Wireless, High-speed Sync
> 0xf0 = Not Connected

> 3 | InternalFlashStrength | int8u | (saved from the most recent flash picture, on a scale of about 0 to 100)
> 4 | TTL_DA_AUp | int8u |
> 5 | TTL_DA_ADown | int8u |
> 6 | TTL_DA_BUp | int8u |
> 7 | TTL_DA_BDown | int8u |
> 24.1 | ExternalFlashGuideNumber | int8u | (val = 2**(raw/16 + 4), with a few exceptions) [Mask 0x1f]

> 25

> ExternalFlashExposureComp

> int8u

> 0 = n/a
> 144 = n/a (Manual Mode)
> 164 = -3.0
> 167 = -2.5
> 168 = -2.0
> 171 = -1.5

> 172 = -1.0
> 175 = -0.5
> 176 = 0.0
> 179 = 0.5
> 180 = 1.0

> 26 | ExternalFlashBounce | int8u | (saved from the most recent external flash picture) 0 = n/a 16 = Direct 48 = Bounce

## Pentax FlashInfoUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Pentax CameraInfo Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PentaxModelID | int32u | --> Pentax PentaxModelID Values
> 1 | ManufactureDate | int32u | (this value, and the values of the tags below, may change if the camera is serviced)
> 2 | ProductionCode | int32u[2] |
> 4 | InternalSerialNumber | int32u |

## Pentax BatteryInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | PowerSource | int8u | [Mask 0x0f] 0x2 = Body Battery 0x3 = Grip Battery 0x4 = External Power Supply

> 1.1

> BodyBatteryState

> int8u

> (*istD, K100D, K200D, K10D and K20D)
> [Mask 0xf0]
> 0x10 = Empty or Missing
> 0x20 = Almost Empty
> 0x30 = Running Low
> 0x40 = Full
> (K-5, K-7, K-r, K-x and 645D)
> [Mask 0xf0]
> 0x10 = Empty or Missing
> 0x20 = Almost Empty
> 0x30 = Running Low
> 0x40 = Close to Full
> 0x50 = Full
> (decoding unknown for other models)
> [Mask 0xf0]

> 1.2

> GripBatteryState
> GripBatteryState?

> int8u
> int8u

> (K10D and K20D)
> [Mask 0x0f]
> 0x1 = Empty or Missing
> 0x2 = Almost Empty
> 0x3 = Running Low
> 0x4 = Full
> (decoding unknown for other models)
> [Mask 0x0f]

> 2 | BodyBatteryADNoLoad BodyBatteryVoltage1 | int8u int16u | (roughly calibrated for K10D with a new Pentax battery)
> 3 | BodyBatteryADLoad | int8u | (roughly calibrated for K10D with a new Pentax battery)
> 4 | GripBatteryADNoLoad BodyBatteryVoltage2 | int8u int16u |
> 5 | GripBatteryADLoad | int8u |
> 6 | BodyBatteryVoltage3 | int16u | (K-5, K-r and 645D only)
> 8 | BodyBatteryVoltage4 | int16u | (K-5 and K-r only)

## Pentax AFInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0

> AFPointsUnknown1?

> int16u

> 0x777 = Central 9 points
> 0x7ff = All
> Bit 0 = Upper-left
> Bit 1 = Top
> Bit 2 = Upper-right
> Bit 3 = Left
> Bit 4 = Mid-left

> Bit 5 = Center
> Bit 6 = Mid-right
> Bit 7 = Right
> Bit 8 = Lower-left
> Bit 9 = Bottom
> Bit 10 = Lower-right

> 2

> AFPointsUnknown2?

> int16u

> 0x0 = Auto
> Bit 0 = Upper-left
> Bit 1 = Top
> Bit 2 = Upper-right
> Bit 3 = Left
> Bit 4 = Mid-left

> Bit 5 = Center
> Bit 6 = Mid-right
> Bit 7 = Right
> Bit 8 = Lower-left
> Bit 9 = Bottom
> Bit 10 = Lower-right

> 4 | AFPredictor | int16s |
> 6 | AFDefocus | int8u |
> 7 | AFIntegrationTime | int8u | (times less than 2 ms give a value of 0)

> 11

> AFPointsInFocus

> int8u

> (may report two points in focus even though a single AFPoint has been selected, in which case the selected AFPoint is the first reported)

> 0 = None
> 1 = Lower-left, Bottom
> 2 = Bottom
> 3 = Lower-right, Bottom
> 4 = Mid-left, Center
> 5 = Center (horizontal)
> 6 = Mid-right, Center
> 7 = Upper-left, Top
> 8 = Top
> 9 = Upper-right, Top
> 10 = Right

> 11 = Lower-left, Mid-left
> 12 = Upper-left, Mid-left
> 13 = Bottom, Center
> 14 = Top, Center
> 15 = Lower-right, Mid-right
> 16 = Upper-right, Mid-right
> 17 = Left
> 18 = Mid-left
> 19 = Center (vertical)
> 20 = Mid-right

## Pentax KelvinWB Tags

White balance Blue/Red gains as a function of color temperature.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | KelvinWB_Daylight | int16u[4] |
> 5 | KelvinWB_01 | int16u[4] |
> 9 | KelvinWB_02 | int16u[4] |
> 13 | KelvinWB_03 | int16u[4] |
> 17 | KelvinWB_04 | int16u[4] |
> 21 | KelvinWB_05 | int16u[4] |
> 25 | KelvinWB_06 | int16u[4] |
> 29 | KelvinWB_07 | int16u[4] |
> 33 | KelvinWB_08 | int16u[4] |
> 37 | KelvinWB_09 | int16u[4] |
> 41 | KelvinWB_10 | int16u[4] |
> 45 | KelvinWB_11 | int16u[4] |
> 49 | KelvinWB_12 | int16u[4] |
> 53 | KelvinWB_13 | int16u[4] |
> 57 | KelvinWB_14 | int16u[4] |
> 61 | KelvinWB_15 | int16u[4] |
> 65 | KelvinWB_16 | int16u[4] |

## Pentax ColorInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 16 | WBShiftAB | int8s | (positive is a shift toward blue)
> 17 | WBShiftGM | int8s | (positive is a shift toward green)

## Pentax EVStepInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | EVSteps | int8u | 0 = 1/2 EV Steps 1 = 1/3 EV Steps
> 1 | SensitivitySteps | int8u | 0 = 1 EV Steps 1 = As EV Steps

## Pentax ShotInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 1

> CameraOrientation

> int8u

> (K-5, K-7, K-r and K-x)

> 0x10 = Horizontal (normal)
> 0x20 = Rotate 180
> 0x30 = Rotate 90 CW
> 0x40 = Rotate 270 CW
> 0x50 = Upwards
> 0x60 = Downwards

## Pentax FacePos Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Face1Position | int16u[2] | (X/Y coordinates of face center in full-sized image)
> 2 | Face2Position | int16u[2] |
> 4 | Face3Position | int16u[2] |
> 6 | Face4Position | int16u[2] |
> 8 | Face5Position | int16u[2] |
> 10 | Face6Position | int16u[2] |
> 12 | Face7Position | int16u[2] |
> 14 | Face8Position | int16u[2] |
> 16 | Face9Position | int16u[2] |
> 18 | Face10Position | int16u[2] |
> 20 | Face11Position | int16u[2] |
> 22 | Face12Position | int16u[2] |
> 24 | Face13Position | int16u[2] |
> 26 | Face14Position | int16u[2] |
> 28 | Face15Position | int16u[2] |
> 30 | Face16Position | int16u[2] |
> 32 | Face17Position | int16u[2] |
> 34 | Face18Position | int16u[2] |
> 36 | Face19Position | int16u[2] |
> 38 | Face20Position | int16u[2] |
> 40 | Face21Position | int16u[2] |
> 42 | Face22Position | int16u[2] |
> 44 | Face23Position | int16u[2] |
> 46 | Face24Position | int16u[2] |
> 48 | Face25Position | int16u[2] |
> 50 | Face26Position | int16u[2] |
> 52 | Face27Position | int16u[2] |
> 54 | Face28Position | int16u[2] |
> 56 | Face29Position | int16u[2] |
> 58 | Face30Position | int16u[2] |
> 60 | Face31Position | int16u[2] |
> 62 | Face32Position | int16u[2] |

## Pentax FaceSize Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Face1Size | int16u[2] |
> 2 | Face2Size | int16u[2] |
> 4 | Face3Size | int16u[2] |
> 6 | Face4Size | int16u[2] |
> 8 | Face5Size | int16u[2] |
> 10 | Face6Size | int16u[2] |
> 12 | Face7Size | int16u[2] |
> 14 | Face8Size | int16u[2] |
> 16 | Face9Size | int16u[2] |
> 18 | Face10Size | int16u[2] |
> 20 | Face11Size | int16u[2] |
> 22 | Face12Size | int16u[2] |
> 24 | Face13Size | int16u[2] |
> 26 | Face14Size | int16u[2] |
> 28 | Face15Size | int16u[2] |
> 30 | Face16Size | int16u[2] |
> 32 | Face17Size | int16u[2] |
> 34 | Face18Size | int16u[2] |
> 36 | Face19Size | int16u[2] |
> 38 | Face20Size | int16u[2] |
> 40 | Face21Size | int16u[2] |
> 42 | Face22Size | int16u[2] |
> 44 | Face23Size | int16u[2] |
> 46 | Face24Size | int16u[2] |
> 48 | Face25Size | int16u[2] |
> 50 | Face26Size | int16u[2] |
> 52 | Face27Size | int16u[2] |
> 54 | Face28Size | int16u[2] |
> 56 | Face29Size | int16u[2] |
> 58 | Face30Size | int16u[2] |
> 60 | Face31Size | int16u[2] |
> 62 | Face32Size | int16u[2] |

## Pentax FilterInfo Tags

The parameters associated with each type of digital filter are unique, and these settings are also extracted with the DigitalFilter tag. Information is not extracted for filters that are "Off" unless the Unknown option is used.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SourceDirectoryIndex | int16u |
> 2 | SourceFileIndex | int16u |
> 5 | DigitalFilter01 | undef[17] | --> Pentax DigitalFilter Values
> 22 | DigitalFilter02 | undef[17] | --> Pentax DigitalFilter Values
> 39 | DigitalFilter03 | undef[17] | --> Pentax DigitalFilter Values
> 56 | DigitalFilter04 | undef[17] | --> Pentax DigitalFilter Values
> 73 | DigitalFilter05 | undef[17] | --> Pentax DigitalFilter Values
> 90 | DigitalFilter06 | undef[17] | --> Pentax DigitalFilter Values
> 107 | DigitalFilter07 | undef[17] | --> Pentax DigitalFilter Values
> 124 | DigitalFilter08 | undef[17] | --> Pentax DigitalFilter Values
> 141 | DigitalFilter09 | undef[17] | --> Pentax DigitalFilter Values
> 158 | DigitalFilter10 | undef[17] | --> Pentax DigitalFilter Values
> 175 | DigitalFilter11 | undef[17] | --> Pentax DigitalFilter Values
> 192 | DigitalFilter12 | undef[17] | --> Pentax DigitalFilter Values
> 209 | DigitalFilter13 | undef[17] | --> Pentax DigitalFilter Values
> 226 | DigitalFilter14 | undef[17] | --> Pentax DigitalFilter Values
> 243 | DigitalFilter15 | undef[17] | --> Pentax DigitalFilter Values
> 260 | DigitalFilter16 | undef[17] | --> Pentax DigitalFilter Values
> 277 | DigitalFilter17 | undef[17] | --> Pentax DigitalFilter Values
> 294 | DigitalFilter18 | undef[17] | --> Pentax DigitalFilter Values
> 311 | DigitalFilter19 | undef[17] | --> Pentax DigitalFilter Values
> 328 | DigitalFilter20 | undef[17] | --> Pentax DigitalFilter Values

## Pentax DigitalFilter Values

> Value | DigitalFilter | Value | DigitalFilter | Value | DigitalFilter
> --- | --- | --- | --- | --- | ---
> 0 | = Off | 7 | = Slim | 16 | = Miniature
> 1 | = Base Parameter Adjust | 9 | = Fisheye | 17 | = Starburst
> 2 | = Soft Focus | 10 | = Toy Camera | 18 | = Posterization
> 3 | = High Contrast | 11 | = Retro | 19 | = Sketch Filter
> 4 | = Color Filter | 12 | = Pastel | 20 | = Shading
> 5 | = Extract Color | 13 | = Water Color | 21 | = Invert Color
> 6 | = Monochrome | 14 | = HDR | 254 | = Custom Filter

## Pentax LevelInfo Tags

Tags decoded from the electronic level information.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0

> LevelOrientation

> int8s

> [Mask 0x0f]

> 1 = Horizontal (normal)
> 2 = Rotate 180
> 3 = Rotate 90 CW
> 4 = Rotate 270 CW
> 9 = Horizontal; Off Level
> 10 = Rotate 180; Off Level
> 11 = Rotate 90 CW; Off Level
> 12 = Rotate 270 CW; Off Level
> 13 = Upwards
> 14 = Downwards

> 0.1 | CompositionAdjust | int8s | [Mask 0xf0] 0x0 = Off 0x20 = Composition Adjust 0xa0 = Composition Adjust + Horizon Correction 0xc0 = Horizon Correction
> 1 | RollAngle | int8s | (degrees of clockwise camera rotation)
> 2 | PitchAngle | int8s | (degrees of upward camera tilt)
> 5 | CompositionAdjustX | int8s | (steps to the right, 1/16 mm per step)
> 6 | CompositionAdjustY | int8s | (steps up, 1/16 mm per step)
> 7 | CompositionAdjustRotation | int8s | (steps clockwise, 1/8 degree per step)

## Pentax WBLevels Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | WB_RGGBLevelsDaylight | int16u[4] |
> 11 | WB_RGGBLevelsShade | int16u[4] |
> 20 | WB_RGGBLevelsCloudy | int16u[4] |
> 29 | WB_RGGBLevelsTungsten | int16u[4] |
> 38 | WB_RGGBLevelsFluorescentD | int16u[4] |
> 47 | WB_RGGBLevelsFluorescentN | int16u[4] |
> 56 | WB_RGGBLevelsFluorescentW | int16u[4] |
> 65 | WB_RGGBLevelsFlash | int16u[4] |
> 74 | WB_RGGBLevelsFluorescentL | int16u[4] |
> 83 | WB_RGGBLevelsUnknown? | int16u[4] |
> 92 | WB_RGGBLevelsUserSelected | int16u[4] |

## Pentax LensInfoQ Tags

More lens information stored by the Pentax Q.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | LensModel | string[30] |
> 42 | LensInfo | string[20] |

## Pentax TempInfoK5 Tags

A number of additional temperature readings are extracted from this 256-byte binary-data block in images from the K-5. It is currently not known where the corresponding temperature sensors are located in the camera.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | CameraTemperature2 | int16s |
> 14 | CameraTemperature3 | int16s |
> 20 | CameraTemperature4 | int16s |
> 22 | CameraTemperature5 | int16s |

## Pentax UnknownInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Pentax Type2 Tags

These tags are used by the Pentax Optio 330 and 430, and are similar to the tags used by Casio.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | RecordingMode | int16u | 0 = Auto 1 = Night Scene 2 = Manual
> 0x0002 | Quality | int16u | 0 = Good 1 = Better 2 = Best
> 0x0003 | FocusMode | int16u | 2 = Custom 3 = Auto
> 0x0004 | FlashMode | int16u | 1 = Auto 2 = On 4 = Off 6 = Red-eye reduction

> 0x0007

> WhiteBalance

> int16u

> 0 = Auto 1 = Daylight 2 = Shade |  | 3 = Tungsten 4 = Fluorescent 5 = Manual |

> 0x000a | DigitalZoom | int32u |
> 0x000b | Sharpness | int16u | 0 = Normal 1 = Soft 2 = Hard
> 0x000c | Contrast | int16u | 0 = Normal 1 = Low 2 = High
> 0x000d | Saturation | int16u | 0 = Normal 1 = Low 2 = High

> 0x0014

> ISO

> int16u

> 10 = 100 16 = 200 50 = 50 |  | 100 = 100 200 = 200 400 = 400 |  | 800 = 800 1600 = 1600 3200 = 3200 |

> 0x0017 | ColorFilter | int16u | 1 = Full 2 = Black & White 3 = Sepia
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x1000 | HometownCityCode | undef[4] |
> 0x1001 | DestinationCityCode | undef[4] |

## Pentax Type4 Tags

The following few tags are extracted from the wealth of information available in maker notes of the Optio E20 and E25. These maker notes are stored as ASCII text in a format very similar to some HP models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'F/W Version' | FirmwareVersion | N |

## Pentax S1 Tags

Tags extracted from the maker notes of AVI videos from the Optio S1.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | MakerNoteVersion | undef[4] |

## Pentax PENT Tags

Tags found in the PENT atom of MOV videos from the Optio WG-2 GPS.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 26 | Model | N |
> 56 | ExposureTime | N |
> 60 | FNumber | N |
> 68 | ExposureCompensation | N |
> 84 | FocalLength | N |
> 113 | DateTime1 | N |
> 139 | DateTime2 | N |
> 167 | ISO | N |
> 199 | GPSVersionID | N |
> 207 | GPSLatitudeRef | N | 'N' = North 'S' = South
> 209 | GPSLatitude | N |
> 233 | GPSLongitudeRef | N | 'E' = East 'W' = West
> 235 | GPSLongitude | N |
> 259 | GPSAltitudeRef | N | 0 = Above Sea Level 1 = Below Sea Level
> 260 | GPSAltitude | N |
> 284 | GPSTimeStamp | N |
> 308 | GPSSatellites | N |
> 311 | GPSStatus | N | 'A' = Measurement Active 'V' = Measurement Void
> 313 | GPSMeasureMode | N | 2 = 2-Dimensional Measurement 3 = 3-Dimensional Measurement
> 315 | GPSMapDatum | N |
> 322 | GPSDateStamp | N |
> 371 | AudioCodecID | N |
> 2003 | PreviewImage | N | (640x480 JPEG preview image)

## Pentax PXTH Tags

Tags found in the PXTH atom of MOV videos from the K-01.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PreviewImageLength | N |
> 4 | PreviewImage | N | (640-pixel-wide JPEG preview)

## Pentax MOV Tags

This information is found in MOV videos from cameras such as the Optio WP.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 38 | ExposureTime | N |
> 42 | FNumber | N |
> 50 | ExposureCompensation | N |

> 68

> WhiteBalance

> N

> 0 = Auto 1 = Daylight 2 = Shade |  | 3 = Fluorescent 4 = Tungsten 5 = Manual |

> 72 | FocalLength | N |
> 175 | ISO | N |

## Pentax Junk Tags

Tags found in the JUNK chunk of AVI videos from the RS1000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | Model | N |

## Pentax Junk2 Tags

This information is found in AVI videos from the Optio RZ18.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 18 | Make | N |
> 44 | Model | N |
> 94 | FNumber | N |
> 131 | DateTime1 | N |
> 157 | DateTime2 | N |
> 299 | ThumbnailWidth | N |
> 301 | ThumbnailHeight | N |
> 303 | ThumbnailLength | N |
> 307 | ThumbnailImage | N | (160x120 JPEG thumbnail image)

## Pentax AVI Tags

Pentax-specific RIFF tags found in AVI videos.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'hymn' | MakerNotes | - | --> Pentax Tags

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised May 14, 2013

<-- ExifTool Tag Names