## PanasonicRaw Tags

These tags are found in IFD0 of Panasonic/Leica RAW, RW2 and RWL images.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | PanasonicRawVersion | undef |
> 0x0002 | SensorWidth | N |
> 0x0003 | SensorHeight | N |
> 0x0004 | SensorTopBorder | N |
> 0x0005 | SensorLeftBorder | N |
> 0x0006 | SensorBottomBorder | N |
> 0x0007 | SensorRightBorder | N |
> 0x0011 | RedBalance | int16u | (found in Digilux 2 RAW images)
> 0x0012 | BlueBalance | int16u |
> 0x0017 | ISO | int16u |
> 0x0024 | WBRedLevel | int16u |
> 0x0025 | WBGreenLevel | int16u |
> 0x0026 | WBBlueLevel | int16u |
> 0x002e | JpgFromRaw | undef! | --> JPEG Tags (processed as an embedded document because it contains full EXIF)
> 0x010f | Make | string |
> 0x0110 | Model | string |
> 0x0111 | StripOffsets | N |

> 0x0112

> Orientation

> int16u

> 1 = Horizontal (normal)
> 2 = Mirror horizontal
> 3 = Rotate 180
> 4 = Mirror vertical
> 5 = Mirror horizontal and rotate 270 CW
> 6 = Rotate 90 CW
> 7 = Mirror horizontal and rotate 90 CW
> 8 = Rotate 270 CW

> 0x0116 | RowsPerStrip | N |
> 0x0117 | StripByteCounts | N |
> 0x0118 | RawDataOffset | N |
> 0x0119 | DistortionInfo | - | --> PanasonicRaw DistortionInfo Tags
> 0x02bc | ApplicationNotes | int8u! | --> XMP Tags
> 0x83bb | IPTC-NAA | int32u! | --> IPTC Tags
> 0x8769 | ExifOffset | - | --> EXIF Tags
> 0x8825 | GPSInfo | - | --> GPS Tags

## PanasonicRaw DistortionInfo Tags

Lens distortion correction information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | DistortionParam02 | int16s |
> 0x0004 | DistortionParam04 | int16s |
> 0x0005 | DistortionScale | int16s |
> 7.1 | DistortionCorrection | int16s | [Mask 0x0f] 0x0 = Off 0x1 = On
> 0x0008 | DistortionParam08 | int16s |
> 0x0009 | DistortionParam09 | int16s |
> 0x000b | DistortionParam11 | int16s |
> 0x000c | DistortionN? | int16s |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Sep 6, 2012

<-- ExifTool Tag Names