## FLIR Tags

Information extracted from the maker notes of JPEG images from thermal imaging cameras by FLIR Systems Inc.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | ImageTemperatureMax | rational64u | (these temperatures may be in Celcius, Kelvin or Fahrenheit, but there is no way to tell which)
> 0x0002 | ImageTemperatureMin | rational64u |
> 0x0003 | Emissivity | rational64u |
> 0x0004 | UnknownTemperature? | rational64u |
> 0x0005 | CameraTemperatureRangeMax? | rational64u |
> 0x0006 | CameraTemperatureRangeMin? | rational64u |

## FLIR FFF Tags

Information extracted from FLIR FFF images and the FLIR APP1 segment of JPEG images.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | RawData | - | --> FLIR RawData Tags
> 0x000e | EmbeddedImage | - | --> FLIR EmbeddedImage Tags
> 0x0020 | CameraInfo | - | --> FLIR CameraInfo Tags
> 0x0022 | PaletteInfo | - | --> FLIR PaletteInfo Tags
> 0x0023 | TextInfo | - | --> FLIR TextInfo Tags
> 0x0024 | EmbeddedAudioFile | N |
> 0x002a | PiP | - | --> FLIR PiP Tags
> 0x002b | GPSInfo | - | --> FLIR GPSInfo Tags
> 0x002e | ParamInfo | - | --> FLIR ParamInfo Tags

## FLIR RawData Tags

The thermal image data may be stored either as raw data, or in PNG format. If stored as raw data, ExifTool adds a TIFF header to allow the data to be viewed as a TIFF image. If stored in PNG format, the PNG image is extracted as-is. Note that most FLIR cameras using the PNG format seem to write the 16-bit raw image data in the wrong byte order.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | RawThermalImageWidth | N |
> 2 | RawThermalImageHeight | N |
> 16 | RawThermalImageType | N | (TIFF or PNG)
> 16.1 | RawThermalImage | N |

## FLIR EmbeddedImage Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | EmbeddedImageWidth | N |
> 2 | EmbeddedImageHeight | N |
> 16 | EmbeddedImageType | N | ("PNG" for PNG image in Y Cb Cr colors, or "DAT" for other image data)
> 16.1 | EmbeddedImage | N |

## FLIR CameraInfo Tags

FLIR camera information. The Planck tags are variables used in the temperature calculation. See http://u88.n24.queensu.ca/exiftool/forum/index.php?topic=4898.msg23972#msg23972 for details.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 32 | Emissivity | N |
> 36 | ObjectDistance | N |
> 40 | ReflectedApparentTemperature | N |
> 44 | AtmosphericTemperature | N |
> 48 | IRWindowTemperature | N |
> 52 | IRWindowTransmission | N |
> 60 | RelativeHumidity | N |
> 88 | PlanckR1 | N |
> 92 | PlanckB | N |
> 96 | PlanckF | N |
> 144 | CameraTemperatureRangeMax | N |
> 148 | CameraTemperatureRangeMin | N |
> 152 | UnknownTemperature1? | N |
> 156 | UnknownTemperature2? | N |
> 160 | UnknownTemperature3? | N |
> 164 | UnknownTemperature4? | N |
> 168 | UnknownTemperature5? | N |
> 172 | UnknownTemperature6? | N |
> 212 | CameraModel | N |
> 244 | CameraPartNumber | N |
> 260 | CameraSerialNumber | N |
> 276 | CameraSoftware | N |
> 368 | LensModel | N |
> 400 | LensPartNumber | N |
> 416 | LensSerialNumber | N |
> 436 | FieldOfView | N |
> 492 | FilterModel | N |
> 508 | FilterPartNumber | N |
> 540 | FilterSerialNumber | N |
> 776 | PlanckO | N |
> 780 | PlanckR2 | N |
> 824 | RawValueMedian | N |
> 828 | RawValueRange | N |
> 900 | DateTimeOriginal | N |
> 912 | FocusStepCount | N |
> 1116 | FocusDistance | N |

## FLIR PaletteInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PaletteColors | N |
> 6 | AboveColor | N | (Y Cr Cb color components)
> 9 | BelowColor | N |
> 12 | OverflowColor | N |
> 15 | UnderflowColor | N |
> 18 | Isotherm1Color | N |
> 21 | Isotherm2Color | N |
> 26 | PaletteMethod | N |
> 27 | PaletteStretch | N |
> 48 | PaletteFileName | N |
> 80 | PaletteName | N |
> 112 | Palette | N | (Y Cr Cb byte values for each palette color)

## FLIR TextInfo Tags

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> Label0 | N |
> Label1 | N |
> Label2 | N |
> Label3 | N |
> Value0 | N |
> Value1 | N |
> Value2 | N |
> Value3 | N |

## FLIR PiP Tags

FLIR Picture in Picture tags.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Real2IR | N |
> 2 | OffsetX | N | (offset from of insertion point from center)
> 3 | OffsetY | N |
> 4 | PiPX1 | N | (crop size for radiometric image)
> 5 | PiPX2 | N |
> 6 | PiPY1 | N |
> 7 | PiPY2 | N |

## FLIR GPSInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 88 | GPSMapDatum | N |

## FLIR ParamInfo Tags

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> DateTimeGenerated | N |
> Param0 | N |
> Param1 | N |
> Param2 | N |
> Param3 | N |

## FLIR FPF Tags

Tags extracted from FLIR Public image Format (FPF) files.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 32 | FPFVersion | N |
> 36 | ImageDataOffset | N |
> 40 | ImageType | N | 0 = Temperature 1 = Temperature Difference 2 = Object Signal 3 = Object Signal Difference
> 42 | ImagePixelFormat | N | 0 = 2-byte short integer 1 = 4-byte long integer 2 = 4-byte float 3 = 8-byte double
> 44 | ImageWidth | N |
> 46 | ImageHeight | N |
> 48 | ExternalTriggerCount | N |
> 52 | SequenceFrameNumber | N |
> 120 | CameraModel | N |
> 152 | CameraPartNumber | N |
> 184 | CameraSerialNumber | N |
> 216 | CameraTemperatureRangeMin | N |
> 220 | CameraTemperatureRangeMax | N |
> 224 | LensModel | N |
> 256 | LensPartNumber | N |
> 288 | LensSerialNumber | N |
> 320 | FilterModel | N |
> 336 | FilterPartNumber | N |
> 384 | FilterSerialNumber | N |
> 480 | Emissivity | N |
> 484 | ObjectDistance | N |
> 488 | ReflectedApparentTemperature | N |
> 492 | AtmosphericTemperature | N |
> 496 | RelativeHumidity | N |
> 500 | ComputedAtmosphericTrans | N |
> 504 | EstimatedAtmosphericTrans | N |
> 508 | ReferenceTemperature | N |
> 512 | IRWindowTemperature | N |
> 516 | IRWindowTransmission | N |
> 584 | DateTimeOriginal | N |
> 676 | CameraScaleMin | N |
> 680 | CameraScaleMax | N |
> 684 | CalculatedScaleMin | N |
> 688 | CalculatedScaleMax | N |
> 692 | ActualScaleMin | N |
> 696 | ActualScaleMax | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised May 14, 2013

<-- ExifTool Tag Names