## Nikon Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MakerNoteVersion | undef[4] |
> 0x0002 | ISO | int16u[2] |
> 0x0003 | ColorMode | string |
> 0x0004 | Quality | string |
> 0x0005 | WhiteBalance | string |
> 0x0006 | Sharpness | string |
> 0x0007 | FocusMode | string |
> 0x0008 | FlashSetting | string |
> 0x0009 | FlashType | string |
> 0x000b | WhiteBalanceFineTune | int16s[n] |
> 0x000c | WB_RBLevels | rational64u[4] |
> 0x000d | ProgramShift | undef[4] |
> 0x000e | ExposureDifference | undef[4] |
> 0x000f | ISOSelection | string |
> 0x0010 | DataDump | N |
> 0x0011 | PreviewIFD | - | --> Nikon PreviewIFD Tags
> 0x0012 | FlashExposureComp | undef[4] | (may be set even if flash does not fire. Does not include the effect of flash bracketing.)
> 0x0013 | ISOSetting | int16u[2] |
> 0x0014 | ColorBalanceA NRWData? | - Y | --> Nikon ColorBalanceA Tags (large unknown block in NRW images, not copied to JPEG images)
> 0x0016 | ImageBoundary | int16u[4] |
> 0x0017 | ExternalFlashExposureComp | undef[4] |
> 0x0018 | FlashExposureBracketValue | undef[4] |
> 0x0019 | ExposureBracketValue | rational64s |
> 0x001a | ImageProcessing | string |
> 0x001b | CropHiSpeed | int16u[7]~ |
> 0x001c | ExposureTuning | undef[3] |
> 0x001d | SerialNumber | string! | (this value is used as a key to decrypt other information -- writing this tag causes the other information to be re-encrypted with the new key)
> 0x001e | ColorSpace | int16u | 1 = sRGB 2 = Adobe RGB
> 0x001f | VRInfo | - | --> Nikon VRInfo Tags
> 0x0020 | ImageAuthentication | int8u | 0 = Off 1 = On
> 0x0021 | FaceDetect | - | --> Nikon FaceDetect Tags

> 0x0022

> ActiveD-Lighting

> int16u

> 0 = Off 1 = Low 3 = Normal 5 = High 7 = Extra High |  | 8 = Extra High 1 9 = Extra High 2 10 = Extra High 3 11 = Extra High 4 65535 = Auto |

> 0x0023 | PictureControlData | undef! | --> Nikon PictureControl Tags
> 0x0024 | WorldTime | - | --> Nikon WorldTime Tags
> 0x0025 | ISOInfo | - | --> Nikon ISOInfo Tags
> 0x002a | VignetteControl | int16u | 0 = Off 1 = Low 3 = Normal 5 = High
> 0x002b | DistortInfo | - | --> Nikon DistortInfo Tags
> 0x002c | UnknownInfo | - | --> Nikon UnknownInfo Tags
> 0x0032 | UnknownInfo2 | - | --> Nikon UnknownInfo2 Tags
> 0x0035 | HDRInfo | - | --> Nikon HDRInfo Tags
> 0x0039 | LocationInfo | - | --> Nikon LocationInfo Tags
> 0x0080 | ImageAdjustment | string |
> 0x0081 | ToneComp | string |
> 0x0082 | AuxiliaryLens | string |
> 0x0083 | LensType | int8u | Bit 0 = MF Bit 1 = D Bit 2 = G Bit 3 = VR
> 0x0084 | Lens | rational64u[4] |
> 0x0085 | ManualFocusDistance | rational64u |
> 0x0086 | DigitalZoom | rational64u |

> 0x0087

> FlashMode

> int8u

> 0 = Did Not Fire
> 1 = Fired, Manual
> 3 = Not Ready
> 7 = Fired, External
> 8 = Fired, Commander Mode
> 9 = Fired, TTL Mode

> 0x0088 | AFInfo | - | --> Nikon AFInfo Tags --> Nikon AFInfo Tags

> 0x0089

> ShootingMode

> int16u~

> (for the D70, Bit 5 = Unused LE-NR Slowdown)
> Bit 0 = Continuous
> Bit 1 = Delay
> Bit 2 = PC Control
> Bit 4 = Exposure Bracketing
> Bit 5 = Auto ISO
> Bit 6 = White-Balance Bracketing
> Bit 7 = IR Control

> 0x008b | LensFStops | undef[4] |
> 0x008c | ContrastCurve | undef! |
> 0x008d | ColorHue | string |
> 0x008f | SceneMode | string |
> 0x0090 | LightSource | string |

> 0x0091

> ShotInfoD40
> ShotInfoD80
> ShotInfoD90
> ShotInfoD3a
> ShotInfoD3b
> ShotInfoD3X
> ShotInfoD3S
> ShotInfoD300a
> ShotInfoD300b
> ShotInfoD300S
> ShotInfoD700
> ShotInfoD800
> ShotInfoD5000
> ShotInfoD5100
> ShotInfoD5200
> ShotInfoD7000
> ShotInfo02xx
> ShotInfoUnknown

> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -
> -

> --> Nikon ShotInfoD40 Tags
> --> Nikon ShotInfoD80 Tags
> --> Nikon ShotInfoD90 Tags
> --> Nikon ShotInfoD3a Tags
> --> Nikon ShotInfoD3b Tags
> --> Nikon ShotInfoD3X Tags
> --> Nikon ShotInfoD3S Tags
> --> Nikon ShotInfoD300a Tags
> --> Nikon ShotInfoD300b Tags
> --> Nikon ShotInfoD300S Tags
> --> Nikon ShotInfoD700 Tags
> --> Nikon ShotInfoD800 Tags
> --> Nikon ShotInfoD5000 Tags
> --> Nikon ShotInfoD5100 Tags
> --> Nikon ShotInfoD5200 Tags
> --> Nikon ShotInfoD7000 Tags
> --> Nikon ShotInfo Tags
> --> Nikon ShotInfo Tags

> 0x0092 | HueAdjustment | int16s |
> 0x0093 | NEFCompression | int16u | 1 = Lossy (type 1) 2 = Uncompressed 3 = Lossless 4 = Lossy (type 2)
> 0x0094 | Saturation | int16s |
> 0x0095 | NoiseReduction | string |
> 0x0096 | NEFLinearizationTable | undef! |

> 0x0097

> ColorBalance0100
> ColorBalance0102
> ColorBalance0103
> ColorBalance0205
> ColorBalance0209
> ColorBalance02
> ColorBalance0211
> ColorBalance0213
> ColorBalance0215
> ColorBalanceUnknown

> -
> -
> -
> -
> -
> -
> -
> -
> -
> -

> --> Nikon ColorBalance1 Tags
> --> Nikon ColorBalance2 Tags
> --> Nikon ColorBalance3 Tags
> --> Nikon ColorBalance2 Tags
> --> Nikon ColorBalance4 Tags
> --> Nikon ColorBalance2 Tags
> --> Nikon ColorBalance4 Tags
> --> Nikon ColorBalance2 Tags
> --> Nikon ColorBalance4 Tags
> --> Nikon ColorBalanceUnknown Tags

> 0x0098

> LensData0100
> LensData0101
> LensData0201
> LensData0204
> LensData0400
> LensDataUnknown

> -
> -
> -
> -
> -
> -

> --> Nikon LensData00 Tags
> --> Nikon LensData01 Tags
> --> Nikon LensData01 Tags
> --> Nikon LensData0204 Tags
> --> Nikon LensData0400 Tags
> --> Nikon LensDataUnknown Tags

> 0x0099 | RawImageCenter | int16u[2] |
> 0x009a | SensorPixelSize | rational64u[2] |
> 0x009c | SceneAssist | string |

> 0x009e

> RetouchHistory

> int16u[10]

> [Values 0-9]

> 0 = None
> 3 = B & W
> 4 = Sepia
> 5 = Trim
> 6 = Small Picture
> 7 = D-Lighting
> 8 = Red Eye
> 9 = Cyanotype
> 10 = Sky Light
> 11 = Warm Tone
> 12 = Color Custom
> 13 = Image Overlay
> 14 = Red Intensifier
> 15 = Green Intensifier
> 16 = Blue Intensifier
> 17 = Cross Screen

> 18 = Quick Retouch
> 19 = NEF Processing
> 23 = Distortion Control
> 25 = Fisheye
> 26 = Straighten
> 29 = Perspective Control
> 30 = Color Outline
> 31 = Soft Filter
> 32 = Resize
> 33 = Miniature Effect
> 34 = Skin Softening
> 35 = Selected Frame
> 37 = Color Sketch
> 38 = Selective Color
> 40 = Drawing

> 0x00a0 | SerialNumber | string |
> 0x00a2 | ImageDataSize | int32u |
> 0x00a5 | ImageCount | int32u |
> 0x00a6 | DeletedImageCount | int32u |
> 0x00a7 | ShutterCount | int32u! | (this value is used as a key to decrypt other information -- writing this tag causes the other information to be re-encrypted with the new key)
> 0x00a8 | FlashInfo0100 FlashInfo0102 FlashInfo0103 FlashInfoUnknown | - - - - | --> Nikon FlashInfo0100 Tags --> Nikon FlashInfo0102 Tags --> Nikon FlashInfo0103 Tags --> Nikon FlashInfoUnknown Tags
> 0x00a9 | ImageOptimization | string |
> 0x00aa | Saturation | string |
> 0x00ab | VariProgram | string |
> 0x00ac | ImageStabilization | string |
> 0x00ad | AFResponse | string |
> 0x00b0 | MultiExposure | - | --> Nikon MultiExposure Tags

> 0x00b1

> HighISONoiseReduction

> int16u

> 0 = Off 1 = Minimal 2 = Low 3 = Medium Low |  | 4 = Normal 5 = Medium High 6 = High |

> 0x00b3 | ToningEffect | string |
> 0x00b6 | PowerUpTime | undef | (date/time when camera was last powered up)
> 0x00b7 | AFInfo2 | - | --> Nikon AFInfo2 Tags
> 0x00b8 | FileInfo | - | --> Nikon FileInfo Tags --> Nikon FileInfo Tags
> 0x00b9 | AFTune | - | --> Nikon AFTune Tags
> 0x00bd | PictureControlData | undef! | --> Nikon PictureControl Tags
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x0e01 | NikonCaptureData | undef! | --> NikonCapture Tags (this data is dropped when copying Nikon MakerNotes since it may be too large to fit in the EXIF segment of a JPEG image, but it may be copied as a block into existing Nikon MakerNotes later if desired)
> 0x0e09 | NikonCaptureVersion | string |
> 0x0e0e | NikonCaptureOffsets | - | --> Nikon CaptureOffsets Tags
> 0x0e10 | NikonScanIFD | - | --> Nikon Scan Tags
> 0x0e13 | NikonCaptureEditVersions NikonCaptureEditVersions | undef undef! | (the ExtractEmbedded option may be used to decode settings from the stored edit versions, otherwise this is extracted as a binary data block) --> NikonCapture Tags
> 0x0e1d | NikonICCProfile | undef! | --> ICC_Profile Tags
> 0x0e1e | NikonCaptureOutput | undef! | --> Nikon CaptureOutput Tags
> 0x0e22 | NEFBitDepth | int16u[4]! | '0 0 0 0' = n/a (JPEG) '8 8 8 0' = 8 x 3 '12 0 0 0' = 12 '14 0 0 0' = 14 '16 16 16 0' = 16 x 3

## Nikon PreviewIFD Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0x00fe

> SubfileType

> N

> 0x0 = Full-resolution Image
> 0x1 = Reduced-resolution image
> 0x2 = Single page of multi-page image
> 0x3 = Single page of multi-page reduced-resolution image
> 0x4 = Transparency mask
> 0x5 = Transparency mask of reduced-resolution image
> 0x6 = Transparency mask of multi-page image
> 0x7 = Transparency mask of reduced-resolution multi-page image
> 0x10001 = Alternate reduced-resolution image
> 0xffffffff = invalid
> Bit 0 = Reduced resolution
> Bit 1 = Single page
> Bit 2 = Transparency mask
> Bit 3 = TIFF/IT final page
> Bit 4 = TIFF-FX mixed raster content

> 0x0103 | Compression | N | --> EXIF Compression Values
> 0x011a | XResolution | N |
> 0x011b | YResolution | N |
> 0x0128 | ResolutionUnit | N | 1 = None 2 = inches 3 = cm
> 0x0201 | PreviewImageStart | int32u* |
> 0x0202 | PreviewImageLength | int32u* |
> 0x0213 | YCbCrPositioning | N | 1 = Centered 2 = Co-sited

## Nikon ColorBalanceA Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 624 | RedBalance | int16u! |
> 625 | BlueBalance | int16u! |

## Nikon VRInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | VRInfoVersion | N |
> 4 | VibrationReduction | int8u | 1 = On 2 = Off
> 6 | VRMode | int8u | 0 = Normal 2 = Active

## Nikon FaceDetect Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | FaceDetectFrameSize | int16u[2] |
> 3 | FacesDetected | int16u |
> 4 | Face1Position | int16u[4] | (top, left, width and height of face detect area in coordinates of FaceDetectFrameSize)
> 8 | Face2Position | int16u[4] |
> 12 | Face3Position | int16u[4] |
> 16 | Face4Position | int16u[4] |
> 20 | Face5Position | int16u[4] |
> 24 | Face6Position | int16u[4] |
> 28 | Face7Position | int16u[4] |
> 32 | Face8Position | int16u[4] |
> 36 | Face9Position | int16u[4] |
> 40 | Face10Position | int16u[4] |
> 44 | Face11Position | int16u[4] |
> 48 | Face12Position | int16u[4] |

## Nikon PictureControl Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PictureControlVersion | N |
> 4 | PictureControlName | string[20] |
> 24 | PictureControlBase | string[20] |
> 48 | PictureControlAdjust | int8u | 0 = Default Settings 1 = Quick Adjust 2 = Full Control
> 49 | PictureControlQuickAdjust | int8u |
> 50 | Sharpness | int8u |
> 51 | Contrast | int8u |
> 52 | Brightness | int8u |
> 53 | Saturation | int8u |
> 54 | HueAdjustment | int8u |

> 55

> FilterEffect

> int8u

> 0x80 = Off 0x81 = Yellow 0x82 = Orange |  | 0x83 = Red 0x84 = Green 0xff = n/a |

> 56

> ToningEffect

> int8u

> 0x80 = B&W
> 0x81 = Sepia
> 0x82 = Cyanotype
> 0x83 = Red
> 0x84 = Yellow
> 0x85 = Green

> 0x86 = Blue-green
> 0x87 = Blue
> 0x88 = Purple-blue
> 0x89 = Red-purple
> 0xff = n/a

> 57 | ToningSaturation | int8u |

## Nikon WorldTime Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Timezone | int16s |
> 2 | DaylightSavings | int8u | 0 = No 1 = Yes
> 3 | DateDisplayFormat | int8u | 0 = Y/M/D 1 = M/D/Y 2 = D/M/Y

## Nikon ISOInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ISO | int8u | (val = 100 * 2**(raw/12-5))

> 4

> ISOExpansion

> int16u

> 0x0 = Off
> 0x101 = Hi 0.3
> 0x102 = Hi 0.5
> 0x103 = Hi 0.7
> 0x104 = Hi 1.0
> 0x105 = Hi 1.3
> 0x106 = Hi 1.5

> 0x107 = Hi 1.7
> 0x108 = Hi 2.0
> 0x201 = Lo 0.3
> 0x202 = Lo 0.5
> 0x203 = Lo 0.7
> 0x204 = Lo 1.0

> 6 | ISO2 | int8u | (val = 100 * 2**(raw/12-5))

> 10

> ISOExpansion2

> int16u

> 0x0 = Off
> 0x101 = Hi 0.3
> 0x102 = Hi 0.5
> 0x103 = Hi 0.7
> 0x104 = Hi 1.0
> 0x105 = Hi 1.3
> 0x106 = Hi 1.5

> 0x107 = Hi 1.7
> 0x108 = Hi 2.0
> 0x201 = Lo 0.3
> 0x202 = Lo 0.5
> 0x203 = Lo 0.7
> 0x204 = Lo 1.0

## Nikon DistortInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DistortionVersion? | N |
> 4 | AutoDistortionControl | int8u | 0 = Off 1 = On

## Nikon UnknownInfo Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | UnknownInfoVersion? | N |

## Nikon UnknownInfo2 Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | UnknownInfo2Version? | N |

## Nikon HDRInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | HDRInfoVersion | string[4] |
> 4 | HDR | int8u | 0 = Off 1 = On 48 = Auto
> 5 | HDRLevel | int8u | 0 = Auto 1 = 1 EV 2 = 2 EV 3 = 3 EV 255 = n/a

> 6

> HDRSmoothing

> int8u

> 0 = Off 1 = Normal 2 = Low |  | 3 = High 48 = Auto 255 = n/a |

> 7 | HDRLevel2 | int8u | 0 = Auto 1 = 1 EV 2 = 2 EV 3 = 3 EV 255 = n/a

## Nikon LocationInfo Tags

Tags written by some Nikon GPS-equipped cameras like the AW100.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LocationInfoVersion | undef[4] |
> 4 | TextEncoding | int8u | 0 = n/a 1 = UTF8 2 = UTF16
> 5 | CountryCode | string[3] |
> 9 | Location | undef[70] |

## Nikon AFInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0

> AFAreaMode

> int8u

> 0 = Single Area
> 1 = Dynamic Area
> 2 = Dynamic Area (closest subject)
> 3 = Group Dynamic
> 4 = Single Area (wide)
> 5 = Dynamic Area (wide)

> 1

> AFPoint

> int8u

> (in some focus modes this value is not meaningful)

> 0 = Center
> 1 = Top
> 2 = Bottom
> 3 = Mid-left
> 4 = Mid-right
> 5 = Upper-left

> 6 = Upper-right
> 7 = Lower-left
> 8 = Lower-right
> 9 = Far Left
> 10 = Far Right

> 2

> AFPointsInFocus

> int16u

> 0x7ff = All 11 Points
> Bit 0 = Center
> Bit 1 = Top
> Bit 2 = Bottom
> Bit 3 = Mid-left
> Bit 4 = Mid-right

> Bit 5 = Upper-left
> Bit 6 = Upper-right
> Bit 7 = Lower-left
> Bit 8 = Lower-right
> Bit 9 = Far Left
> Bit 10 = Far Right

## Nikon ShotInfoD40 Tags

These tags are extracted from encrypted data in D40 and D40X images.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 582 | ShutterCount | int32u |
> 586.1 | VibrationReduction | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 729 | CustomSettingsD40 | - | --> NikonCustom SettingsD40 Tags

## Nikon ShotInfoD80 Tags

These tags are extracted from encrypted data in D80 images.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 586 | ShutterCount | int32u |
> 590.1 | Rotation | int8u | [Mask 0x07] 0x0 = Horizontal 0x1 = Rotated 270 CW 0x2 = Rotated 90 CW 0x3 = Rotated 180
> 590.2 | VibrationReduction | int8u | [Mask 0x18] 0x0 = Off 0x18 = On
> 590.3 | FlashFired | int8u | [Mask 0xe0] Bit 6 = Internal Bit 7 = External
> 708 | NikonImageSize | int8u | [Mask 0xf0] 0x0 = Large (10.0 M) 0x10 = Medium (5.6 M) 0x20 = Small (2.5 M)

> 708.1

> ImageQuality

> int8u

> [Mask 0x0f]

> 0x0 = NEF (RAW)
> 0x1 = JPEG Fine
> 0x2 = JPEG Normal
> 0x3 = JPEG Basic
> 0x4 = NEF (RAW) + JPEG Fine
> 0x5 = NEF (RAW) + JPEG Normal
> 0x6 = NEF (RAW) + JPEG Basic

> 748 | CustomSettingsD80 | - | --> NikonCustom SettingsD80 Tags

## Nikon ShotInfoD90 Tags

These tags are extracted from encrypted data in images from the D90 with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 693 | ISO2 | int8u |
> 725 | ShutterCount | int32u |
> 884 | CustomSettingsD90 | - | --> NikonCustom SettingsD90 Tags

## Nikon ShotInfoD3a Tags

These tags are extracted from encrypted data in images from the D3 with firmware 1.00 and earlier.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 598 | ISO2 | int8u |
> 630 | ShutterCount | int32u |
> 723.1 | NikonImageSize | int8u | [Mask 0x18] 0x0 = Large 0x8 = Medium 0x10 = Small

> 723.2

> ImageQuality

> int8u

> [Mask 0x07]

> 0x0 = NEF (RAW) + JPEG Fine
> 0x1 = NEF (RAW) + JPEG Norm
> 0x2 = NEF (RAW) + JPEG Basic
> 0x3 = NEF (RAW)
> 0x4 = TIF (RGB)
> 0x5 = JPEG Fine
> 0x6 = JPEG Normal
> 0x7 = JPEG Basic

> 769 | CustomSettingsD3 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD3b Tags

These tags are extracted from encrypted data in images from the D3 with firmware 1.10, 2.00, 2.01 and 2.02.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 16 | ImageArea | int8u | 0 = FX (36.0 x 23.9 mm) 1 = DX (23.5 x 15.6 mm) 2 = 5:4 (30.0 x 23.9 mm)
> 605 | ISO2 | int8u |
> 637 | ShutterCount | int32u | (firmware 1.10)
> 639 | ShutterCount | int32u | (firmware 2.00, 2.01 and 2.02)
> 650 | PreFlashReturnStrength | int8u | (valid in TTL and TTL-BL flash control modes)
> 732.1 | NikonImageSize | int8u | [Mask 0x18] 0x0 = Large 0x8 = Medium 0x10 = Small

> 732.2

> ImageQuality

> int8u

> [Mask 0x07]

> 0x0 = NEF (RAW) + JPEG Fine
> 0x1 = NEF (RAW) + JPEG Norm
> 0x2 = NEF (RAW) + JPEG Basic
> 0x3 = NEF (RAW)
> 0x4 = TIF (RGB)
> 0x5 = JPEG Fine
> 0x6 = JPEG Normal
> 0x7 = JPEG Basic

> 778 | CustomSettingsD3 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD3X Tags

These tags are extracted from encrypted data in images from the D3X with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 605 | ISO2 | int8u |
> 640 | ShutterCount | int32u |
> 779 | CustomSettingsD3X | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD3S Tags

These tags are extracted from encrypted data in images from the D3S with firmware 1.00 and earlier.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 16 | ImageArea | int8u | 0 = FX (36x24) 1 = DX (24x16) 2 = 5:4 (30x24) 3 = 1.2x (30x20)
> 545 | ISO2 | int8u |
> 578 | ShutterCount | int32u |
> 718 | CustomSettingsD3S | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD300a Tags

These tags are extracted from encrypted data in images from the D300 with firmware 1.00 and earlier.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 604 | ISO2 | int8u |
> 633 | ShutterCount | int32u |

> 721

> AFFineTuneAdj

> int16u

> 0x0 = 0
> 0x3a = +1
> 0x3b = +2
> 0x3c = +4
> 0x3d = +8
> 0x3e = +16
> 0xc2 = -16
> 0xc3 = -8
> 0xc4 = -4
> 0xc5 = -2
> 0xc6 = -1
> 0x103e = +17
> 0x10c2 = -17
> 0x203d = +9

> 0x203e = +18
> 0x20c2 = -18
> 0x20c3 = -9
> 0x303e = +19
> 0x30c2 = -19
> 0x403c = +5
> 0x403d = +10
> 0x403e = +20
> 0x40c2 = -20
> 0x40c3 = -10
> 0x40c4 = -5
> 0x603d = +11
> 0x60c3 = -11
> 0x803b = +3

> 0x803c = +6
> 0x803d = +12
> 0x80c3 = -12
> 0x80c4 = -6
> 0x80c5 = -3
> 0xa03d = +13
> 0xa0c3 = -13
> 0xc03c = +7
> 0xc03d = +14
> 0xc0c3 = -14
> 0xc0c4 = -7
> 0xe03d = +15
> 0xe0c3 = -15

> 790 | CustomSettingsD300 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD300b Tags

These tags are extracted from encrypted data in images from the D300 with firmware 1.10.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 613 | ISO2 | int8u |
> 644 | ShutterCount | int32u |

> 732

> AFFineTuneAdj

> int16u

> (firmware version 1.10B)

> 0x0 = 0
> 0x83e = +11
> 0x8c2 = -11
> 0x203c = +3
> 0x203d = +6
> 0x203e = +12
> 0x20c2 = -12
> 0x20c3 = -6
> 0x20c4 = -3
> 0x383e = +13
> 0x38c2 = -13
> 0x503d = +7
> 0x503e = +14
> 0x50c2 = -14

> 0x50c3 = -7
> 0x683e = +15
> 0x68c2 = -15
> 0x803a = +1
> 0x803b = +2
> 0x803c = +4
> 0x803d = +8
> 0x803e = +16
> 0x80c2 = -16
> 0x80c3 = -8
> 0x80c4 = -4
> 0x80c5 = -2
> 0x80c6 = -1
> 0x983e = +17

> 0x98c2 = -17
> 0xb03d = +9
> 0xb03e = +18
> 0xb0c2 = -18
> 0xb0c3 = -9
> 0xc83e = +19
> 0xc8c2 = -19
> 0xe03c = +5
> 0xe03d = +10
> 0xe03e = +20
> 0xe0c2 = -20
> 0xe0c3 = -10
> 0xe0c4 = -5

> (other versions)

> 0x0 = 0
> 0x43e = +13
> 0x4c2 = -13
> 0x183d = +7
> 0x183e = +14
> 0x18c2 = -14
> 0x18c3 = -7
> 0x2c3e = +15
> 0x2cc2 = -15
> 0x403a = +1
> 0x403b = +2
> 0x403c = +4
> 0x403d = +8
> 0x403e = +16

> 0x40c2 = -16
> 0x40c3 = -8
> 0x40c4 = -4
> 0x40c5 = -2
> 0x40c6 = -1
> 0x543e = +17
> 0x54c2 = -17
> 0x683d = +9
> 0x683e = +18
> 0x68c2 = -18
> 0x68c3 = -9
> 0x7c3e = +19
> 0x7cc2 = -19
> 0x903c = +5

> 0x903d = +10
> 0x903e = +20
> 0x90c2 = -20
> 0x90c3 = -10
> 0x90c4 = -5
> 0xb83d = +11
> 0xb8c3 = -11
> 0xe03b = +3
> 0xe03c = +6
> 0xe03d = +12
> 0xe0c3 = -12
> 0xe0c4 = -6
> 0xe0c5 = -3

> 802 | CustomSettingsD300 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD300S Tags

These tags are extracted from encrypted data in images from the D300S with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 613 | ISO2 | int8u |
> 646 | ShutterCount | int32u |
> 804 | CustomSettingsD300S | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD700 Tags

These tags are extracted from encrypted data in images from the D700 with firmware 1.02f.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 613 | ISO2 | int8u |
> 647 | ShutterCount | int32u |
> 804 | CustomSettingsD700 | - | --> NikonCustom SettingsD700 Tags

## Nikon ShotInfoD800 Tags

These tags are extracted from encrypted data in images from the D800.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 1216 | RepeatingFlashOutputExternal | int8u |
> 1218 | RepeatingFlashRateExternal | int8u |
> 1219 | RepeatingFlashCountExternal | int8u |
> 1234 | FlashExposureComp2 | int8s | (includes the effect of flash bracketing)
> 1242 | RepeatingFlashRateBuilt-in | int8u |
> 1243 | RepeatingFlashCountBuilt-in | int8u |
> 1308 | SequenceNumber | int8u |
> 1531 | ShutterCount | int32u |
> 1772 | CustomSettingsD800 | - | --> NikonCustom SettingsD800 Tags

## Nikon ShotInfoD5000 Tags

These tags are extracted from encrypted data in images from the D5000 with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 693 | ISO2 | int8u |
> 726 | ShutterCount | int32u |
> 888 | CustomSettingsD5000 | - | --> NikonCustom SettingsD5000 Tags

## Nikon ShotInfoD5100 Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 801 | ShutterCount | int32u |
> 1031 | CustomSettingsD5100 | - | --> NikonCustom SettingsD5100 Tags

## Nikon ShotInfoD5200 Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 3032 | ShutterCount | int32u |
> 3285 | CustomSettingsD5200 | - | --> NikonCustom SettingsD5200 Tags

## Nikon ShotInfoD7000 Tags

These tags are extracted from encrypted data in images from the D7000 with firmware 1.01b.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 800 | ShutterCount | int32u |
> 1028 | CustomSettingsD7000 | - | --> NikonCustom SettingsD7000 Tags

## Nikon ShotInfo Tags

This information is encrypted for ShotInfoVersion 02xx, and some tags are only valid for specific models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | N |
> 4 | FirmwareVersion | N |
> 16 | DistortionControl | int8u | (P6000) 0 = Off 1 = On
> 102 | VR_0x66? | int8u | (D2X, D2Xs (unverified)) 0 = Off 1 = On (normal) 2 = On (active)
> 106 | ShutterCount | int32u | (D2X, D2Xs)
> 110 | DeletedImageCount | int32u | (D2X, D2Xs)
> 117 | VibrationReduction | int8u | (D200) 0 = Off 1 = On (1) 2 = On (2) 3 = On (3)
> 130 | VibrationReduction | int8u | (D2X, D2Xs) 0 = Off 1 = On
> 343 | ShutterCount | undef[2] | (D50)
> 430 | VibrationReduction | int8u | (D50) 0x0 = n/a 0xc = Off 0xf = On
> 589 | ShutterCount | int32u | (D60)

## Nikon ColorBalance1 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_RBGGLevels | int16u[4]! |

## Nikon ColorBalance2 Tags

This information is encrypted for most camera models.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_RGGBLevels | int16u[4]! |

## Nikon ColorBalance3 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_RGBGLevels | int16u[4]! |

## Nikon ColorBalance4 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_GRBGLevels | int16u[4]! |

## Nikon ColorBalanceUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ColorBalanceVersion | undef[4] |

## Nikon LensData00 Tags

This structure is used by the D100, and D1X with firmware version 1.1.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | N |
> 6 | LensIDNumber | int8u | (see LensID values below)
> 7 | LensFStops | int8u |
> 8 | MinFocalLength | int8u |
> 9 | MaxFocalLength | int8u |
> 10 | MaxApertureAtMinFocal | int8u |
> 11 | MaxApertureAtMaxFocal | int8u |
> 12 | MCUVersion | int8u |

## Nikon LensData01 Tags

Nikon encrypts the LensData information below if LensDataVersion is 0201 or higher, but the decryption algorithm is known so the information can be extracted.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | N |
> 4 | ExitPupilPosition | int8u |
> 5 | AFAperture | int8u |
> 8 | FocusPosition | int8u |
> 9 | FocusDistance | int8u | (this focus distance is approximate, and not very accurate for some lenses)
> 10 | FocalLength | int8u |
> 11 | LensIDNumber | int8u | (see LensID values below)
> 12 | LensFStops | int8u |
> 13 | MinFocalLength | int8u |
> 14 | MaxFocalLength | int8u |
> 15 | MaxApertureAtMinFocal | int8u |
> 16 | MaxApertureAtMaxFocal | int8u |
> 17 | MCUVersion | int8u |
> 18 | EffectiveMaxAperture | int8u |

## Nikon LensData0204 Tags

Nikon encrypts the LensData information below if LensDataVersion is 0201 or higher, but the decryption algorithm is known so the information can be extracted.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | N |
> 4 | ExitPupilPosition | int8u |
> 5 | AFAperture | int8u |
> 8 | FocusPosition | int8u |
> 10 | FocusDistance | int8u | (this focus distance is approximate, and not very accurate for some lenses)
> 11 | FocalLength | int8u |
> 12 | LensIDNumber | int8u | (see LensID values below)
> 13 | LensFStops | int8u |
> 14 | MinFocalLength | int8u |
> 15 | MaxFocalLength | int8u |
> 16 | MaxApertureAtMinFocal | int8u |
> 17 | MaxApertureAtMaxFocal | int8u |
> 18 | MCUVersion | int8u |
> 19 | EffectiveMaxAperture | int8u |

## Nikon LensData0400 Tags

Tags extracted from the encrypted lens data of Nikon 1 models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | N |
> 394 | LensModel | string[64] |

## Nikon LensDataUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | N |

## Nikon FlashInfo0100 Tags

These tags are used by the D2H, D2Hs, D2X, D2Xs, D50, D70, D70s, D80 and D200.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | N |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8 | ExternalFlashFlags | int8u | Bit 0 = Fired Bit 2 = Bounce Flash Bit 4 = Wide Flash Adapter Bit 5 = Dome Diffuser
> 9.1 | FlashCommanderMode | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 9.2 | FlashControlMode | int8u | [Mask 0x7f] --> Nikon FlashControlMode Values
> 10 | FlashOutput FlashCompensation | int8u int8s |
> 11 | FlashFocalLength | int8u |
> 12 | RepeatingFlashRate | int8u |
> 13 | RepeatingFlashCount | int8u |
> 14 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values
> 15 | FlashGroupAControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values
> 16 | FlashGroupBControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values
> 17 | FlashGroupAOutput FlashGroupACompensation | int8u int8s |
> 18 | FlashGroupBOutput FlashGroupBCompensation | int8u int8s |

## Nikon FlashFirmware Values

> Value | FlashFirmware | Value | FlashFirmware
> --- | --- | --- | ---
> '0 0' | = n/a | '4 1' | = 4.01 (SB-400)
> '1 1' | = 1.01 (SB-800 or Metz 58 AF-1) | '4 2' | = 4.02 (SB-400)
> '1 3' | = 1.03 (SB-800) | '4 4' | = 4.04 (SB-400)
> '2 1' | = 2.01 (SB-800) | '5 1' | = 5.01 (SB-900)
> '2 4' | = 2.04 (SB-600) | '5 2' | = 5.02 (SB-900)
> '2 5' | = 2.05 (SB-600) | '7 1' | = 7.01 (SB-910)
> '3 1' | = 3.01 (SU-800 Remote Commander) |  |

## Nikon FlashControlMode Values

> Value | FlashControlMode | Value | FlashControlMode | Value | FlashControlMode
> --- | --- | --- | --- | --- | ---
> 0x0 | = Off | 0x3 | = Auto Aperture | 0x6 | = Manual
> 0x1 | = iTTL-BL | 0x4 | = Automatic | 0x7 | = Repeating Flash
> 0x2 | = iTTL | 0x5 | = GN (distance priority) |  |

## Nikon FlashGNDistance Values

> Value | FlashGNDistance | Value | FlashGNDistance | Value | FlashGNDistance
> --- | --- | --- | --- | --- | ---
> 0 | = 0 | 13 | = 1.4 m | 26 | = 6.3 m
> 1 | = 0.1 m | 14 | = 1.6 m | 27 | = 7.1 m
> 2 | = 0.2 m | 15 | = 1.8 m | 28 | = 8.0 m
> 3 | = 0.3 m | 16 | = 2.0 m | 29 | = 9.0 m
> 4 | = 0.4 m | 17 | = 2.2 m | 30 | = 10.0 m
> 5 | = 0.5 m | 18 | = 2.5 m | 31 | = 11.0 m
> 6 | = 0.6 m | 19 | = 2.8 m | 32 | = 13.0 m
> 7 | = 0.7 m | 20 | = 3.2 m | 33 | = 14.0 m
> 8 | = 0.8 m | 21 | = 3.6 m | 34 | = 16.0 m
> 9 | = 0.9 m | 22 | = 4.0 m | 35 | = 18.0 m
> 10 | = 1.0 m | 23 | = 4.5 m | 36 | = 20.0 m
> 11 | = 1.1 m | 24 | = 5.0 m | 255 | = n/a
> 12 | = 1.3 m | 25 | = 5.6 m |  |

## Nikon FlashInfo0102 Tags

These tags are used by the D3 (firmware 1.x), D40, D40X, D60 and D300 (firmware 1.00).

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | N |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8 | ExternalFlashFlags | int8u | Bit 0 = Fired Bit 2 = Bounce Flash Bit 4 = Wide Flash Adapter Bit 5 = Dome Diffuser
> 9.1 | FlashCommanderMode | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 9.2 | FlashControlMode | int8u | [Mask 0x7f] --> Nikon FlashControlMode Values
> 10 | FlashOutput FlashCompensation | int8u int8s |
> 12 | FlashFocalLength | int8u |
> 13 | RepeatingFlashRate | int8u |
> 14 | RepeatingFlashCount | int8u |
> 15 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values
> 16.1 | FlashGroupAControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group A tags may apply to the built-in flash settings for some models)
> 17.1 | FlashGroupBControlMode | int8u | [Mask 0xf0] --> Nikon FlashControlMode Values (note: group B tags may apply to group A settings for some models)
> 17.2 | FlashGroupCControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group C tags may apply to group B settings for some models)
> 18 | FlashGroupAOutput FlashGroupACompensation | int8u int8s |
> 19 | FlashGroupBOutput FlashGroupBCompensation | int8u int8s |
> 20 | FlashGroupCOutput FlashGroupCCompensation | int8u int8s |

## Nikon FlashInfo0103 Tags

These tags are used by the D3 (firmware 2.x), D3X, D3S, D4, D90, D300 (firmware 1.10), D300S, D600, D700, D800, D3000, D3100, D3200, D5000, D5100, D5200, D7000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | N |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8 | ExternalFlashFlags | int8u | Bit 0 = Fired Bit 2 = Bounce Flash Bit 4 = Wide Flash Adapter Bit 5 = Dome Diffuser
> 9.1 | FlashCommanderMode | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 9.2 | FlashControlMode | int8u | [Mask 0x7f] --> Nikon FlashControlMode Values
> 10 | FlashOutput FlashCompensation | int8u int8s |
> 12 | FlashFocalLength | int8u |
> 13 | RepeatingFlashRate | int8u |
> 14 | RepeatingFlashCount | int8u |
> 15 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values

> 16

> FlashColorFilter

> int8u

> 0 = None 1 = FL-GL1 2 = FL-GL2 |  | 9 = TN-A1 10 = TN-A2 65 = Red |  | 66 = Blue 67 = Yellow 68 = Amber |

> 17.1 | FlashGroupAControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group A tags may apply to the built-in flash settings for some models)
> 18.1 | FlashGroupBControlMode | int8u | [Mask 0xf0] --> Nikon FlashControlMode Values (note: group B tags may apply to group A settings for some models)
> 18.2 | FlashGroupCControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group C tags may apply to group B settings for some models)
> 19 | FlashGroupAOutput FlashGroupACompensation | int8u int8s |
> 20 | FlashGroupBOutput FlashGroupBCompensation | int8u int8s |
> 21 | FlashGroupCOutput FlashGroupCCompensation | int8u int8s |
> 27 | ExternalFlashCompensation | int8s |
> 29 | FlashExposureComp3 | int8s | (does not include the effect of flash bracketing)
> 39 | FlashExposureComp4 | int8s | (includes the effect of flash bracketing. Valid for repeating flash)

## Nikon FlashInfoUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | N |

## Nikon MultiExposure Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MultiExposureVersion | N |
> 1 | MultiExposureMode | int32u | 0 = Off 1 = Multiple Exposure 2 = Image Overlay 3 = HDR
> 2 | MultiExposureShots | int32u |
> 3 | MultiExposureAutoGain | int32u | 0 = Off 1 = On

## Nikon AFInfo2 Tags

These tags are written by Nikon DSLR's which have the live view feature.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFInfo2Version | N |
> 4 | ContrastDetectAF | int8u | (this is Off for the hybrid AF used in Nikon 1 models) 0 = Off 1 = On

> 5

> AFAreaMode

> int8u

> (ContrastDetectAF Off)

> 0 = Single Area
> 1 = Dynamic Area
> 2 = Dynamic Area (closest subject)
> 3 = Group Dynamic
> 4 = Dynamic Area (9 points)
> 5 = Dynamic Area (21 points)
> 6 = Dynamic Area (51 points)
> 7 = Dynamic Area (51 points, 3D-tracking)
> 8 = Auto-area
> 9 = Dynamic Area (3D-tracking)
> 10 = Single Area (wide)
> 11 = Dynamic Area (wide)
> 12 = Dynamic Area (wide, 3D-tracking)
> 128 = Single (135 points)
> 129 = Auto (41 points)
> 130 = Subject Tracking (41 points)
> 131 = Face Priority (41 points)

> (ContrastDetectAF On)
> 0 = Contrast-detect
> 1 = Contrast-detect (normal area)
> 2 = Contrast-detect (wide area)
> 3 = Contrast-detect (face priority)
> 4 = Contrast-detect (subject tracking)

> 6

> PhaseDetectAF

> int8u

> (PrimaryAFPoint and AFPointsUsed below are only valid when this is On)
> 0 = Off
> 1 = On (51-point)
> 2 = On (11-point)
> 3 = On (39-point)
> 4 = On (hybrid)

> 7

> PrimaryAFPoint

> int8u

> (models with 51-point AF: D3, D3S, D3X, D300, D300S, D700 and D800)

> 0 = (none)
> 1 = C6 (Center)
> 2 = B6
> 3 = A5
> 4 = D6
> 5 = E5
> 6 = C7
> 7 = B7
> 8 = A6
> 9 = D7
> 10 = E6

> 11 = C5
> 12 = B5
> 13 = A4
> 14 = D5
> 15 = E4
> 16 = C8
> 17 = B8
> 18 = A7
> 19 = D8
> 20 = E7
> 21 = C9

> 22 = B9
> 23 = A8
> 24 = D9
> 25 = E8
> 26 = C10
> 27 = B10
> 28 = A9
> 29 = D10
> 30 = E9
> 31 = C11
> 32 = B11

> 33 = D11
> 34 = C4
> 35 = B4
> 36 = A3
> 37 = D4
> 38 = E3
> 39 = C3
> 40 = B3
> 41 = A2
> 42 = D3
> 43 = E2

> 44 = C2
> 45 = B2
> 46 = A1
> 47 = D2
> 48 = E1
> 49 = C1
> 50 = B1
> 51 = D1

> (models with 11-point AF: D90, D3000, D3100, D5000 and D5100)

> 0 = (none)
> 1 = Center
> 2 = Top
> 3 = Bottom
> 4 = Mid-left
> 5 = Upper-left

> 6 = Lower-left
> 7 = Far Left
> 8 = Mid-right
> 9 = Upper-right
> 10 = Lower-right
> 11 = Far Right

> (models with 39-point AF: D600 and D7000)

> 0 = (none)
> 1 = C6 (Center)
> 2 = B6
> 3 = A2
> 4 = D6
> 5 = E2
> 6 = C7
> 7 = B7

> 8 = A3
> 9 = D7
> 10 = E3
> 11 = C5
> 12 = B5
> 13 = A1
> 14 = D5
> 15 = E1

> 16 = C8
> 17 = B8
> 18 = D8
> 19 = C9
> 20 = B9
> 21 = D9
> 22 = C10
> 23 = B10

> 24 = D10
> 25 = C11
> 26 = B11
> 27 = D11
> 28 = C4
> 29 = B4
> 30 = D4
> 31 = C3

> 32 = B3
> 33 = D3
> 34 = C2
> 35 = B2
> 36 = D2
> 37 = C1
> 38 = B1
> 39 = D1

> (models with 135-point AF: Nikon 1 models)

> 0 = (none)
> 1 = E8 (Center)
> 2 = D8
> 3 = C8
> 4 = B8
> 5 = A8
> 6 = F8
> 7 = G8
> 8 = H8
> 9 = I8
> 10 = E9
> 11 = D9
> 12 = C9
> 13 = B9
> 14 = A9
> 15 = F9
> 16 = G9
> 17 = H9
> 18 = I9
> 19 = E7
> 20 = D7
> 21 = C7
> 22 = B7
> 23 = A7
> 24 = F7
> 25 = G7
> 26 = H7
> 27 = I7

> 28 = E10
> 29 = D10
> 30 = C10
> 31 = B10
> 32 = A10
> 33 = F10
> 34 = G10
> 35 = H10
> 36 = I10
> 37 = E11
> 38 = D11
> 39 = C11
> 40 = B11
> 41 = A11
> 42 = F11
> 43 = G11
> 44 = H11
> 45 = I11
> 46 = E12
> 47 = D12
> 48 = C12
> 49 = B12
> 50 = A12
> 51 = F12
> 52 = G12
> 53 = H12
> 54 = I12
> 55 = E13

> 56 = D13
> 57 = C13
> 58 = B13
> 59 = A13
> 60 = F13
> 61 = G13
> 62 = H13
> 63 = I13
> 64 = E14
> 65 = D14
> 66 = C14
> 67 = B14
> 68 = A14
> 69 = F14
> 70 = G14
> 71 = H14
> 72 = I14
> 73 = E15
> 74 = D15
> 75 = C15
> 76 = B15
> 77 = A15
> 78 = F15
> 79 = G15
> 80 = H15
> 81 = I15
> 82 = E6
> 83 = D6

> 84 = C6
> 85 = B6
> 86 = A6
> 87 = F6
> 88 = G6
> 89 = H6
> 90 = I6
> 91 = E5
> 92 = D5
> 93 = C5
> 94 = B5
> 95 = A5
> 96 = F5
> 97 = G5
> 98 = H5
> 99 = I5
> 100 = E4
> 101 = D4
> 102 = C4
> 103 = B4
> 104 = A4
> 105 = F4
> 106 = G4
> 107 = H4
> 108 = I4
> 109 = E3
> 110 = D3
> 111 = C3

> 112 = B3
> 113 = A3
> 114 = F3
> 115 = G3
> 116 = H3
> 117 = I3
> 118 = E2
> 119 = D2
> 120 = C2
> 121 = B2
> 122 = A2
> 123 = F2
> 124 = G2
> 125 = H2
> 126 = I2
> 127 = E1
> 128 = D1
> 129 = C1
> 130 = B1
> 131 = A1
> 132 = F1
> 133 = G1
> 134 = H1
> 135 = I1

> (future models?...)
> 0 = (none)
> 1 = Center

> 8

> AFPointsUsed
> AFPointsUsed
> AFPointsUsed
> AFPointsUsed
> AFPointsUsed

> undef[7]
> undef[2]
> undef[7]
> undef[17]
> undef[7]

> (models with 51-point AF -- 5 rows: A1-9, B1-11, C1-11, D1-11, E1-9. Center point is C6)
> (models with 11-point AF)

> 0x7ff = All 11 Points
> Bit 0 = Center
> Bit 1 = Top
> Bit 2 = Bottom
> Bit 3 = Mid-left
> Bit 4 = Upper-left

> Bit 5 = Lower-left
> Bit 6 = Far Left
> Bit 7 = Mid-right
> Bit 8 = Upper-right
> Bit 9 = Lower-right
> Bit 10 = Far Right

> (models with 39-point AF -- 5 rows: A1-3, B1-11, C1-11, D1-11, E1-3. Center point is C6)
> (models with 135-point AF -- 9 rows (A-I) and 15 columns (1-15). Center point is E8. The odd-numbered columns, columns 2 and 14, and the remaining corner points are not used for 41-point AF mode)

> 16 | AFImageWidth | int16u | (this and the following tags are valid only for contrast-detect AF)
> 18 | AFImageHeight | int16u |
> 20 | AFAreaXPosition | int16u | (center of AF area in AFImage coordinates)
> 22 | AFAreaYPosition | int16u |
> 24 | AFAreaWidth | int16u | (size of AF area in AFImage coordinates)
> 26 | AFAreaHeight | int16u |
> 28 | ContrastDetectAFInFocus | int8u | 0 = No 1 = Yes

## Nikon FileInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FileInfoVersion | N |
> 6 | DirectoryNumber | int16u |
> 8 | FileNumber | int16u |

## Nikon AFTune Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFFineTune | int8u | 0 = Off 1 = On (1) 2 = On (2)
> 1 | AFFineTuneIndex | int8u | (index of saved lens)
> 2 | AFFineTuneAdj | int8s | (may only be valid for saved lenses)

## Nikon CaptureOffsets Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | IFD0_Offset | N |
> 0x0002 | PreviewIFD_Offset | N |
> 0x0003 | SubIFD_Offset | N |

## Nikon Scan Tags

This information is written by the Nikon Scan software.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | FilmType | string |
> 0x0040 | MultiSample | string |
> 0x0041 | BitDepth | int16u |
> 0x0050 | MasterGain | rational64s |
> 0x0051 | ColorGain | rational64s[3] |
> 0x0060 | ScanImageEnhancer | int32u | 0 = Off 1 = On
> 0x0100 | DigitalICE | string |
> 0x0110 | ROCInfo | - | --> Nikon ROC Tags
> 0x0120 | GEMInfo | - | --> Nikon GEM Tags
> 0x0200 | DigitalDEEShadowAdj | int32u |
> 0x0201 | DigitalDEEThreshold | int32u |
> 0x0202 | DigitalDEEHighlightAdj | int32u |

## Nikon ROC Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DigitalROC | int32u |

## Nikon GEM Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DigitalGEM | int32u |

## Nikon CaptureOutput Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | OutputImageWidth | int32u |
> 3 | OutputImageHeight | int32u |
> 4 | OutputResolution | int32u |

## Nikon Type2 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0003 | Quality | Y |
> 0x0004 | ColorMode | Y |
> 0x0005 | ImageAdjustment | Y |
> 0x0006 | CCDSensitivity | Y |
> 0x0007 | WhiteBalance | Y |
> 0x0008 | Focus | Y |
> 0x000a | DigitalZoom | Y |
> 0x000b | Converter | Y |

## Nikon NCDT Tags

Nikon-specific QuickTime tags found in the NCDT atom of MOV videos from some Nikon cameras such as the Coolpix S8000.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'NCHD' | MakerNoteVersion | N |
> 'NCTG' | NikonTags | - | --> Nikon NCTG Tags
> 'NCTH' | ThumbnailImage | N |
> 'NCVW' | PreviewImage | N |

## Nikon NCTG Tags

These tags are found in proprietary-format records of the NCTG atom in MOV videos from some Nikon cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | Make | N |
> 0x0002 | Model | N |
> 0x0003 | Software | N |
> 0x0011 | CreateDate | N |
> 0x0012 | DateTimeOriginal | N |
> 0x0013 | FrameCount | N |
> 0x0016 | FrameRate | N |
> 0x0022 | FrameWidth | N |
> 0x0023 | FrameHeight | N |
> 0x0032 | AudioChannels | N |
> 0x0033 | AudioBitsPerSample | N |
> 0x0034 | AudioSampleRate | N |

> 0x1108822

> ExposureProgram

> N

> 0 = Not Defined
> 1 = Manual
> 2 = Program AE
> 3 = Aperture-priority AE
> 4 = Shutter speed priority AE
> 5 = Creative (Slow speed)
> 6 = Action (High speed)
> 7 = Portrait
> 8 = Landscape

> 0x1109204 | ExposureCompensation | N |

> 0x1109207

> MeteringMode

> N

> 0 = Unknown
> 1 = Average
> 2 = Center-weighted average
> 3 = Spot
> 4 = Multi-spot
> 5 = Multi-segment
> 6 = Partial
> 255 = Other

> 0x110a434 | LensModel | N |
> 0x1200000 | GPSVersionID | N |
> 0x1200001 | GPSLatitudeRef | N | 'N' = North 'S' = South
> 0x1200002 | GPSLatitude | N |
> 0x1200003 | GPSLongitudeRef | N | 'E' = East 'W' = West
> 0x1200004 | GPSLongitude | N |
> 0x1200005 | GPSAltitudeRef | N | 0 = Above Sea Level 1 = Below Sea Level
> 0x1200006 | GPSAltitude | N |
> 0x1200007 | GPSTimeStamp | N |
> 0x1200008 | GPSSatellites | N |
> 0x1200010 | GPSImgDirectionRef | N | 'M' = Magnetic North 'T' = True North
> 0x1200011 | GPSImgDirection | N |
> 0x1200012 | GPSMapDatum | N |
> 0x120001d | GPSDateStamp | N |
> 0x2000001 | MakerNoteVersion | N |
> 0x2000005 | WhiteBalance | N |
> 0x200000b | WhiteBalanceFineTune | N |
> 0x200001e | ColorSpace | N | 1 = sRGB 2 = Adobe RGB
> 0x2000023 | PictureControlData | - | --> Nikon PictureControl Tags
> 0x2000024 | WorldTime | - | --> Nikon WorldTime Tags
> 0x200002c | UnknownInfo | - | --> Nikon UnknownInfo Tags
> 0x2000032 | UnknownInfo2 | - | --> Nikon UnknownInfo Tags
> 0x2000039 | LocationInfo | - | --> Nikon LocationInfo Tags
> 0x2000083 | LensType | N | Bit 0 = MF Bit 1 = D Bit 2 = G Bit 3 = VR
> 0x2000084 | Lens | N |
> 0x20000ab | VariProgram | string |

## Nikon MOV Tags

This information is found in MOV and QT videos from some Nikon cameras.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N |
> 38 | ExposureTime | N |
> 42 | FNumber | N |
> 50 | ExposureCompensation | N |

> 68

> WhiteBalance

> N

> 0 = Auto 1 = Daylight 2 = Shade |  | 3 = Fluorescent 4 = Tungsten 5 = Manual |

> 72 | FocalLength | N |
> 175 | Software | N |
> 223 | ISO | N |

## Nikon AVI Tags

Nikon-specific RIFF tags found in AVI videos.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'nctg' | NikonTags | - | --> Nikon AVITags Tags
> 'ncth' | ThumbnailImage | N |
> 'ncvr' | NikonVers | - | --> Nikon AVIVers Tags
> 'ncvw' | PreviewImage | N |

## Nikon AVITags Tags

These tags and the AVIVer tags below are found in proprietary-format records of Nikon AVI videos.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0003 | Make | N |
> 0x0004 | Model | N |
> 0x0005 | Software | N |
> 0x0006 | Equipment | N |

> 0x0007

> Orientation

> N

> 1 = Horizontal (normal)
> 2 = Mirror horizontal
> 3 = Rotate 180
> 4 = Mirror vertical
> 5 = Mirror horizontal and rotate 270 CW
> 6 = Rotate 90 CW
> 7 = Mirror horizontal and rotate 90 CW
> 8 = Rotate 270 CW

> 0x0008 | ExposureTime | N |
> 0x0009 | FNumber | N |
> 0x000a | ExposureCompensation | N |
> 0x000b | MaxApertureValue | N |

> 0x000c

> MeteringMode

> N

> 0 = Unknown
> 1 = Average
> 2 = Center-weighted average
> 3 = Spot
> 4 = Multi-spot
> 5 = Multi-segment
> 6 = Partial
> 255 = Other

> 0x000f | FocalLength | N |
> 0x0010 | XResolution | N |
> 0x0011 | YResolution | N |
> 0x0012 | ResolutionUnit | N | 1 = None 2 = inches 3 = cm
> 0x0013 | DateTimeOriginal | N |
> 0x0014 | CreateDate | N |
> 0x0016 | Duration | N |
> 0x0018 | FocusMode | N |
> 0x001b | DigitalZoom | N |
> 0x001d | ColorMode | N |
> 0x001e | Sharpness | N |
> 0x001f | WhiteBalance | N |
> 0x0020 | NoiseReduction | N |

## Nikon AVIVers Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MakerNoteType | N |
> 0x0002 | MakerNoteVersion | N |

## Nikon LensID Values

The Nikon LensID is constructed as a Composite tag from the raw hex values of 8 other tags: LensIDNumber, LensFStops, MinFocalLength, MaxFocalLength, MaxApertureAtMinFocal, MaxApertureAtMaxFocal, MCUVersion and LensType, in that order. (source: http://www.rottmerhusen.com/objektives/lensid/thirdparty.html.) Multiple lenses with the same LensID are differentiated by decimal values in the list below. The user-defined "Lenses" list may be used to specify the lens for ExifTool to choose in these cases (see the sample config file for details).

> Value | LensID
> --- | ---
> '00 00 00 00 00 00 00 01' | = Manual Lens No CPU
> '00 00 00 00 00 00 E1 12' | = TC-17E II
> '00 00 00 00 00 00 F1 0C' | = TC-14E [II] or Sigma APO Tele Converter 1.4x EX DG or Kenko Teleplus PRO 300 DG 1.4x
> '00 00 00 00 00 00 F2 18' | = TC-20E [II] or Sigma APO Tele Converter 2x EX DG or Kenko Teleplus PRO 300 DG 2.0x
> '00 00 48 48 53 53 00 01' | = Loreo 40mm F11-22 3D Lens in a Cap 9005
> '00 36 1C 2D 34 3C 00 06' | = Tamron SP AF 11-18mm f/4.5-5.6 Di II LD Aspherical (IF) (A13)
> '00 3C 1F 37 30 30 00 06' | = Tokina AT-X 124 AF PRO DX (AF 12-24mm f/4)
> '00 3E 80 A0 38 3F 00 02' | = Tamron SP AF 200-500mm f/5-6.3 Di LD (IF) (A08)
> '00 3F 2D 80 2B 40 00 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) (A14)
> '00 3F 2D 80 2C 40 00 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) Macro (A14)
> '00 3F 80 A0 38 3F 00 02' | = Tamron SP AF 200-500mm f/5-6.3 Di (A08)
> '00 40 11 11 2C 2C 00 00' | = Samyang 8mm f/3.5 Fish-Eye
> '00 40 18 2B 2C 34 00 06' | = Tokina AT-X 107 DX Fisheye (AF 10-17mm f/3.5-4.5)
> '00 40 2A 72 2C 3C 00 06' | = Tokina AT-X 16.5-135 DX (AF 16.5-135mm F3.5-5.6)
> '00 40 2B 2B 2C 2C 00 02' | = Tokina AT-X 17 AF PRO (AF 17mm f/3.5)
> '00 40 2D 2D 2C 2C 00 00' | = Carl Zeiss Distagon T* 3.5/18 ZF.2
> '00 40 2D 80 2C 40 00 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) Macro (A14NII)
> '00 40 2D 88 2C 40 00 06' | = Tamron AF 18-250mm f/3.5-6.3 Di II LD Aspherical (IF) Macro (A18NII)
> '00 40 2D 88 2C 40 62 06' | = Tamron AF 18-250mm f/3.5-6.3 Di II LD Aspherical (IF) Macro (A18)
> '00 40 31 31 2C 2C 00 00' | = Voigtlander Color Skopar 20mm F3.5 SLII Aspherical
> '00 40 37 80 2C 3C 00 02' | = Tokina AT-X 242 AF (AF 24-200mm f/3.5-5.6)
> '00 40 64 64 2C 2C 00 00' | = Voigtlander APO-Lanthar 90mm F3.5 SLII Close Focus
> '00 44 60 98 34 3C 00 02' | = Tokina AT-X 840 D (AF 80-400mm f/4.5-5.6)
> '00 47 10 10 24 24 00 00' | = Fisheye Nikkor 8mm f/2.8 AiS
> '00 47 25 25 24 24 00 02' | = Tamron SP AF 14mm f/2.8 Aspherical (IF) (69E)
> '00 47 44 44 24 24 00 06' | = Tokina AT-X M35 PRO DX (AF 35mm f/2.8 Macro)
> '00 47 53 80 30 3C 00 06' | = Tamron AF 55-200mm f/4-5.6 Di II LD (A15)
> '00 48 1C 29 24 24 00 06' | = Tokina AT-X 116 PRO DX (AF 11-16mm f/2.8)
> '00 48 29 3C 24 24 00 06' | = Tokina AT-X 16-28 AF PRO FX (AF 16-28mm f/2.8)
> '00 48 29 50 24 24 00 06' | = Tokina AT-X 165 PRO DX (AF 16-50mm f/2.8)
> '00 48 32 32 24 24 00 00' | = Carl Zeiss Distagon T* 2.8/21 ZF.2
> '00 48 3C 60 24 24 00 02' | = Tokina AT-X 280 AF PRO (AF 28-80mm f/2.8)
> '00 48 3C 6A 24 24 00 02' | = Tamron SP AF 28-105mm f/2.8 LD Aspherical IF (176D)
> '00 48 50 50 18 18 00 00' | = Nikkor H 50mm f/2
> '00 48 50 72 24 24 00 06' | = Tokina AT-X 535 PRO DX (AF 50-135mm f/2.8)
> '00 48 5C 8E 30 3C 00 06' | = Tamron AF 70-300mm f/4-5.6 Di LD Macro 1:2 (A17NII)
> '00 48 68 68 24 24 00 00' | = Series E 100mm f/2.8
> '00 48 80 80 30 30 00 00' | = Nikkor 200mm f/4 AiS
> '00 49 30 48 22 2B 00 02' | = Tamron SP AF 20-40mm f/2.7-3.5 (166D)
> '00 4C 6A 6A 20 20 00 00' | = Nikkor 105mm f/2.5 AiS
> '00 4C 7C 7C 2C 2C 00 02' | = Tamron SP AF 180mm f/3.5 Di Model (B01)
> '00 53 2B 50 24 24 00 06' | = Tamron SP AF 17-50mm f/2.8 XR Di II LD Aspherical (IF) (A16)
> '00 54 2B 50 24 24 00 06' | = Tamron SP AF 17-50mm f/2.8 XR Di II LD Aspherical (IF) (A16NII)
> '00 54 3C 3C 18 18 00 00' | = Carl Zeiss Distagon T* 2/28 ZF.2
> '00 54 44 44 0C 0C 00 00' | = Nikkor 35mm f/1.4 AiS
> '00 54 44 44 18 18 00 00' | = Carl Zeiss Distagon T* 2/35 ZF.2
> '00 54 48 48 18 18 00 00' | = Voigtlander Ultron 40mm F2 SLII Aspherical
> '00 54 50 50 0C 0C 00 00' | = Carl Zeiss Planar T* 1.4/50 ZF.2
> '00 54 50 50 18 18 00 00' | = Carl Zeiss Makro-Planar T* 2/50 ZF.2
> '00 54 55 55 0C 0C 00 00' | = Voigtlander Nokton 58mm F1.4 SLII
> '00 54 56 56 30 30 00 00' | = Coastal Optical Systems 60mm 1:4 UV-VIS-IR Macro Apo
> '00 54 62 62 0C 0C 00 00' | = Carl Zeiss Planar T* 1.4/85 ZF.2
> '00 54 68 68 18 18 00 00' | = Carl Zeiss Makro-Planar T* 2/100 ZF.2
> '00 54 68 68 24 24 00 02' | = Tokina AT-X M100 PRO D (AF 100mm f/2.8 Macro)
> '00 54 8E 8E 24 24 00 02' | = Tokina AT-X 300 AF PRO (AF 300mm f/2.8)
> '00 58 64 64 20 20 00 00' | = Soligor C/D Macro MC 90mm f/2.5
> '01 00 00 00 00 00 02 00' | = TC-16A
> '01 00 00 00 00 00 08 00' | = TC-16A
> '01 58 50 50 14 14 02 00' | = AF Nikkor 50mm f/1.8
> '02 2F 98 98 3D 3D 02 00' | = Sigma APO 400mm F5.6
> '02 34 A0 A0 44 44 02 00' | = Sigma APO 500mm F7.2
> '02 37 5E 8E 35 3D 02 00' | = Sigma 75-300mm F4.5-5.6 APO
> '02 37 A0 A0 34 34 02 00' | = Sigma APO 500mm F4.5
> '02 3A 5E 8E 32 3D 02 00' | = Sigma 75-300mm F4.0-5.6
> '02 3B 44 61 30 3D 02 00' | = Sigma 35-80mm F4-5.6
> '02 3C B0 B0 3C 3C 02 00' | = Sigma APO 800mm F5.6
> '02 3F 24 24 2C 2C 02 00' | = Sigma 14mm F3.5
> '02 3F 3C 5C 2D 35 02 00' | = Sigma 28-70mm F3.5-4.5 UC
> '02 40 44 5C 2C 34 02 00' | = Exakta AF 35-70mm 1:3.5-4.5 MC
> '02 40 44 73 2B 36 02 00' | = Sigma 35-135mm F3.5-4.5 a
> '02 42 44 5C 2A 34 02 00' | = AF Zoom-Nikkor 35-70mm f/3.3-4.5
> '02 42 44 5C 2A 34 08 00' | = AF Zoom-Nikkor 35-70mm f/3.3-4.5
> '02 46 37 37 25 25 02 00' | = Sigma 24mm F2.8 Super Wide II Macro
> '02 46 3C 5C 25 25 02 00' | = Sigma 28-70mm F2.8
> '02 46 5C 82 25 25 02 00' | = Sigma 70-210mm F2.8 APO
> '02 48 50 50 24 24 02 00' | = Sigma Macro 50mm F2.8
> '02 48 65 65 24 24 02 00' | = Sigma Macro 90mm F2.8
> '03 43 5C 81 35 35 02 00' | = Soligor AF C/D Zoom UMCS 70-210mm 1:4.5
> '03 48 5C 81 30 30 02 00' | = AF Zoom-Nikkor 70-210mm f/4
> '04 48 3C 3C 24 24 03 00' | = AF Nikkor 28mm f/2.8
> '05 54 50 50 0C 0C 04 00' | = AF Nikkor 50mm f/1.4
> '06 3F 68 68 2C 2C 06 00' | = Cosina AF 100mm F3.5 Macro
> '06 54 53 53 24 24 06 00' | = AF Micro-Nikkor 55mm f/2.8
> '07 36 3D 5F 2C 3C 03 00' | = Cosina AF Zoom 28-80mm F3.5-5.6 MC Macro
> '07 3E 30 43 2D 35 03 00' | = Soligor AF Zoom 19-35mm 1:3.5-4.5 MC
> '07 40 2F 44 2C 34 03 02' | = Tamron AF 19-35mm f/3.5-4.5 (A10)
> '07 40 30 45 2D 35 03 02' | = Tamron AF 19-35mm f/3.5-4.5 (A10)
> '07 40 3C 5C 2C 35 03 00' | = Tokina AF 270 II (AF 28-70mm f/3.5-4.5)
> '07 40 3C 62 2C 34 03 00' | = AF Zoom-Nikkor 28-85mm f/3.5-4.5
> '07 46 2B 44 24 30 03 02' | = Tamron SP AF 17-35mm f/2.8-4 Di LD Aspherical (IF) (A05)
> '07 46 3D 6A 25 2F 03 00' | = Cosina AF Zoom 28-105mm F2.8-3.8 MC
> '07 47 3C 5C 25 35 03 00' | = Tokina AF 287 SD (AF 28-70mm f/2.8-4.5)
> '07 48 3C 5C 24 24 03 00' | = Tokina AT-X 287 AF (AF 28-70mm f/2.8)
> '08 40 44 6A 2C 34 04 00' | = AF Zoom-Nikkor 35-105mm f/3.5-4.5
> '09 48 37 37 24 24 04 00' | = AF Nikkor 24mm f/2.8
> '0A 48 8E 8E 24 24 03 00' | = AF Nikkor 300mm f/2.8 IF-ED
> '0A 48 8E 8E 24 24 05 00' | = AF Nikkor 300mm f/2.8 IF-ED N
> '0B 3E 3D 7F 2F 3D 0E 00' | = Tamron AF 28-200mm f/3.8-5.6 (71D)
> '0B 3E 3D 7F 2F 3D 0E 02' | = Tamron AF 28-200mm f/3.8-5.6D (171D)
> '0B 48 7C 7C 24 24 05 00' | = AF Nikkor 180mm f/2.8 IF-ED
> '0D 40 44 72 2C 34 07 00' | = AF Zoom-Nikkor 35-135mm f/3.5-4.5
> '0E 48 5C 81 30 30 05 00' | = AF Zoom-Nikkor 70-210mm f/4
> '0E 4A 31 48 23 2D 0E 02' | = Tamron SP AF 20-40mm f/2.7-3.5 (166D)
> '0F 58 50 50 14 14 05 00' | = AF Nikkor 50mm f/1.8 N
> '10 3D 3C 60 2C 3C D2 02' | = Tamron AF 28-80mm f/3.5-5.6 Aspherical (177D)
> '10 48 8E 8E 30 30 08 00' | = AF Nikkor 300mm f/4 IF-ED
> '11 48 44 5C 24 24 08 00' | = AF Zoom-Nikkor 35-70mm f/2.8
> '12 36 5C 81 35 3D 09 00' | = Cosina AF Zoom 70-210mm F4.5-5.6 MC Macro
> '12 36 69 97 35 42 09 00' | = Soligor AF Zoom 100-400mm 1:4.5-6.7 MC
> '12 39 5C 8E 34 3D 08 02' | = Cosina AF Zoom 70-300mm F4.5-5.6 MC Macro
> '12 3B 68 8D 3D 43 09 02' | = Cosina AF Zoom 100-300mm F5.6-6.7 MC Macro
> '12 3B 98 98 3D 3D 09 00' | = Tokina AT-X 400 AF SD (AF 400mm f/5.6)
> '12 3D 3C 80 2E 3C DF 02' | = Tamron AF 28-200mm f/3.8-5.6 AF Aspherical LD (IF) (271D)
> '12 44 5E 8E 34 3C 09 00' | = Tokina AF 730 (AF 75-300mm F4.5-5.6)
> '12 48 5C 81 30 3C 09 00' | = AF Nikkor 70-210mm f/4-5.6
> '12 4A 5C 81 31 3D 09 00' | = Soligor AF C/D Auto Zoom+Macro 70-210mm 1:4-5.6 UMCS
> '13 42 37 50 2A 34 0B 00' | = AF Zoom-Nikkor 24-50mm f/3.3-4.5
> '14 48 60 80 24 24 0B 00' | = AF Zoom-Nikkor 80-200mm f/2.8 ED
> '14 48 68 8E 30 30 0B 00' | = Tokina AT-X 340 AF (AF 100-300mm f/4)
> '14 54 60 80 24 24 0B 00' | = Tokina AT-X 828 AF (AF 80-200mm f/2.8)
> '15 4C 62 62 14 14 0C 00' | = AF Nikkor 85mm f/1.8
> '17 3C A0 A0 30 30 0F 00' | = Nikkor 500mm f/4 P ED IF
> '17 3C A0 A0 30 30 11 00' | = Nikkor 500mm f/4 P ED IF
> '18 40 44 72 2C 34 0E 00' | = AF Zoom-Nikkor 35-135mm f/3.5-4.5 N
> '1A 54 44 44 18 18 11 00' | = AF Nikkor 35mm f/2
> '1B 44 5E 8E 34 3C 10 00' | = AF Zoom-Nikkor 75-300mm f/4.5-5.6
> '1C 48 30 30 24 24 12 00' | = AF Nikkor 20mm f/2.8
> '1D 42 44 5C 2A 34 12 00' | = AF Zoom-Nikkor 35-70mm f/3.3-4.5 N
> '1E 54 56 56 24 24 13 00' | = AF Micro-Nikkor 60mm f/2.8
> '1E 5D 64 64 20 20 13 00' | = Tamron SP AF 90mm f/2.5 (52E)
> '1F 54 6A 6A 24 24 14 00' | = AF Micro-Nikkor 105mm f/2.8
> '20 3C 80 98 3D 3D 1E 02' | = Tamron AF 200-400mm f/5.6 LD IF (75D)
> '20 48 60 80 24 24 15 00' | = AF Zoom-Nikkor 80-200mm f/2.8 ED
> '20 5A 64 64 20 20 14 00' | = Tamron SP AF 90mm f/2.5 Macro (152E)
> '21 40 3C 5C 2C 34 16 00' | = AF Zoom-Nikkor 28-70mm f/3.5-4.5
> '21 56 8E 8E 24 24 14 00' | = Tamron SP AF 300mm f/2.8 LD-IF (60E)
> '22 48 72 72 18 18 16 00' | = AF DC-Nikkor 135mm f/2
> '22 53 64 64 24 24 E0 02' | = Tamron SP AF 90mm f/2.8 Macro 1:1 (72E)
> '23 30 BE CA 3C 48 17 00' | = Zoom-Nikkor 1200-1700mm f/5.6-8 P ED IF
> '24 44 60 98 34 3C 1A 02' | = Tokina AT-X 840 AF-II (AF 80-400mm f/4.5-5.6)
> '24 48 60 80 24 24 1A 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '24 54 60 80 24 24 1A 02' | = Tokina AT-X 828 AF PRO (AF 80-200mm f/2.8)
> '25 44 44 8E 34 42 1B 02' | = Tokina AF 353 (AF 35-300mm f/4.5-6.7)
> '25 48 3C 5C 24 24 1B 02.1' | = Tokina AT-X 270 AF PRO II (AF 28-70mm f/2.6-2.8)
> '25 48 3C 5C 24 24 1B 02.2' | = Tokina AT-X 287 AF PRO SV (AF 28-70mm f/2.8)
> '25 48 44 5C 24 24 1B 02' | = AF Zoom-Nikkor 35-70mm f/2.8D
> '25 48 44 5C 24 24 52 02' | = AF Zoom-Nikkor 35-70mm f/2.8D
> '26 3C 54 80 30 3C 1C 06' | = Sigma 55-200mm F4-5.6 DC
> '26 3C 5C 82 30 3C 1C 02' | = Sigma 70-210mm F4-5.6 UC-II
> '26 3C 5C 8E 30 3C 1C 02' | = Sigma 70-300mm F4-5.6 DG Macro
> '26 3C 98 98 3C 3C 1C 02' | = Sigma APO Tele Macro 400mm F5.6
> '26 3D 3C 80 2F 3D 1C 02' | = Sigma 28-300mm F3.8-5.6 Aspherical
> '26 3E 3C 6A 2E 3C 1C 02' | = Sigma 28-105mm F3.8-5.6 UC-III Aspherical IF
> '26 40 27 3F 2C 34 1C 02' | = Sigma 15-30mm F3.5-4.5 EX DG Aspherical DF
> '26 40 2D 44 2B 34 1C 02' | = Sigma 18-35 F3.5-4.5 Aspherical
> '26 40 2D 50 2C 3C 1C 06' | = Sigma 18-50mm F3.5-5.6 DC
> '26 40 2D 70 2B 3C 1C 06' | = Sigma 18-125mm F3.5-5.6 DC
> '26 40 2D 80 2C 40 1C 06' | = Sigma 18-200mm F3.5-6.3 DC
> '26 40 37 5C 2C 3C 1C 02' | = Sigma 24-70mm F3.5-5.6 Aspherical HF
> '26 40 3C 5C 2C 34 1C 02' | = AF Zoom-Nikkor 28-70mm f/3.5-4.5D
> '26 40 3C 60 2C 3C 1C 02' | = Sigma 28-80mm F3.5-5.6 Mini Zoom Macro II Aspherical
> '26 40 3C 65 2C 3C 1C 02' | = Sigma 28-90mm F3.5-5.6 Macro
> '26 40 3C 80 2B 3C 1C 02' | = Sigma 28-200mm F3.5-5.6 Compact Aspherical Hyperzoom Macro
> '26 40 3C 80 2C 3C 1C 02' | = Sigma 28-200mm F3.5-5.6 Compact Aspherical Hyperzoom Macro
> '26 40 3C 8E 2C 40 1C 02' | = Sigma 28-300mm F3.5-6.3 Macro
> '26 40 7B A0 34 40 1C 02' | = Sigma APO 170-500mm F5-6.3 Aspherical RF
> '26 41 3C 8E 2C 40 1C 02' | = Sigma 28-300mm F3.5-6.3 DG Macro
> '26 44 73 98 34 3C 1C 02' | = Sigma 135-400mm F4.5-5.6 APO Aspherical
> '26 48 11 11 30 30 1C 02' | = Sigma 8mm F4 EX Circular Fisheye
> '26 48 27 27 24 24 1C 02' | = Sigma 15mm F2.8 EX Diagonal Fisheye
> '26 48 2D 50 24 24 1C 06' | = Sigma 18-50mm F2.8 EX DC
> '26 48 31 49 24 24 1C 02' | = Sigma 20-40mm F2.8
> '26 48 37 56 24 24 1C 02' | = Sigma 24-60mm F2.8 EX DG
> '26 48 3C 5C 24 24 1C 06' | = Sigma 28-70mm F2.8 EX DG
> '26 48 3C 5C 24 30 1C 02' | = Sigma 28-70mm F2.8-4 DG
> '26 48 3C 6A 24 30 1C 02' | = Sigma 28-105mm F2.8-4 Aspherical
> '26 48 8E 8E 30 30 1C 02' | = Sigma APO Tele Macro 300mm F4
> '26 54 2B 44 24 30 1C 02' | = Sigma 17-35mm F2.8-4 EX Aspherical
> '26 54 37 5C 24 24 1C 02' | = Sigma 24-70mm F2.8 EX DG Macro
> '26 54 37 73 24 34 1C 02' | = Sigma 24-135mm F2.8-4.5
> '26 54 3C 5C 24 24 1C 02' | = Sigma 28-70mm F2.8 EX
> '26 58 31 31 14 14 1C 02' | = Sigma 20mm F1.8 EX DG Aspherical RF
> '26 58 37 37 14 14 1C 02' | = Sigma 24mm F1.8 EX DG Aspherical Macro
> '26 58 3C 3C 14 14 1C 02' | = Sigma 28mm F1.8 EX DG Aspherical Macro
> '27 48 8E 8E 24 24 1D 02' | = AF-I Nikkor 300mm f/2.8D IF-ED
> '27 48 8E 8E 24 24 E1 02' | = AF-I Nikkor 300mm f/2.8D IF-ED + TC-17E
> '27 48 8E 8E 24 24 F1 02' | = AF-I Nikkor 300mm f/2.8D IF-ED + TC-14E
> '27 48 8E 8E 24 24 F2 02' | = AF-I Nikkor 300mm f/2.8D IF-ED + TC-20E
> '27 48 8E 8E 30 30 1D 02' | = Tokina AT-X 304 AF (AF 300mm f/4.0)
> '27 54 8E 8E 24 24 1D 02' | = Tamron SP AF 300mm f/2.8 LD-IF (360E)
> '28 3C A6 A6 30 30 1D 02' | = AF-I Nikkor 600mm f/4D IF-ED
> '28 3C A6 A6 30 30 E1 02' | = AF-I Nikkor 600mm f/4D IF-ED + TC-17E
> '28 3C A6 A6 30 30 F1 02' | = AF-I Nikkor 600mm f/4D IF-ED + TC-14E
> '28 3C A6 A6 30 30 F2 02' | = AF-I Nikkor 600mm f/4D IF-ED + TC-20E
> '2A 54 3C 3C 0C 0C 26 02' | = AF Nikkor 28mm f/1.4D
> '2B 3C 44 60 30 3C 1F 02' | = AF Zoom-Nikkor 35-80mm f/4-5.6D
> '2C 48 6A 6A 18 18 27 02' | = AF DC-Nikkor 105mm f/2D
> '2D 48 80 80 30 30 21 02' | = AF Micro-Nikkor 200mm f/4D IF-ED
> '2E 48 5C 82 30 3C 22 02' | = AF Nikkor 70-210mm f/4-5.6D
> '2E 48 5C 82 30 3C 28 02' | = AF Nikkor 70-210mm f/4-5.6D
> '2F 40 30 44 2C 34 29 02.1' | = Tokina AF 235 II (AF 20-35mm f/3.5-4.5)
> '2F 40 30 44 2C 34 29 02.2' | = Tokina AF 193 (AF 19-35mm f/3.5-4.5)
> '2F 48 30 44 24 24 29 02.1' | = AF Zoom-Nikkor 20-35mm f/2.8D IF
> '2F 48 30 44 24 24 29 02.2' | = Tokina AT-X 235 AF PRO (AF 20-35mm f/2.8)
> '30 48 98 98 24 24 24 02' | = AF-I Nikkor 400mm f/2.8D IF-ED
> '30 48 98 98 24 24 E1 02' | = AF-I Nikkor 400mm f/2.8D IF-ED + TC-17E
> '30 48 98 98 24 24 F1 02' | = AF-I Nikkor 400mm f/2.8D IF-ED + TC-14E
> '30 48 98 98 24 24 F2 02' | = AF-I Nikkor 400mm f/2.8D IF-ED + TC-20E
> '31 54 56 56 24 24 25 02' | = AF Micro-Nikkor 60mm f/2.8D
> '32 53 64 64 24 24 35 02' | = Tamron SP AF 90mm f/2.8 [Di] Macro 1:1 (172E/272E)
> '32 54 50 50 24 24 35 02' | = Sigma Macro 50mm F2.8 EX DG
> '32 54 6A 6A 24 24 35 02.1' | = AF Micro-Nikkor 105mm f/2.8D
> '32 54 6A 6A 24 24 35 02.2' | = Sigma Macro 105mm F2.8 EX DG
> '33 48 2D 2D 24 24 31 02' | = AF Nikkor 18mm f/2.8D
> '33 54 3C 5E 24 24 62 02' | = Tamron SP AF 28-75mm f/2.8 XR Di LD Aspherical (IF) Macro (A09)
> '34 48 29 29 24 24 32 02' | = AF Fisheye Nikkor 16mm f/2.8D
> '35 3C A0 A0 30 30 33 02' | = AF-I Nikkor 500mm f/4D IF-ED
> '35 3C A0 A0 30 30 E1 02' | = AF-I Nikkor 500mm f/4D IF-ED + TC-17E
> '35 3C A0 A0 30 30 F1 02' | = AF-I Nikkor 500mm f/4D IF-ED + TC-14E
> '35 3C A0 A0 30 30 F2 02' | = AF-I Nikkor 500mm f/4D IF-ED + TC-20E
> '36 48 37 37 24 24 34 02' | = AF Nikkor 24mm f/2.8D
> '37 48 30 30 24 24 36 02' | = AF Nikkor 20mm f/2.8D
> '38 4C 62 62 14 14 37 02' | = AF Nikkor 85mm f/1.8D
> '3A 40 3C 5C 2C 34 39 02' | = AF Zoom-Nikkor 28-70mm f/3.5-4.5D
> '3B 48 44 5C 24 24 3A 02' | = AF Zoom-Nikkor 35-70mm f/2.8D N
> '3C 48 60 80 24 24 3B 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '3D 3C 44 60 30 3C 3E 02' | = AF Zoom-Nikkor 35-80mm f/4-5.6D
> '3E 48 3C 3C 24 24 3D 02' | = AF Nikkor 28mm f/2.8D
> '3F 40 44 6A 2C 34 45 02' | = AF Zoom-Nikkor 35-105mm f/3.5-4.5D
> '41 48 7C 7C 24 24 43 02' | = AF Nikkor 180mm f/2.8D IF-ED
> '42 54 44 44 18 18 44 02' | = AF Nikkor 35mm f/2D
> '43 54 50 50 0C 0C 46 02' | = AF Nikkor 50mm f/1.4D
> '44 44 60 80 34 3C 47 02' | = AF Zoom-Nikkor 80-200mm f/4.5-5.6D
> '45 3D 3C 60 2C 3C 48 02' | = Tamron AF 28-80mm f/3.5-5.6 Aspherical (177D)
> '45 40 3C 60 2C 3C 48 02' | = AF Zoom-Nikkor 28-80mm f/3.5-5.6D
> '45 41 37 72 2C 3C 48 02' | = Tamron SP AF 24-135mm f/3.5-5.6 AD Aspherical (IF) Macro (190D)
> '46 3C 44 60 30 3C 49 02' | = AF Zoom-Nikkor 35-80mm f/4-5.6D N
> '47 42 37 50 2A 34 4A 02' | = AF Zoom-Nikkor 24-50mm f/3.3-4.5D
> '48 38 1F 37 34 3C 4B 06' | = Sigma 12-24mm F4.5-5.6 EX DG Aspherical HSM
> '48 3C 19 31 30 3C 4B 06' | = Sigma 10-20mm F4-5.6 EX DC HSM
> '48 3C 50 A0 30 40 4B 02' | = Sigma 50-500mm F4-6.3 EX APO RF HSM
> '48 3C 8E B0 3C 3C 4B 02' | = Sigma APO 300-800mm F5.6 EX DG HSM
> '48 3C B0 B0 3C 3C 4B 02' | = Sigma APO 800mm F5.6 EX HSM
> '48 44 A0 A0 34 34 4B 02' | = Sigma APO 500mm F4.5 EX HSM
> '48 48 24 24 24 24 4B 02' | = Sigma 14mm F2.8 EX Aspherical HSM
> '48 48 2B 44 24 30 4B 06' | = Sigma 17-35mm F2.8-4 EX DG Aspherical HSM
> '48 48 68 8E 30 30 4B 02' | = Sigma 100-300mm F4 EX IF HSM
> '48 48 76 76 24 24 4B 06' | = Sigma 150mm F2.8 EX DG APO Macro HSM
> '48 48 8E 8E 24 24 4B 02' | = AF-S Nikkor 300mm f/2.8D IF-ED
> '48 48 8E 8E 24 24 E1 02' | = AF-S Nikkor 300mm f/2.8D IF-ED + TC-17E
> '48 48 8E 8E 24 24 F1 02' | = AF-S Nikkor 300mm f/2.8D IF-ED + TC-14E
> '48 48 8E 8E 24 24 F2 02' | = AF-S Nikkor 300mm f/2.8D IF-ED + TC-20E
> '48 4C 7C 7C 2C 2C 4B 02' | = Sigma 180mm F3.5 EX DG Macro
> '48 4C 7D 7D 2C 2C 4B 02' | = Sigma APO Macro 180mm F3.5 EX DG HSM
> '48 54 3E 3E 0C 0C 4B 06' | = Sigma 30mm F1.4 EX DC HSM
> '48 54 5C 80 24 24 4B 02' | = Sigma 70-200mm F2.8 EX APO IF HSM
> '48 54 6F 8E 24 24 4B 02' | = Sigma APO 120-300mm F2.8 EX DG HSM
> '48 54 8E 8E 24 24 4B 02' | = Sigma APO 300mm F2.8 EX DG HSM
> '49 3C A6 A6 30 30 4C 02' | = AF-S Nikkor 600mm f/4D IF-ED
> '49 3C A6 A6 30 30 E1 02' | = AF-S Nikkor 600mm f/4D IF-ED + TC-17E
> '49 3C A6 A6 30 30 F1 02' | = AF-S Nikkor 600mm f/4D IF-ED + TC-14E
> '49 3C A6 A6 30 30 F2 02' | = AF-S Nikkor 600mm f/4D IF-ED + TC-20E
> '4A 40 11 11 2C 0C 4D 02' | = Samyang 8mm f/3.5 Fish-Eye CS
> '4A 48 24 24 24 0C 4D 02' | = Samyang AE 14mm f/2.8 ED AS IF UMC
> '4A 54 62 62 0C 0C 4D 02' | = AF Nikkor 85mm f/1.4D IF
> '4A 60 44 44 0C 0C 4D 02' | = Samyang 35mm f/1.4 AS UMC
> '4A 60 62 62 0C 0C 4D 02' | = Samyang AE 85mm f/1.4 AS IF UMC
> '4B 3C A0 A0 30 30 4E 02' | = AF-S Nikkor 500mm f/4D IF-ED
> '4B 3C A0 A0 30 30 E1 02' | = AF-S Nikkor 500mm f/4D IF-ED + TC-17E
> '4B 3C A0 A0 30 30 F1 02' | = AF-S Nikkor 500mm f/4D IF-ED + TC-14E
> '4B 3C A0 A0 30 30 F2 02' | = AF-S Nikkor 500mm f/4D IF-ED + TC-20E
> '4C 40 37 6E 2C 3C 4F 02' | = AF Zoom-Nikkor 24-120mm f/3.5-5.6D IF
> '4D 40 3C 80 2C 3C 62 02' | = AF Zoom-Nikkor 28-200mm f/3.5-5.6D IF
> '4D 41 3C 8E 2B 40 62 02' | = Tamron AF 28-300mm f/3.5-6.3 XR Di LD Aspherical (IF) (A061)
> '4D 41 3C 8E 2C 40 62 02' | = Tamron AF 28-300mm f/3.5-6.3 XR LD Aspherical (IF) (185D)
> '4E 48 72 72 18 18 51 02' | = AF DC-Nikkor 135mm f/2D
> '4F 40 37 5C 2C 3C 53 06' | = IX-Nikkor 24-70mm f/3.5-5.6
> '50 48 56 7C 30 3C 54 06' | = IX-Nikkor 60-180mm f/4-5.6
> '53 48 60 80 24 24 57 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '53 48 60 80 24 24 60 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '54 44 5C 7C 34 3C 58 02' | = AF Zoom-Micro Nikkor 70-180mm f/4.5-5.6D ED
> '54 44 5C 7C 34 3C 61 02' | = AF Zoom-Micro Nikkor 70-180mm f/4.5-5.6D ED
> '56 3C 5C 8E 30 3C 1C 02' | = Sigma 70-300mm F4-5.6 APO Macro Super II
> '56 48 5C 8E 30 3C 5A 02' | = AF Zoom-Nikkor 70-300mm f/4-5.6D ED
> '59 48 98 98 24 24 5D 02' | = AF-S Nikkor 400mm f/2.8D IF-ED
> '59 48 98 98 24 24 E1 02' | = AF-S Nikkor 400mm f/2.8D IF-ED + TC-17E
> '59 48 98 98 24 24 F1 02' | = AF-S Nikkor 400mm f/2.8D IF-ED + TC-14E
> '59 48 98 98 24 24 F2 02' | = AF-S Nikkor 400mm f/2.8D IF-ED + TC-20E
> '5A 3C 3E 56 30 3C 5E 06' | = IX-Nikkor 30-60mm f/4-5.6
> '5B 44 56 7C 34 3C 5F 06' | = IX-Nikkor 60-180mm f/4.5-5.6
> '5D 48 3C 5C 24 24 63 02' | = AF-S Zoom-Nikkor 28-70mm f/2.8D IF-ED
> '5E 48 60 80 24 24 64 02' | = AF-S Zoom-Nikkor 80-200mm f/2.8D IF-ED
> '5F 40 3C 6A 2C 34 65 02' | = AF Zoom-Nikkor 28-105mm f/3.5-4.5D IF
> '60 40 3C 60 2C 3C 66 02' | = AF Zoom-Nikkor 28-80mm f/3.5-5.6D
> '61 44 5E 86 34 3C 67 02' | = AF Zoom-Nikkor 75-240mm f/4.5-5.6D
> '63 48 2B 44 24 24 68 02' | = AF-S Nikkor 17-35mm f/2.8D IF-ED
> '64 00 62 62 24 24 6A 02' | = PC Micro-Nikkor 85mm f/2.8D
> '65 44 60 98 34 3C 6B 0A' | = AF VR Zoom-Nikkor 80-400mm f/4.5-5.6D ED
> '66 40 2D 44 2C 34 6C 02' | = AF Zoom-Nikkor 18-35mm f/3.5-4.5D IF-ED
> '67 48 37 62 24 30 6D 02' | = AF Zoom-Nikkor 24-85mm f/2.8-4D IF
> '67 54 37 5C 24 24 1C 02' | = Sigma 24-70mm F2.8 EX DG Macro
> '68 42 3C 60 2A 3C 6E 06' | = AF Zoom-Nikkor 28-80mm f/3.3-5.6G
> '69 47 5C 8E 30 3C 00 02' | = Tamron AF 70-300mm f/4-5.6 Di LD Macro 1:2 (A17N)
> '69 48 5C 8E 30 3C 6F 02' | = Tamron AF 70-300mm f/4-5.6 LD Macro 1:2 (772D)
> '69 48 5C 8E 30 3C 6F 06' | = AF Zoom-Nikkor 70-300mm f/4-5.6G
> '6A 48 8E 8E 30 30 70 02' | = AF-S Nikkor 300mm f/4D IF-ED
> '6B 48 24 24 24 24 71 02' | = AF Nikkor ED 14mm f/2.8D
> '6D 48 8E 8E 24 24 73 02' | = AF-S Nikkor 300mm f/2.8D IF-ED II
> '6E 48 98 98 24 24 74 02' | = AF-S Nikkor 400mm f/2.8D IF-ED II
> '6F 3C A0 A0 30 30 75 02' | = AF-S Nikkor 500mm f/4D IF-ED II
> '70 3C A6 A6 30 30 76 02' | = AF-S Nikkor 600mm f/4D IF-ED II
> '72 48 4C 4C 24 24 77 00' | = Nikkor 45mm f/2.8 P
> '74 40 37 62 2C 34 78 06' | = AF-S Zoom-Nikkor 24-85mm f/3.5-4.5G IF-ED
> '75 40 3C 68 2C 3C 79 06' | = AF Zoom-Nikkor 28-100mm f/3.5-5.6G
> '76 58 50 50 14 14 7A 02' | = AF Nikkor 50mm f/1.8D
> '77 44 61 98 34 3C 7B 0E' | = Sigma 80-400mm F4.5-5.6 EX OS
> '77 48 5C 80 24 24 7B 0E' | = AF-S VR Zoom-Nikkor 70-200mm f/2.8G IF-ED
> '78 40 37 6E 2C 3C 7C 0E' | = AF-S VR Zoom-Nikkor 24-120mm f/3.5-5.6G IF-ED
> '79 40 11 11 2C 2C 1C 06' | = Sigma 8mm F3.5 EX Circular Fisheye
> '79 40 3C 80 2C 3C 7F 06' | = AF Zoom-Nikkor 28-200mm f/3.5-5.6G IF-ED
> '79 48 5C 5C 24 24 1C 06' | = Sigma Macro 70mm F2.8 EX DG
> '7A 3B 53 80 30 3C 4B 06' | = Sigma 55-200mm F4-5.6 DC HSM
> '7A 3C 1F 37 30 30 7E 06.1' | = AF-S DX Zoom-Nikkor 12-24mm f/4G IF-ED
> '7A 3C 1F 37 30 30 7E 06.2' | = Tokina AT-X 124 AF PRO DX II (AF 12-24mm f/4)
> '7A 40 2D 50 2C 3C 4B 06' | = Sigma 18-50mm F3.5-5.6 DC HSM
> '7A 40 2D 80 2C 40 4B 0E' | = Sigma 18-200mm F3.5-6.3 DC OS HSM
> '7A 47 2B 5C 24 34 4B 06' | = Sigma 17-70mm F2.8-4.5 DC Macro Asp. IF HSM
> '7A 47 50 76 24 24 4B 06' | = Sigma 50-150mm F2.8 EX APO DC HSM
> '7A 48 2B 5C 24 34 4B 06' | = Sigma 17-70mm F2.8-4.5 DC Macro Asp. IF HSM
> '7A 48 2D 50 24 24 4B 06' | = Sigma 18-50mm F2.8 EX DC Macro
> '7A 48 5C 80 24 24 4B 06' | = Sigma 70-200mm F2.8 EX APO DG Macro HSM II
> '7A 54 6E 8E 24 24 4B 02' | = Sigma APO 120-300mm F2.8 EX DG HSM
> '7B 48 80 98 30 30 80 0E' | = AF-S VR Zoom-Nikkor 200-400mm f/4G IF-ED
> '7D 48 2B 53 24 24 82 06' | = AF-S DX Zoom-Nikkor 17-55mm f/2.8G IF-ED
> '7F 40 2D 5C 2C 34 84 06' | = AF-S DX Zoom-Nikkor 18-70mm f/3.5-4.5G IF-ED
> '7F 48 2B 5C 24 34 1C 06' | = Sigma 17-70mm F2.8-4.5 DC Macro Asp. IF
> '7F 48 2D 50 24 24 1C 06' | = Sigma 18-50mm F2.8 EX DC Macro
> '80 48 1A 1A 24 24 85 06' | = AF DX Fisheye-Nikkor 10.5mm f/2.8G ED
> '81 54 80 80 18 18 86 0E' | = AF-S VR Nikkor 200mm f/2G IF-ED
> '82 48 8E 8E 24 24 87 0E' | = AF-S VR Nikkor 300mm f/2.8G IF-ED
> '83 00 B0 B0 5A 5A 88 04' | = FSA-L2, EDG 65, 800mm F13 G
> '89 3C 53 80 30 3C 8B 06' | = AF-S DX Zoom-Nikkor 55-200mm f/4-5.6G ED
> '8A 54 6A 6A 24 24 8C 0E' | = AF-S VR Micro-Nikkor 105mm f/2.8G IF-ED
> '8B 40 2D 80 2C 3C 8D 0E' | = AF-S DX VR Zoom-Nikkor 18-200mm f/3.5-5.6G IF-ED
> '8B 40 2D 80 2C 3C FD 0E' | = AF-S DX VR Zoom-Nikkor 18-200mm f/3.5-5.6G IF-ED [II]
> '8C 40 2D 53 2C 3C 8E 06' | = AF-S DX Zoom-Nikkor 18-55mm f/3.5-5.6G ED
> '8D 44 5C 8E 34 3C 8F 0E' | = AF-S VR Zoom-Nikkor 70-300mm f/4.5-5.6G IF-ED
> '8F 40 2D 72 2C 3C 91 06' | = AF-S DX Zoom-Nikkor 18-135mm f/3.5-5.6G IF-ED
> '90 3B 53 80 30 3C 92 0E' | = AF-S DX VR Zoom-Nikkor 55-200mm f/4-5.6G IF-ED
> '92 2C 2D 88 2C 40 4B 0E' | = Sigma 18-250mm F3.5-6.3 DC Macro OS HSM
> '92 48 24 37 24 24 94 06' | = AF-S Zoom-Nikkor 14-24mm f/2.8G ED
> '93 48 37 5C 24 24 95 06' | = AF-S Zoom-Nikkor 24-70mm f/2.8G ED
> '94 40 2D 53 2C 3C 96 06' | = AF-S DX Zoom-Nikkor 18-55mm f/3.5-5.6G ED II
> '95 00 37 37 2C 2C 97 06' | = PC-E Nikkor 24mm f/3.5D ED
> '95 4C 37 37 2C 2C 97 02' | = PC-E Nikkor 24mm f/3.5D ED
> '96 48 98 98 24 24 98 0E' | = AF-S VR Nikkor 400mm f/2.8G ED
> '97 3C A0 A0 30 30 99 0E' | = AF-S VR Nikkor 500mm f/4G ED
> '98 3C A6 A6 30 30 9A 0E' | = AF-S VR Nikkor 600mm f/4G ED
> '99 40 29 62 2C 3C 9B 0E' | = AF-S DX VR Zoom-Nikkor 16-85mm f/3.5-5.6G ED
> '9A 40 2D 53 2C 3C 9C 0E' | = AF-S DX VR Zoom-Nikkor 18-55mm f/3.5-5.6G
> '9B 00 4C 4C 24 24 9D 06' | = PC-E Micro Nikkor 45mm f/2.8D ED
> '9B 54 4C 4C 24 24 9D 02' | = PC-E Micro Nikkor 45mm f/2.8D ED
> '9B 54 62 62 0C 0C 4B 06' | = Sigma 85mm F1.4 EX DG HSM
> '9C 48 5C 80 24 24 4B 0E' | = Sigma 70-200mm F2.8 EX DG OS HSM
> '9C 54 56 56 24 24 9E 06' | = AF-S Micro Nikkor 60mm f/2.8G ED
> '9D 00 62 62 24 24 9F 06' | = PC-E Micro Nikkor 85mm f/2.8D
> '9D 48 2B 50 24 24 4B 0E' | = Sigma 17-50mm F2.8 EX DC OS HSM
> '9D 54 62 62 24 24 9F 02' | = PC-E Micro Nikkor 85mm f/2.8D
> '9E 38 11 29 34 3C 4B 06' | = Sigma 8-16mm F4.5-5.6 DC HSM
> '9E 40 2D 6A 2C 3C A0 0E' | = AF-S DX VR Zoom-Nikkor 18-105mm f/3.5-5.6G ED
> '9F 37 50 A0 34 40 4B 0E' | = Sigma 50-500mm F4.5-6.3 DG OS HSM
> '9F 58 44 44 14 14 A1 06' | = AF-S DX Nikkor 35mm f/1.8G
> 'A0 54 50 50 0C 0C A2 06' | = AF-S Nikkor 50mm f/1.4G
> 'A1 40 18 37 2C 34 A3 06' | = AF-S DX Nikkor 10-24mm f/3.5-4.5G ED
> 'A1 41 19 31 2C 2C 4B 06' | = Sigma 10-20mm F3.5 EX DC HSM
> 'A2 48 5C 80 24 24 A4 0E' | = AF-S Nikkor 70-200mm f/2.8G ED VR II
> 'A3 3C 29 44 30 30 A5 0E' | = AF-S Nikkor 16-35mm f/4G ED VR
> 'A3 3C 5C 8E 30 3C 4B 0E' | = Sigma 70-300mm F4-5.6 DG OS
> 'A4 47 2D 50 24 34 4B 0E' | = Sigma 18-50mm F2.8-4.5 DC OS HSM
> 'A4 54 37 37 0C 0C A6 06' | = AF-S Nikkor 24mm f/1.4G ED
> 'A5 40 2D 88 2C 40 4B 0E' | = Sigma 18-250mm F3.5-6.3 DC OS HSM
> 'A5 40 3C 8E 2C 3C A7 0E' | = AF-S Nikkor 28-300mm f/3.5-5.6G ED VR
> 'A6 48 37 5C 24 24 4B 06' | = Sigma 24-70mm F2.8 IF EX DG HSM
> 'A6 48 8E 8E 24 24 A8 0E' | = AF-S VR Nikkor 300mm f/2.8G IF-ED II
> 'A7 49 80 A0 24 24 4B 06' | = Sigma APO 200-500mm F2.8 EX DG
> 'A7 4B 62 62 2C 2C A9 0E' | = AF-S DX Micro Nikkor 85mm f/3.5G ED VR
> 'A8 48 80 98 30 30 AA 0E' | = AF-S VR Zoom-Nikkor 200-400mm f/4G IF-ED II
> 'A9 54 80 80 18 18 AB 0E' | = AF-S Nikkor 200mm f/2G ED VR II
> 'AA 3C 37 6E 30 30 AC 0E' | = AF-S Nikkor 24-120mm f/4G ED VR
> 'AC 38 53 8E 34 3C AE 0E' | = AF-S DX VR Nikkor 55-300mm 4.5-5.6G ED
> 'AD 3C 2D 8E 2C 3C AF 0E' | = AF-S DX Nikkor 18-300mm 3.5-5.6G ED VR
> 'AE 54 62 62 0C 0C B0 06' | = AF-S Nikkor 85mm f/1.4G
> 'AF 54 44 44 0C 0C B1 06' | = AF-S Nikkor 35mm f/1.4G
> 'B0 4C 50 50 14 14 B2 06' | = AF-S Nikkor 50mm f/1.8G
> 'B1 48 48 48 24 24 B3 06' | = AF-S DX Micro Nikkor 40mm f/2.8G
> 'B2 48 5C 80 30 30 B4 0E' | = AF-S Nikkor 70-200mm f/4G ED VR
> 'B3 4C 62 62 14 14 B5 06' | = AF-S Nikkor 85mm f/1.8G
> 'B4 40 37 62 2C 34 B6 0E' | = AF-S VR Zoom-Nikkor 24-85mm f/3.5-4.5G IF-ED
> 'B5 4C 3C 3C 14 14 B7 06' | = AF-S Nikkor 28mm f/1.8G
> 'B6 48 37 56 24 24 1C 02' | = Sigma 24-60mm F2.8 EX DG
> 'B7 44 60 98 34 3C B9 0E' | = AF-S Nikkor 80-400mm f/4.5-5.6G ED VR
> 'CD 3D 2D 70 2E 3C 4B 0E' | = Sigma 18-125mm F3.8-5.6 DC OS HSM
> 'CE 34 76 A0 38 40 4B 0E' | = Sigma 150-500mm F5-6.3 DG OS APO HSM
> 'CF 38 6E 98 34 3C 4B 0E' | = Sigma APO 120-400mm F4.5-5.6 DG OS HSM
> 'DC 48 19 19 24 24 4B 06' | = Sigma 10mm F2.8 EX DC HSM Fisheye
> 'DE 54 50 50 0C 0C 4B 06' | = Sigma 50mm F1.4 EX DG HSM
> 'E0 3C 5C 8E 30 3C 4B 06' | = Sigma 70-300mm F4-5.6 APO DG Macro HSM
> 'E1 58 37 37 14 14 1C 02' | = Sigma 24mm F1.8 EX DG Aspherical Macro
> 'E3 54 50 50 24 24 35 02' | = Sigma Macro 50mm F2.8 EX DG
> 'E5 54 6A 6A 24 24 35 02' | = Sigma Macro 105mm F2.8 EX DG
> 'E6 41 3C 8E 2C 40 1C 02' | = Sigma 28-300mm F3.5-6.3 DG Macro
> 'E9 54 37 5C 24 24 1C 02' | = Sigma 24-70mm F2.8 EX DG Macro
> 'ED 40 2D 80 2C 40 4B 0E' | = Sigma 18-200mm F3.5-6.3 DC OS HSM
> 'EE 48 5C 80 24 24 4B 06' | = Sigma 70-200mm F2.8 EX APO DG Macro HSM II
> 'F0 38 1F 37 34 3C 4B 06' | = Sigma 12-24mm F4.5-5.6 EX DG Aspherical HSM
> 'F0 3F 2D 8A 2C 40 DF 0E' | = Tamron AF 18-270mm f/3.5-6.3 Di II VC PZD (B008)
> 'F1 44 A0 A0 34 34 4B 02' | = Sigma APO 500mm F4.5 EX DG HSM
> 'F1 47 5C 8E 30 3C DF 0E' | = Tamron SP 70-300mm f/4-5.6 Di VC USD (A005)
> 'F3 48 68 8E 30 30 4B 02' | = Sigma APO 100-300mm F4 EX IF HSM
> 'F3 54 2B 50 24 24 84 0E' | = Tamron SP AF 17-50mm f/2.8 XR Di II VC LD Aspherical (IF) (B005)
> 'F4 54 56 56 18 18 84 06' | = Tamron SP AF 60mm f/2.0 Di II Macro 1:1 (G005)
> 'F5 40 2C 8A 2C 40 40 0E' | = Tamron AF 18-270mm f/3.5-6.3 Di II VC LD Aspherical (IF) Macro (B003)
> 'F5 48 76 76 24 24 4B 06' | = Sigma 150mm F2.8 EX DG APO Macro HSM
> 'F6 3F 18 37 2C 34 84 06' | = Tamron SP AF 10-24mm f/3.5-4.5 Di II LD Aspherical (IF) (B001)
> 'F6 48 2D 50 24 24 4B 06' | = Sigma 18-50mm F2.8 EX DC Macro
> 'F7 53 5C 80 24 24 40 06' | = Tamron SP AF 70-200mm f/2.8 Di LD (IF) Macro (A001)
> 'F7 53 5C 80 24 24 84 06' | = Tamron SP AF 70-200mm f/2.8 Di LD (IF) Macro (A001)
> 'F8 54 3E 3E 0C 0C 4B 06' | = Sigma 30mm F1.4 EX DC HSM
> 'F8 54 64 64 24 24 DF 06' | = Tamron SP AF 90mm f/2.8 Di Macro 1:1 (272NII)
> 'F8 55 64 64 24 24 84 06' | = Tamron SP AF 90mm f/2.8 Di Macro 1:1 (272NII)
> 'F9 3C 19 31 30 3C 4B 06' | = Sigma 10-20mm F4-5.6 EX DC HSM
> 'F9 40 3C 8E 2C 40 40 0E' | = Tamron AF 28-300mm f/3.5-6.3 XR Di VC LD Aspherical (IF) Macro (A20)
> 'FA 54 3C 5E 24 24 84 06' | = Tamron SP AF 28-75mm f/2.8 XR Di LD Aspherical (IF) Macro (A09NII)
> 'FA 54 3C 5E 24 24 DF 06' | = Tamron SP AF 28-75mm F/2.8 XR Di LD Aspherical (IF) Macro (A09NII)
> 'FA 54 6E 8E 24 24 4B 02' | = Sigma APO 120-300mm F2.8 EX DG HSM
> 'FB 54 2B 50 24 24 84 06' | = Tamron SP AF 17-50mm f/2.8 XR Di II LD Aspherical (IF) (A16NII)
> 'FB 54 8E 8E 24 24 4B 02' | = Sigma APO 300mm F2.8 EX DG HSM
> 'FC 40 2D 80 2C 40 DF 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) Macro (A14NII)
> 'FD 47 50 76 24 24 4B 06' | = Sigma 50-150mm F2.8 EX APO DC HSM II
> 'FE 47 00 00 24 24 4B 06' | = Sigma 4.5mm F2.8 EX DC HSM Circular Fisheye
> 'FE 48 37 5C 24 24 DF 0E' | = Tamron SP 24-70mm f/2.8 Di VC USD
> 'FE 53 5C 80 24 24 84 06' | = Tamron SP AF 70-200mm f/2.8 Di LD (IF) Macro (A001)

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised May 13, 2013

<-- ExifTool Tag Names