## Kodak Tags

Many Kodak models don't store the maker notes in standard IFD format, and these formats vary with different models. Some information has been decoded, but much of the Kodak information remains unknown.

The table below contains the most common set of Kodak tags. The following Kodak camera models have been tested and found to use these tags: C360, C663, C875, CX6330, CX6445, CX7330, CX7430, CX7525, CX7530, DC4800, DC4900, DX3500, DX3600, DX3900, DX4330, DX4530, DX4900, DX6340, DX6440, DX6490, DX7440, DX7590, DX7630, EasyShare-One, LS420, LS443, LS633, LS743, LS753, V530, V550, V570, V603, V610, V705, Z650, Z700, Z710, Z730, Z740, Z760 and Z7590.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | KodakModel | string[8] |
> 9 | Quality | int8u | 1 = Fine 2 = Normal
> 10 | BurstMode | int8u | 0 = Off 1 = On
> 12 | KodakImageWidth | int16u |
> 14 | KodakImageHeight | int16u |
> 16 | YearCreated | int16u |
> 18 | MonthDayCreated | int8u[2] |
> 20 | TimeCreated | int8u[4] |
> 24 | BurstMode2? | int16u |
> 27 | ShutterMode | int8u | 0 = Auto 8 = Aperture Priority 32 = Manual?
> 28 | MeteringMode | int8u | 0 = Multi-segment 1 = Center-weighted average 2 = Spot
> 29 | SequenceNumber | int8u |
> 30 | FNumber | int16u |
> 32 | ExposureTime | int32u |
> 36 | ExposureCompensation | int16s |
> 38 | VariousModes? | int16u |
> 40 | Distance1? | int32u |
> 44 | Distance2? | int32u |
> 48 | Distance3? | int32u |
> 52 | Distance4? | int32u |
> 56 | FocusMode | int8u | 0 = Normal 2 = Macro
> 58 | VariousModes2? | int16u |
> 60 | PanoramaMode? | int16u |
> 62 | SubjectDistance? | int16u |
> 64 | WhiteBalance | int8u | 0 = Auto 1 = Flash? 2 = Tungsten 3 = Daylight

> 92

> FlashMode

> int8u

> 0x0 = Auto 0x1 = Fill Flash 0x2 = Off 0x3 = Red-Eye |  | 0x10 = Fill Flash 0x20 = Off 0x40 = Red-Eye? |

> 93 | FlashFired | int8u | 0 = No 1 = Yes
> 94 | ISOSetting | int16u |
> 96 | ISO | int16u |
> 98 | TotalZoom | int16u |
> 100 | DateTimeStamp | int16u |

> 102

> ColorMode

> int16u

> 0x1 = B&W 0x2 = Sepia 0x3 = B&W Yellow Filter 0x4 = B&W Red Filter 0x20 = Saturated Color |  | 0x40 = Neutral Color 0x100 = Saturated Color 0x200 = Neutral Color 0x2000 = B&W 0x4000 = Sepia |

> 104 | DigitalZoom | int16u |
> 107 | Sharpness | int8s | 0 = Normal

## Kodak Type2 Tags

These tags are used by the Kodak DC220, DC260, DC265 and DC290, Hewlett-Packard PhotoSmart 618, C500 and C912, Pentax EI-200 and EI-2000, and Minolta EX1500Z.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 8 | KodakMaker | string[32] |
> 40 | KodakModel | string[32] |
> 108 | KodakImageWidth | int32u |
> 112 | KodakImageHeight | int32u |

## Kodak Type3 Tags

These tags are used by the DC240, DC280, DC3400 and DC5000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | YearCreated | int16u |
> 14 | MonthDayCreated | int8u[2] |
> 16 | TimeCreated | int8u[4] |
> 30 | OpticalZoom | int16u |
> 55 | Sharpness | int8s | 0 = Normal
> 56 | ExposureTime | int32u |
> 60 | FNumber | int16u |
> 78 | ISO | int16u |

## Kodak Type4 Tags

These tags are used by the DC200 and DC215.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 32 | OriginalFileName | string[12] |

## Kodak Type5 Tags

These tags are used by the CX4200, CX4210, CX4230, CX4300, CX4310, CX6200 and CX6230.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 20 | ExposureTime | int32u |
> 26 | WhiteBalance | int8u | 1 = Daylight 2 = Flash 3 = Tungsten
> 28 | FNumber | int16u |
> 30 | ISO | int16u |
> 32 | OpticalZoom | int16u |
> 34 | DigitalZoom | int16u |
> 39 | FlashMode | int8u | 0 = Auto 1 = On 2 = Off 3 = Red-Eye
> 42 | ImageRotated | int8u | 0 = No 1 = Yes
> 43 | Macro | int8u | 0 = On 1 = Off

## Kodak Type6 Tags

These tags are used by the DX3215 and DX3700.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 16 | ExposureTime | int32u |
> 20 | ISOSetting? | int32u |
> 24 | FNumber | int16u |
> 26 | ISO | int16u |
> 28 | OpticalZoom | int16u |
> 30 | DigitalZoom | int16u |
> 34 | Flash | int16u | 0 = No Flash 1 = Fired

## Kodak Type7 Tags

The maker notes of models such as the C340, C433, CC533, LS755, V803 and V1003 seem to start with the camera serial number. The C310, C315, C330, C643, C743, CD33, CD43, CX7220 and CX7300 maker notes are also decoded using this table, although the strings for these cameras don't conform to the usual Kodak serial number format, and instead have the model name followed by 8 digits.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SerialNumber | string[16] |

## Kodak Type8 Tags

Kodak models such as the ZD710, P712, P850, P880, V1233, V1253, V1275, V1285, Z612, Z712, Z812, Z885 use standard TIFF IFD format for the maker notes. In keeping with Kodak's strategy of inconsistent makernotes, models such as the M380, M1033, M1093, V1073, V1273, Z1012, Z1085 and Z8612 also use these tags, but these makernotes begin with a TIFF header instead of an IFD entry count and use relative instead of absolute offsets. There is a large amount of information stored in these maker notes (apparently with much duplication), but relatively few tags have so far been decoded.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0xfc00 | SubIFD0 | - | --> Kodak SubIFD0 Tags --> Kodak SubIFD0 Tags
> 0xfc01 | SubIFD1 | - | --> Kodak SubIFD1 Tags --> Kodak SubIFD1 Tags
> 0xfc02 | SubIFD2 | - | --> Kodak SubIFD2 Tags --> Kodak SubIFD2 Tags
> 0xfc03 | SubIFD3 | - | --> Kodak SubIFD3 Tags --> Kodak SubIFD3 Tags
> 0xfc04 | SubIFD4 | - | --> Kodak SubIFD4 Tags --> Kodak SubIFD4 Tags
> 0xfc05 | SubIFD5 | - | --> Kodak SubIFD5 Tags --> Kodak SubIFD5 Tags
> 0xfc06 | SubIFD6 | - | --> Kodak SubIFD6 Tags --> Kodak SubIFD6 Tags
> 0xfcff | SubIFD255 | - | --> Kodak SubIFD0 Tags
> 0xff00 | CameraInfo | - | --> Kodak CameraInfo Tags

## Kodak SubIFD0 Tags

SubIFD0 through SubIFD5 tags are written a number of newer Kodak models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0xfa02

> SceneMode

> int16u

> (may not be valid for some models)

> 1 = Sport
> 3 = Portrait
> 4 = Landscape
> 6 = Beach
> 7 = Night Portrait
> 8 = Night Landscape
> 9 = Snow
> 10 = Text
> 11 = Fireworks
> 12 = Macro
> 13 = Museum
> 16 = Children

> 17 = Program
> 18 = Aperture Priority
> 19 = Shutter Priority
> 20 = Manual
> 25 = Back Light
> 28 = Candlelight
> 29 = Sunset
> 31 = Panorama Left-Right
> 32 = Panorama Right-Left
> 33 = Smart Scene
> 34 = High ISO

> 0xfa19 | SerialNumber | string |
> 0xfa1d | KodakImageWidth | int16u |
> 0xfa1e | KodakImageHeight | int16u |
> 0xfa20 | SensorWidth | int16u |
> 0xfa21 | SensorHeight | int16u |
> 0xfa23 | FNumber | int16u |
> 0xfa24 | ExposureTime | int32u |
> 0xfa2e | ISO | int16u |
> 0xfa3d | OpticalZoom | int16u |
> 0xfa46 | ISO | int16u |
> 0xfa51 | KodakImageWidth | int16u |
> 0xfa52 | KodakImageHeight | int16u |
> 0xfa54 | ThumbnailWidth | int16u |
> 0xfa55 | ThumbnailHeight | int16u |
> 0xfa57 | PreviewImageWidth | int16u |
> 0xfa58 | PreviewImageHeight | int16u |

## Kodak SubIFD1 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0027 | ISO | int16u |
> 0x0028 | ISO | int16u |

## Kodak SubIFD2 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 0x6002

> SceneModeUsed

> int32u

> 0 = Program
> 2 = Aperture Priority
> 3 = Shutter Priority
> 4 = Manual
> 5 = Portrait
> 6 = Sport
> 7 = Children
> 8 = Museum
> 10 = High ISO
> 11 = Text
> 12 = Macro

> 13 = Back Light
> 16 = Landscape
> 17 = Night Landscape
> 18 = Night Portrait
> 19 = Snow
> 20 = Beach
> 21 = Fireworks
> 22 = Sunset
> 23 = Candlelight
> 28 = Panorama

> 0x6006 | OpticalZoom | int32u |
> 0x6103 | MaxAperture | int32u |

> 0xf002

> SceneModeUsed

> int32u

> 0 = Program
> 2 = Aperture Priority
> 3 = Shutter Priority
> 4 = Manual
> 5 = Portrait
> 6 = Sport
> 7 = Children
> 8 = Museum
> 10 = High ISO
> 11 = Text
> 12 = Macro

> 13 = Back Light
> 16 = Landscape
> 17 = Night Landscape
> 18 = Night Portrait
> 19 = Snow
> 20 = Beach
> 21 = Fireworks
> 22 = Sunset
> 23 = Candlelight
> 28 = Panorama

> 0xf006 | OpticalZoom | int32u |
> 0xf103 | FNumber | int32u |
> 0xf104 | ExposureTime | int32u |
> 0xf105 | ISO | int32u |

## Kodak SubIFD3 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x1000 | OpticalZoom | int16u |

## Kodak SubIFD4 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Kodak SubIFD5 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x000f | OpticalZoom | int16u |

## Kodak SubIFD6 Tags

SubIFD6 is written by the M580.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Kodak CameraInfo Tags

These tags are used by the P712, P850 and P880.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0xf900 | SensorWidth | int16u | (effective sensor size)
> 0xf901 | SensorHeight | int16u |
> 0xf902 | BayerPattern | string |
> 0xf903 | SensorFullWidth | int16u | (includes black border?)
> 0xf904 | SensorFullHeight | int16u |
> 0xf907 | KodakImageWidth | int16u |
> 0xf908 | KodakImageHeight | int16u |
> 0xfa00 | KodakInfoType | string |
> 0xfa04 | SerialNumber | string |
> 0xfd04 | FNumber | int16u |
> 0xfd05 | ExposureTime | int32u |
> 0xfd06 | ISO | int16u |

## Kodak Type9 Tags

These tags are used by the Kodak C140, C180, C913, C1013, M320, M340 and M550, as well as various cameras marketed by other manufacturers.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | FNumber | int16u |
> 16 | ExposureTime | int32u |
> 20 | DateTimeOriginal | string[20] |
> 52 | ISO | int16u |
> 87 | FirmwareVersion | string[16] | (Kodak only)
> 168 | UnknownNumber | N | (Kodak only)
> 196 | UnknownNumber | N | (Kodak only)

## Kodak Type10 Tags

Another variation of the IFD-format type, this time with just a byte order indicator instead of a full TIFF header. These tags are used by the Z980.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | PreviewImageSize | int16u[2] |
> 0x0012 | ExposureTime | int32u |
> 0x0013 | FNumber | int16u |
> 0x0014 | ISO | int16u |
> 0x001d | FocalLength | int32u |

## Kodak Unknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Kodak IFD Tags

These tags are found in a separate IFD of JPEG, TIFF, DCR and KDC images from some older Kodak models such as the DC50, DC120, DCS760C, DCS Pro 14N, 14nx, SLR/n, Pro Back and Canon EOS D2000.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | UnknownEV? | rational64u |
> 0x0003 | ExposureValue | rational64u |
> 0x03e9 | OriginalFileName | string |
> 0x03eb | SensorLeftBorder | N |
> 0x03ec | SensorTopBorder | N |
> 0x03ed | SensorImageWidth | N |
> 0x03ee | SensorImageHeight | N |
> 0x03f1 | TextualInfo | - | --> Kodak TextualInfo Tags
> 0x03fc | WhiteBalance | int16u |
> 0x03fd | Processing | - | --> Kodak Processing Tags
> 0x0401 | Time | string |
> 0x0414 | NCDFileInfo | string |
> 0x0846 | ColorTemperature | int16u |
> 0x0852 | WB_RGBMul0 | N |
> 0x0853 | WB_RGBMul1 | N |
> 0x0854 | WB_RGBMul2 | N |
> 0x0855 | WB_RGBMul3 | N |
> 0x085c | WB_RGBCoeffs0 | N |
> 0x085d | WB_RGBCoeffs1 | N |
> 0x085e | WB_RGBCoeffs2 | N |
> 0x085f | WB_RGBCoeffs3 | N |
> 0x0ce5 | FirmwareVersion | string |
> 0x1391 | ToneCurveFileName | string |
> 0x1784 | ISO | int32u |

## Kodak TextualInfo Tags

Below is a list of tags which have been observed in the Kodak TextualInfo data, however ExifTool will extract information from any tags found here.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'AF Function' | AFMode | N |
> 'Actual Compensation' | ActualCompensation | N |
> 'Aperture' | Aperture | N |
> 'Auto Bracket' | AutoBracket | N |
> 'Brightness Value' | BrightnessValue | N |
> 'Camera' | CameraModel | N |
> 'Camera body' | CameraBody | N |
> 'Compensation' | ExposureCompensation | N |
> 'Date' | Date | N |
> 'Exposure Bias' | ExposureBias | N |
> 'Exposure Mode' | ExposureMode | N | 'A' = Aperture Priority 'B' = Bulb 'M' = Manual 'P' = Program 'S' = Shutter Priority
> 'Firmware Version' | FirmwareVersion | N |
> 'Flash Compensation' | FlashExposureComp | N |
> 'Flash Fired' | FlashFired | N |
> 'Flash Sync Mode' | FlashSyncMode | N |
> 'Focal Length' | FocalLength | N |
> 'Height' | KodakImageHeight | N |
> 'ISO' | ISO | N |
> 'ISO Speed' | ISO | N |
> 'Image Number' | ImageNumber | N |
> 'Max Aperture' | MaxAperture | N |
> 'Meter Mode' | MeterMode | N |
> 'Min Aperture' | MinAperture | N |
> 'Popup Flash' | PopupFlash | N |
> 'Serial Number' | SerialNumber | N |
> 'Shooting Mode' | ShootingMode | N |
> 'Shutter' | ShutterSpeed | N |
> 'Temperature' | Temperature | N |
> 'Time' | Time | N |
> 'White balance' | WhiteBalance | N |
> 'Width' | KodakImageWidth | N |
> '_other_info' | OtherInfo | N | (any other information without a tag name)

## Kodak Processing Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 20 | WB_RGBLevels | N |

## Kodak Meta Tags

These tags are found in the APP3 "Meta" segment of JPEG images from Kodak cameras such as the DC280, DC3400, DC5000, MC3, M580, Z950 and Z981. The structure of this segment is similar to the APP1 "Exif" segment, but a different set of tags is used.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0xc350 | FilmProductCode | N |
> 0xc351 | ImageSourceEK | N |
> 0xc352 | CaptureConditionsPAR | N |
> 0xc353 | CameraOwner | undef |
> 0xc354 | SerialNumber | undef |
> 0xc355 | UserSelectGroupTitle | N |
> 0xc356 | DealerIDNumber | N |
> 0xc357 | CaptureDeviceFID | N |
> 0xc358 | EnvelopeNumber | N |
> 0xc359 | FrameNumber | N |
> 0xc35a | FilmCategory | N |
> 0xc35b | FilmGencode | N |
> 0xc35c | ModelAndVersion | N |
> 0xc35d | FilmSize | N |
> 0xc35e | SBA_RGBShifts | N |
> 0xc35f | SBAInputImageColorspace | N |
> 0xc360 | SBAInputImageBitDepth | N |
> 0xc361 | SBAExposureRecord | N |
> 0xc362 | UserAdjSBA_RGBShifts | N |
> 0xc363 | ImageRotationStatus | N |
> 0xc364 | RollGuidElements | N |
> 0xc365 | MetadataNumber | N |
> 0xc366 | EditTagArray | N |
> 0xc367 | Magnification | N |
> 0xc36c | NativeXResolution | N |
> 0xc36d | NativeYResolution | N |
> 0xc36e | KodakEffectsIFD | - | --> Kodak SpecialEffects Tags
> 0xc36f | KodakBordersIFD | - | --> Kodak Borders Tags
> 0xc37a | NativeResolutionUnit | N |
> 0xc418 | SourceImageDirectory | N |
> 0xc419 | SourceImageFileName | N |
> 0xc41a | SourceImageVolumeName | N |
> 0xc46c | PrintQuality | N |
> 0xc46e | ImagePrintStatus | N |

## Kodak SpecialEffects Tags

The Kodak SpecialEffects and Borders tags are found in sub-IFD's within the Kodak JPEG APP3 "Meta" segment.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | DigitalEffectsVersion | N |
> 0x0001 | DigitalEffectsName | N |
> 0x0002 | DigitalEffectsType | N |

## Kodak Borders Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | BordersVersion | N |
> 0x0001 | BorderName | N |
> 0x0002 | BorderID | N |
> 0x0003 | BorderLocation | N |
> 0x0004 | BorderType | N |
> 0x0008 | WatermarkType | N |

## Kodak KDC_IFD Tags

These tags are found in a separate IFD of KDC images from some newer Kodak models such as the P880 and Z1015IS.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0xfa00 | SerialNumber | string |
> 0xfa0d | WhiteBalance | int8u | 0 = Auto 1 = Fluorescent 2 = Tungsten 3 = Daylight 6 = Shade
> 0xfa25 | WB_RGBLevelsAuto | N |
> 0xfa27 | WB_RGBLevelsTungsten | N |
> 0xfa28 | WB_RGBLevelsFluorescent | N |
> 0xfa29 | WB_RGBLevelsDaylight | N |
> 0xfa2a | WB_RGBLevelsShade | N |

## Kodak Free Tags

Information stored in the "free" atom of Kodak MP4 videos. (VERY bad form for Kodak to store useful information in an atom intended for unused space!)

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'AprV' | ApertureValue | N |
> 'BrtV' | BrightnessValue | N |
> 'Expc' | ExposureCompensation | N |
> 'Expo' | ExposureTime | N |
> 'FL35' | FocalLengthIn35mmFormat | N |
> 'FNum' | FNumber | N |
> 'FoLn' | FocalLength | N |
> 'ISOS' | ISO | N |
> 'SVer' | FirmwareVersion | N |
> 'Scrn' | PreviewInfo | - | --> Kodak Scrn Tags
> 'Seri' | SerialNumber | N |
> 'StSV' | ShutterSpeedValue | N |

## Kodak Scrn Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PreviewImageWidth | N |
> 1 | PreviewImageHeight | N |
> 2 | PreviewImageLength | N |
> 4 | PreviewImage | N |

## Kodak DcMD Tags

Metadata directory found in MOV and MP4 videos from some Kodak cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'CMbo' | CameraByteOrder | N | 'II' = Little-endian (Intel, II) 'MM' = Big-endian (Motorola, MM)
> 'Cmbo' | CameraByteOrder | N | 'II' = Little-endian (Intel, II) 'MM' = Big-endian (Motorola, MM)
> 'DcEM' | DcEM | - | --> Kodak DcEM Tags
> 'DcME' | DcME | - | --> Kodak DcME Tags

## Kodak DcEM Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Kodak DcME Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Kodak MOV Tags

This information is found in the TAGS atom of MOV videos from Kodak models such as the P880.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 22 | Model | N |
> 64 | ModelType | N |
> 78 | ExposureTime | N |
> 82 | FNumber | N |
> 90 | ExposureCompensation | N |
> 112 | FocalLength | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Feb 7, 2013

<-- ExifTool Tag Names